NV_ESN_I           					0  		;NV_ESN_I           			/* Electronic Serial Number                     */
NV_ESN_CHKSUM_I         				1  		;NV_ESN_CHKSUM_I         		/* Electronic Serial Number checksum            */
NV_VERNO_MAJ_I          				2  		;NV_VERNO_MAJ_I          		/* NV Major version number                      */
NV_VERNO_MIN_I          				3  		;NV_VERNO_MIN_I          		/* NV Minor version number                      */
NV_SCM_I                				4  		;NV_SCM_I                		/* SCMp                                         */
NV_SLOT_CYCLE_INDEX_I   				5  		;NV_SLOT_CYCLE_INDEX_I   		/* Slot cycle index                             */
NV_MOB_CAI_REV_I        				6  		;NV_MOB_CAI_REV_I        		/* Mobile CAI revision number                   */
NV_MOB_FIRM_REV_I       				7  		;NV_MOB_FIRM_REV_I       		/* Mobile firmware revision number              */
NV_MOB_MODEL_I          				8  		;NV_MOB_MODEL_I          		/* Mobile model                                 */
NV_CONFIG_CHKSUM_I      				9  		;NV_CONFIG_CHKSUM_I      		/* Checksum of physical configuration parameters*/
NV_PREF_MODE_I          				10 		;NV_PREF_MODE_I          		/* Digital/Analog mode preference        */ /*10*/
NV_CDMA_PREF_SERV_I     				11 		;NV_CDMA_PREF_SERV_I     		/* CDMA preferred serving system (A/B)          */
NV_ANALOG_PREF_SERV_I   				12 		;NV_ANALOG_PREF_SERV_I   		/* Analog preferred serving system (A/B)        */
NV_CDMA_SID_LOCK_I      				13 		;NV_CDMA_SID_LOCK_I      		/* CDMA SID(s) to lockout                       */
NV_CDMA_SID_ACQ_I       				14 		;NV_CDMA_SID_ACQ_I       		/* CDMA SID to acquire                          */
NV_ANALOG_SID_LOCK_I    				15 		;NV_ANALOG_SID_LOCK_I    		/* ANALOG SID(s) to lockout                     */
NV_ANALOG_SID_ACQ_I     				16 		;NV_ANALOG_SID_ACQ_I     		/* ANALOG SID to acquire                        */
NV_ANALOG_FIRSTCHP_I    				17 		;NV_ANALOG_FIRSTCHP_I    		/* Analog FIRSTCHPp                             */
NV_ANALOG_HOME_SID_I    				18 		;NV_ANALOG_HOME_SID_I    		/* Analog HOME_SIDp                             */
NV_ANALOG_REG_I         				19 		;NV_ANALOG_REG_I         		/* Analog registration setting                  */
NV_PCDMACH_I            				20 		;NV_PCDMACH_I            		/* Primary CDMA channel   */                /*20*/
NV_SCDMACH_I            				21 		;NV_SCDMACH_I            		/* Secondary CDMA channel                       */
NV_PPCNCH_I             				22 		;NV_PPCNCH_I             		/* Primary PCN channel                          */
NV_SPCNCH_I             				23 		;NV_SPCNCH_I             		/* Secondary PCN channel                        */
NV_NAM_CHKSUM_I         				24 		;NV_NAM_CHKSUM_I         		/* NAM checksum                                 */
NV_A_KEY_I              				25 		;NV_A_KEY_I              		/* Authentication A key                         */
NV_A_KEY_CHKSUM_I       				26 		;NV_A_KEY_CHKSUM_I       		/* Authentication A key checksum                */
NV_SSD_A_I              				27 		;NV_SSD_A_I              		/* SSD_Asp                                      */
NV_SSD_A_CHKSUM_I       				28 		;NV_SSD_A_CHKSUM_I       		/* SSD_Asp checksum                             */
NV_SSD_B_I              				29 		;NV_SSD_B_I              		/* SSD_Bsp                                      */
NV_SSD_B_CHKSUM_I       				30 		;NV_SSD_B_CHKSUM_I       		/* SSD_Bsp checksum        */               /*30*/
NV_COUNT_I              				31 		;NV_COUNT_I              		/* COUNTsp                                      */
NV_MIN1_I               				32 		;NV_MIN1_I               		/* MIN1p                                        */
NV_MIN2_I               				33 		;NV_MIN2_I               		/* MIN2p                                        */
NV_MOB_TERM_HOME_I      				34 		;NV_MOB_TERM_HOME_I      		/* CDMA MOB_TERM_HOMEp registration flag        */
NV_MOB_TERM_FOR_SID_I   				35 		;NV_MOB_TERM_FOR_SID_I   		/* CDMA MOB_TERM_FOR_SIDp registration flag     */
NV_MOB_TERM_FOR_NID_I   				36 		;NV_MOB_TERM_FOR_NID_I   		/* CDMA MOB_TERM_FOR_NIDp registration flag     */
NV_ACCOLC_I             				37 		;NV_ACCOLC_I             		/* ACCOLCp                                      */
NV_SID_NID_I            				38 		;NV_SID_NID_I            		/* CDMA SID/NID pairs                           */
NV_MIN_CHKSUM_I         				39 		;NV_MIN_CHKSUM_I         		/* MIN checksum                                 */
NV_CURR_NAM_I           				40 		;NV_CURR_NAM_I           		/* Current NAM     */                       /*40*/
NV_ORIG_MIN_I           				41 		;NV_ORIG_MIN_I           		/* Call origination MIN within NAM              */
NV_AUTO_NAM_I           				42 		;NV_AUTO_NAM_I           		/* Select NAM automatically on roaming          */
NV_NAME_NAM_I           				43 		;NV_NAME_NAM_I           		/* A user selectable name for each NAM          */
NV_NXTREG_I             				44 		;NV_NXTREG_I             		/* NXTREGsp                                     */
NV_LSTSID_I             				45 		;NV_LSTSID_I             		/* SIDsp (last SID registered)                  */
NV_LOCAID_I             				46 		;NV_LOCAID_I             		/* LOCAIDsp                                     */
NV_PUREG_I              				47 		;NV_PUREG_I              		/* PUREGsp                                      */
NV_ZONE_LIST_I          				48 		;NV_ZONE_LIST_I          		/* ZONE_LISTsp                                  */
NV_SID_NID_LIST_I       				49 		;NV_SID_NID_LIST_I       		/* SID_NID_LISTsp                               */
NV_DIST_REG_I           				50 		;NV_DIST_REG_I           		/* Distance registration variables   */     /*50*/
NV_LAST_CDMACH_I        				51 		;NV_LAST_CDMACH_I        		/* Last CDMA channel acquired                   */
NV_CALL_TIMER_I      					52 		;NV_CALL_TIMER_I      			/* Last call time                                  */
NV_AIR_TIMER_I       					53 		;NV_AIR_TIMER_I       			/* Air time (resettable cummulative call timer)    */
NV_ROAM_TIMER_I      					54 		;NV_ROAM_TIMER_I      			/* Roam time (resettable cummulative roam timer)   */
NV_LIFE_TIMER_I      					55 		;NV_LIFE_TIMER_I      			/* Life time (non-resettable cumm. call timer)     */
NV_RUN_TIMER_I       					56 		;NV_RUN_TIMER_I       			/* Run timer (time hardware has been running)      */
NV_DIAL_I            					57 		;NV_DIAL_I            			/* Speed dial number                               */
NV_STACK_I           					58 		;NV_STACK_I           			/* Call stack number                               */
NV_STACK_IDX_I       					59 		;NV_STACK_IDX_I       			/* Call stack last number index                    */
NV_PAGE_SET_I        					60 		;NV_PAGE_SET_I        			/* OBSOLETE Page setting     */                /*60*/
NV_PAGE_MSG_I        					61 		;NV_PAGE_MSG_I        			/* OBSOLETE Page message and time                  */
NV_EAR_LVL_I         					62 		;NV_EAR_LVL_I         			/* Handset ear piece volume level                  */
NV_SPEAKER_LVL_I     					63 		;NV_SPEAKER_LVL_I     			/* Handsfree speaker volume level                  */
NV_RINGER_LVL_I      					64 		;NV_RINGER_LVL_I      			/* Ringer volume level                             */
NV_BEEP_LVL_I        					65 		;NV_BEEP_LVL_I        			/* Key beep volume level                           */
NV_CALL_BEEP_I       					66 		;NV_CALL_BEEP_I       			/* One minute call beeper select                   */
NV_CONT_KEY_DTMF_I   					67 		;NV_CONT_KEY_DTMF_I   			/* Continuous keypad DTMF tones select             */
NV_CONT_STR_DTMF_I   					68 		;NV_CONT_STR_DTMF_I   			/* Continuous string (memory) DTMF tones select    */
NV_SVC_AREA_ALERT_I  					69 		;NV_SVC_AREA_ALERT_I  			/* Service area enter/exit alert select            */
NV_CALL_FADE_ALERT_I 					70 		;NV_CALL_FADE_ALERT_I 			/* Call fade alert select     */               /*70*/
NV_BANNER_I          					71 		;NV_BANNER_I          			/* Idle banner to display                          */
NV_LCD_I             					72 		;NV_LCD_I             			/* Display brightness setting                      */
NV_AUTO_POWER_I      					73 		;NV_AUTO_POWER_I      			/* Auto power settings (power savings)             */
NV_AUTO_ANSWER_I     					74 		;NV_AUTO_ANSWER_I     			/* Auto answer setting                             */
NV_AUTO_REDIAL_I     					75 		;NV_AUTO_REDIAL_I     			/* Auto redial setting                             */
NV_AUTO_HYPHEN_I     					76 		;NV_AUTO_HYPHEN_I     			/* Auto hyphen setting                             */
NV_BACK_LIGHT_I      					77 		;NV_BACK_LIGHT_I      			/* Backlighting manual/auto mode                   */
NV_AUTO_MUTE_I       					78 		;NV_AUTO_MUTE_I       			/* Auto radio mute setting                         */
NV_MAINTRSN_I    					79 		;NV_MAINTRSN_I    			/* Base station maintance required reason              */
NV_LCKRSN_P_I    					80 		;NV_LCKRSN_P_I    			/* Base station lock reason until power cycled */ /*80*/
NV_LOCK_I        					81 		;NV_LOCK_I        			/* Indicator of whether user locked the phone          */
NV_LOCK_CODE_I   					82 		;NV_LOCK_CODE_I   			/* Lock code string                                    */
NV_AUTO_LOCK_I   					83 		;NV_AUTO_LOCK_I   			/* Auto lock setting                                   */
NV_CALL_RSTRC_I  					84 		;NV_CALL_RSTRC_I  			/* Call restrictions                                   */
NV_SEC_CODE_I    					85 		;NV_SEC_CODE_I    			/* Security code                                       */
NV_HORN_ALERT_I  					86 		;NV_HORN_ALERT_I  			/* Horn alert setting                                  */
NV_ERR_LOG_I         					87 		;NV_ERR_LOG_I         			/* Error log                                       */
NV_UNIT_ID_I         					88 		;NV_UNIT_ID_I         			/* Unit hardware id  (obsolete)                    */
NV_FREQ_ADJ_I        					89 		;NV_FREQ_ADJ_I        			/* Frequency adjust values  (obsolete)             */
NV_VBATT_I           					90 		;NV_VBATT_I           			/* V battery regulator array for min/max */    /*90*/
NV_FM_TX_PWR_I       					91 		;NV_FM_TX_PWR_I       			/* Analog TX power level array                     */
NV_FR_TEMP_OFFSET_I                                     92                 ;NV_FR_TEMP_OFFSET_I                     
NV_DM_IO_MODE_I      					93 		;NV_DM_IO_MODE_I      			/* External port (I/O) mode for DM service         */
NV_CDMA_TX_LIMIT_I   					94 		;NV_CDMA_TX_LIMIT_I   			/* To limit TX_GAIN_ADJ when output exceeded       */
NV_FM_RSSI_I         					95 		;NV_FM_RSSI_I         			/* Analog RSSI adjustment                          */
NV_CDMA_RIPPLE_I     					96 		;NV_CDMA_RIPPLE_I     			/* CDMA UHF Ripple Compensation                    */
NV_CDMA_RX_OFFSET_I  					97 		;NV_CDMA_RX_OFFSET_I  			/* CDMA RX Offset compensation                     */
NV_CDMA_RX_POWER_I   					98 		;NV_CDMA_RX_POWER_I   			/* CDMA True RX Power Table                        */
NV_CDMA_RX_ERROR_I   					99 		;NV_CDMA_RX_ERROR_I   			/* CDMA RX Linear and Non-linear error table       */
NV_CDMA_TX_SLOPE_1_I 					100		;NV_CDMA_TX_SLOPE_1_I 			/* CDMA TX Gain Comp Slope Compensation tbl*/ /*100*/
NV_CDMA_TX_SLOPE_2_I 					101		;NV_CDMA_TX_SLOPE_2_I 			/* CDMA TX Gain Adjust Slope Compensation table    */
NV_CDMA_TX_ERROR_I   					102		;NV_CDMA_TX_ERROR_I   			/* CDMA TX Non-linear Error Compensation table     */
NV_PA_CURRENT_CTL_I  					103		;NV_PA_CURRENT_CTL_I  			/* PA Current Control table                        */
NV_SONY_ATTEN_1_I                                       104                ;NV_SONY_ATTEN_1_I                       
NV_SONY_ATTEN_2_I                                       105                ;NV_SONY_ATTEN_2_I                       
NV_VOC_GAIN_I                                           106                ;NV_VOC_GAIN_I                           
NV_SPARE_1_I                                            107                ;NV_SPARE_1_I                            
NV_SPARE_2_I                                            108                ;NV_SPARE_2_I                            
NV_DATA_SRVC_STATE_I   					109		;NV_DATA_SRVC_STATE_I   			/* Data Service(Task) Enabled/Disabled           */
NV_DATA_IO_MODE_I      					110		;NV_DATA_IO_MODE_I      			/* External port (I/O) mode for Data svc */ /*110*/
NV_IDLE_DATA_TIMEOUT_I 					111		;NV_IDLE_DATA_TIMEOUT_I 			/* Data service idle time in seconds             */
NV_MAX_TX_ADJ_I                                         112                ;NV_MAX_TX_ADJ_I                         
NV_INI_MUTE_I                                           113                ;NV_INI_MUTE_I                           
NV_FACTORY_INFO_I                                       114                ;NV_FACTORY_INFO_I                       
NV_SONY_ATTEN_3_I                                       115                ;NV_SONY_ATTEN_3_I                       
NV_SONY_ATTEN_4_I                                       116                ;NV_SONY_ATTEN_4_I                       
NV_SONY_ATTEN_5_I                                       117                ;NV_SONY_ATTEN_5_I                       
NV_DM_ADDR_I                                            118                ;NV_DM_ADDR_I                            
NV_CDMA_PN_MASK_I                                       119                ;NV_CDMA_PN_MASK_I                       
NV_SEND_TIMEOUT_I             				120		;NV_SEND_TIMEOUT_I             		                                     /*120*/
NV_FM_AGC_SET_VS_PWR_I        				121		;NV_FM_AGC_SET_VS_PWR_I        		/* FM TX_AGC_ADJ setting vs power         */
NV_FM_AGC_SET_VS_FREQ_I       				122		;NV_FM_AGC_SET_VS_FREQ_I       		/* FM TX_AGC_ADJ setting vs frequency     */
NV_FM_AGC_SET_VS_TEMP_I       				123		;NV_FM_AGC_SET_VS_TEMP_I       		/* FM TX_AGC_ADJ setting vs temperature   */
NV_FM_EXP_HDET_VS_PWR_I       				124		;NV_FM_EXP_HDET_VS_PWR_I       		/* FM expected HDET reading vs power      */
NV_FM_ERR_SLP_VS_PWR_I        				125		;NV_FM_ERR_SLP_VS_PWR_I        		/* FM HDET error slope vs power           */
NV_FM_FREQ_SENSE_GAIN_I       				126		;NV_FM_FREQ_SENSE_GAIN_I       		/* deviation adj. trim                    */
NV_CDMA_RX_LIN_OFF_0_I        				127		;NV_CDMA_RX_LIN_OFF_0_I        		/* CDMA Rx linearizer offset              */
NV_CDMA_RX_LIN_SLP_I          				128		;NV_CDMA_RX_LIN_SLP_I          		/* CDMA Rx linearizer slope               */
NV_CDMA_RX_COMP_VS_FREQ_I     				129		;NV_CDMA_RX_COMP_VS_FREQ_I     		/* CDMA Rx gain comp vs frequency         */
NV_CDMA_TX_COMP_VS_FREQ_I     				130		;NV_CDMA_TX_COMP_VS_FREQ_I     		/* CDMA Tx gain comp vs frequency */ /*130*/
NV_CDMA_TX_COMP_VS_VOLT_I     				131		;NV_CDMA_TX_COMP_VS_VOLT_I     		/* CDMA Tx gain comp vs voltage           */
NV_CDMA_TX_LIN_MASTER_OFF_0_I 				132		;NV_CDMA_TX_LIN_MASTER_OFF_0_I 		/* CDMA Tx linearizer master offset       */
NV_CDMA_TX_LIN_MASTER_SLP_I   				133		;NV_CDMA_TX_LIN_MASTER_SLP_I   		/* CDMA Tx linearizer master slope        */
NV_CDMA_TX_LIN_VS_TEMP_I      				134		;NV_CDMA_TX_LIN_VS_TEMP_I      		/* CDMA Tx linearizer trim vs temp        */
NV_CDMA_TX_LIN_VS_VOLT_I      				135		;NV_CDMA_TX_LIN_VS_VOLT_I      		/* CDMA Tx linearizer trim vs voltage     */                                          
NV_CDMA_TX_LIM_VS_TEMP_I      				136		;NV_CDMA_TX_LIM_VS_TEMP_I      		/* CDMA Tx power limit vs temperature     */
NV_CDMA_TX_LIM_VS_VOLT_I      				137		;NV_CDMA_TX_LIM_VS_VOLT_I      		/* CDMA Tx power limit vs voltage         */
NV_CDMA_TX_LIM_VS_FREQ_I      				138		;NV_CDMA_TX_LIM_VS_FREQ_I      		/* CDMA Tx power limit vs frequency       */
NV_CDMA_EXP_HDET_VS_AGC_I     				139		;NV_CDMA_EXP_HDET_VS_AGC_I     		/* CDMA expected HDET reading vs AGC PDM  */
NV_CDMA_ERR_SLP_VS_HDET_I  				140		;NV_CDMA_ERR_SLP_VS_HDET_I  		/*CDMA HDET err slope vs HDET reading*/ /*140*/
NV_THERM_I                    				141		;NV_THERM_I                    		/* RF & LCD temp. based compensation      */
NV_VBATT_PA_I                 				142		;NV_VBATT_PA_I                 		/* RF comp. based on voltage              */
NV_HDET_OFF_I                 				143		;NV_HDET_OFF_I                 		/* ADC HDET reading offset                */
NV_HDET_SPN_I                 				144		;NV_HDET_SPN_I                 		/* ADC HDET reading span                  */
NV_ONETOUCH_DIAL_I            				145		;NV_ONETOUCH_DIAL_I            		/* ena/dis UI one touch dialing           */
NV_FM_AGC_ADJ_VS_FREQ_I                                 146                ;NV_FM_AGC_ADJ_VS_FREQ_I                 
NV_FM_AGC_ADJ_VS_TEMP_I                                 147                ;NV_FM_AGC_ADJ_VS_TEMP_I                 
NV_RF_CONFIG_I                                          148                ;NV_RF_CONFIG_I                          
NV_R1_RISE_I                                            149                ;NV_R1_RISE_I                            
NV_R1_FALL_I                                            150           	;NV_R1_FALL_I                            /*150*/
NV_R2_RISE_I                                            151                ;NV_R2_RISE_I                            
NV_R2_FALL_I                                            152                ;NV_R2_FALL_I                            
NV_R3_RISE_I                                            153                ;NV_R3_RISE_I                            
NV_R3_FALL_I                                            154                ;NV_R3_FALL_I                            
NV_PA_RANGE_STEP_CAL_I                                  155                ;NV_PA_RANGE_STEP_CAL_I                  
NV_LNA_RANGE_POL_I                                      156                ;NV_LNA_RANGE_POL_I                      
NV_LNA_RANGE_RISE_I                                     157                ;NV_LNA_RANGE_RISE_I                     
NV_LNA_RANGE_FALL_I                                     158                ;NV_LNA_RANGE_FALL_I                     
NV_LNA_RANGE_OFFSET_I                                   159                ;NV_LNA_RANGE_OFFSET_I                   
NV_POWER_CYCLES_I                                       160           	;NV_POWER_CYCLES_I                       /*160*/
NV_ALERTS_LVL_I                                         161                ;NV_ALERTS_LVL_I                         
NV_ALERTS_LVL_SHADOW_I                                  162                ;NV_ALERTS_LVL_SHADOW_I                  
NV_RINGER_LVL_SHADOW_I                                  163                ;NV_RINGER_LVL_SHADOW_I                  
NV_BEEP_LVL_SHADOW_I                                    164                ;NV_BEEP_LVL_SHADOW_I                    
NV_EAR_LVL_SHADOW_I                                     165                ;NV_EAR_LVL_SHADOW_I                     
NV_TIME_SHOW_I                                          166                ;NV_TIME_SHOW_I                          
NV_MESSAGE_ALERT_I                                      167                ;NV_MESSAGE_ALERT_I                      
NV_AIR_CNT_I                                            168                ;NV_AIR_CNT_I                            
NV_ROAM_CNT_I                                           169                ;NV_ROAM_CNT_I                           
NV_LIFE_CNT_I                                           170           	;NV_LIFE_CNT_I                           /*170*/
NV_SEND_PIN_I                                           171                ;NV_SEND_PIN_I                           
NV_AUTO_ANSWER_SHADOW_I                                 172                ;NV_AUTO_ANSWER_SHADOW_I                 
NV_AUTO_REDIAL_SHADOW_I                                 173                ;NV_AUTO_REDIAL_SHADOW_I                 
NV_SMS_I                                                174                ;NV_SMS_I                                
NV_SMS_DM_I                                             175                ;NV_SMS_DM_I                             
NV_IMSI_MCC_I                                           176                ;NV_IMSI_MCC_I                           
NV_IMSI_11_12_I                                         177                ;NV_IMSI_11_12_I                         
NV_DIR_NUMBER_I                                         178                ;NV_DIR_NUMBER_I                         
NV_VOICE_PRIV_I                                         179                ;NV_VOICE_PRIV_I                         
NV_SPARE_B1_I                                           180           	;NV_SPARE_B1_I                           /*180*/
NV_SPARE_B2_I                                           181                ;NV_SPARE_B2_I                           
NV_SPARE_W1_I                                           182                ;NV_SPARE_W1_I                           
NV_SPARE_W2_I                                           183                ;NV_SPARE_W2_I                           
NV_FSC_I                                                184                ;NV_FSC_I                                
NV_ALARMS_I                                             185                ;NV_ALARMS_I                             
NV_STANDING_ALARM_I                                     186                ;NV_STANDING_ALARM_I                     
NV_ISD_STD_PASSWD_I                                     187                ;NV_ISD_STD_PASSWD_I                     
NV_ISD_STD_RESTRICT_I                                   188                ;NV_ISD_STD_RESTRICT_I                   
NV_DIALING_PLAN_I                                       189                ;NV_DIALING_PLAN_I                       
NV_FM_LNA_CTL_I                                         190           	;NV_FM_LNA_CTL_I                         /*190*/
NV_LIFE_TIMER_G_I                                       191                ;NV_LIFE_TIMER_G_I                       
NV_CALL_TIMER_G_I                                       192                ;NV_CALL_TIMER_G_I                       
NV_PWR_DWN_CNT_I                                        193                ;NV_PWR_DWN_CNT_I                        
NV_FM_AGC_I                                             194                ;NV_FM_AGC_I                             
NV_FSC2_I                                               195                ;NV_FSC2_I                               
NV_FSC2_CHKSUM_I                                        196                ;NV_FSC2_CHKSUM_I                        
NV_WDC_I                                                197                ;NV_WDC_I                                
NV_HW_CONFIG_I                                          198                ;NV_HW_CONFIG_I                          
NV_CDMA_RX_LIN_VS_TEMP_I            			199		;NV_CDMA_RX_LIN_VS_TEMP_I            	/* CDMA Rx linearizer vs temperature*/
NV_CDMA_ADJ_FACTOR_I                			200		;NV_CDMA_ADJ_FACTOR_I                	/* CDMA adjustment factor */   /*200*/
NV_CDMA_TX_LIM_BOOSTER_OFF_I                            201                ;NV_CDMA_TX_LIM_BOOSTER_OFF_I            
NV_CDMA_RX_SLP_VS_TEMP_I                                202                ;NV_CDMA_RX_SLP_VS_TEMP_I                
NV_CDMA_TX_SLP_VS_TEMP_I                                203                ;NV_CDMA_TX_SLP_VS_TEMP_I                
NV_PA_RANGE_VS_TEMP_I                                   204                ;NV_PA_RANGE_VS_TEMP_I                   
NV_LNA_SWITCH_VS_TEMP_I                                 205                ;NV_LNA_SWITCH_VS_TEMP_I                 
NV_FM_EXP_HDET_VS_TEMP_I                                206                ;NV_FM_EXP_HDET_VS_TEMP_I                
NV_N1M_I                                                207                ;NV_N1M_I                                
NV_IMSI_I                           			208		;NV_IMSI_I                           	/* OBSOLETE InternationaMobileStationID*/
NV_IMSI_ADDR_NUM_I                  			209		;NV_IMSI_ADDR_NUM_I                  	/* Length of IMSI                   */
NV_ASSIGNING_TMSI_ZONE_LEN_I        			210		;NV_ASSIGNING_TMSI_ZONE_LEN_I        	/* TMSI_ZONE_LENs-p  */        /*210*/
NV_ASSIGNING_TMSI_ZONE_I            			211		;NV_ASSIGNING_TMSI_ZONE_I            	/* TMSI_ZONEs-p                     */
NV_TMSI_CODE_I                      			212		;NV_TMSI_CODE_I                      	/* TMSI_CODEs-p                     */
NV_TMSI_EXP_I                       			213		;NV_TMSI_EXP_I                       	/* TMSI expiration time             */
NV_HOME_PCS_FREQ_BLOCK_I            			214		;NV_HOME_PCS_FREQ_BLOCK_I            	/* Subscriber's home block          */
NV_DIR_NUMBER_PCS_I                 			215		;NV_DIR_NUMBER_PCS_I                 	/* Directory number PCS format     */
NV_ROAMING_LIST_I                   			216		;NV_ROAMING_LIST_I                   	/* The roaming list                 */
NV_MRU_TABLE_I                      			217		;NV_MRU_TABLE_I                      	/* Most recently used channels      */
NV_REDIAL_I                 				218		;NV_REDIAL_I                 		/* Last number redial                       */
NV_OTKSL_I                  				219		;NV_OTKSL_I                  		/* One-time keypad subsidy lock             */
NV_TIMED_PREF_MODE_I        				220		;NV_TIMED_PREF_MODE_I        		/* To allow analog-only operation */   /*220*/
NV_ANY_KEY_ANSWER_I         				221		;NV_ANY_KEY_ANSWER_I         		/* Answer call with any key                 */
NV_BACK_LIGHT_HFK_I         				222		;NV_BACK_LIGHT_HFK_I         		/* Hands Free Kit backlight setting         */
NV_RESTRICT_GLOBAL_I        				223		;NV_RESTRICT_GLOBAL_I        		/* Global phone book restriction            */
NV_KEY_SOUND_I              				224		;NV_KEY_SOUND_I              		/* Type of keypress sound emitted           */
NV_DIALS_SORTING_METHOD_I   				225		;NV_DIALS_SORTING_METHOD_I   		/* Phone book sorting method                */
NV_LANGUAGE_SELECTION_I     				226		;NV_LANGUAGE_SELECTION_I     		/* Language for user interface              */
NV_MENU_FORMAT_I            				227		;NV_MENU_FORMAT_I            		/* Type of user interface menus             */
NV_RINGER_TYPE_I            				228		;NV_RINGER_TYPE_I            		/* Ringer type setting                      */
NV_RINGER_SPKR_LVL_I        				229		;NV_RINGER_SPKR_LVL_I        		/* External speaker ringer volume           */
NV_BEEP_SPKR_LVL_I          				230		;NV_BEEP_SPKR_LVL_I          		/* External speaker key beep volume */ /*230*/
NV_MRU2_TABLE_I             				231		;NV_MRU2_TABLE_I             		/* New format Most Recently Used channels  */
NV_VIBRATOR_I               				232		;NV_VIBRATOR_I               		/* Use vibrator instead of ringer           */
NV_FLIP_ANSWERS_I           				233		;NV_FLIP_ANSWERS_I           		/* Opening clamshell answers call           */
NV_DIAL_RESTRICT_LVLS_I     				234		;NV_DIAL_RESTRICT_LVLS_I     		/* ISS2 dialing restriction levels          */
NV_DIAL_STATE_TABLE_LEN_I   				235		;NV_DIAL_STATE_TABLE_LEN_I   		/* Number elements in state table           */
NV_DIAL_STATE_TABLE_I       				236		;NV_DIAL_STATE_TABLE_I       		/* ISS2 dialing plan state table            */
NV_VOICE_PRIV_ALERT_I       				237		;NV_VOICE_PRIV_ALERT_I       		/* Voice privacy alert for TGP              */
NV_IP_ADDRESS_I             				238		;NV_IP_ADDRESS_I             		/* IP/Port address  (obsolete)              */
NV_CURR_GATEWAY_I           				239		;NV_CURR_GATEWAY_I           		/* Last active IP address (obsolete)        */
NV_DATA_QNC_ENABLED_I       				240		;NV_DATA_QNC_ENABLED_I       		/* QNC enabled flag                 */ /*240*/
NV_DATA_SO_SET_I            				241		;NV_DATA_SO_SET_I            		/* Which Service Option set is in effect    */
NV_UP_LINK_INFO_I           				242		;NV_UP_LINK_INFO_I           		/* IP addresses and key data                */
NV_UP_PARMS_I               				243		;NV_UP_PARMS_I               		/* Current gateway alert state etc.       */
NV_UP_CACHE_I               				244		;NV_UP_CACHE_I               		/* The Unwired Planet cache                 */
NV_ELAPSED_TIME_I           				245		;NV_ELAPSED_TIME_I           		/* Timer for formal test use                */
NV_PDM2_I                   				246		;NV_PDM2_I                   		/* For RF Cal use                           */
NV_RX_AGC_MINMAX_I          				247		;NV_RX_AGC_MINMAX_I          		/* Receiver AGC min-max                     */
NV_VBATT_AUX_I              				248		;NV_VBATT_AUX_I              		/* Auxillary VBATT min-max                  */
NV_DTACO_CONTROL_I            				249		;NV_DTACO_CONTROL_I            		/* DTACO enabled/disabled control         */
NV_DTACO_INTERDIGIT_TIMEOUT_I 				250		;NV_DTACO_INTERDIGIT_TIMEOUT_I 		/* DTACO interdigit timeout       */ /*250*/
NV_PDM1_I                   				251		;NV_PDM1_I                   		/* For RF Cal use                           */
NV_BELL_MODEM_I             				252		;NV_BELL_MODEM_I             		/* Flag for ISS2                            */
NV_PDM1_VS_TEMP_I           				253		;NV_PDM1_VS_TEMP_I           		/* For RF Cal use                           */
NV_PDM2_VS_TEMP_I           				254		;NV_PDM2_VS_TEMP_I           		/* For RF Cal use                           */
NV_SID_NID_LOCK_I           				255		;NV_SID_NID_LOCK_I           		/* CDMA SID(s) and NID(s) to lockout        */
NV_PRL_ENABLED_I            				256		;NV_PRL_ENABLED_I            		/* If the roaming list is enabled or not    */
NV_ROAMING_LIST_683_I       				257		;NV_ROAMING_LIST_683_I       		/* IS-683-A format roaming list             */  
NV_SYSTEM_PREF_I            				258		;NV_SYSTEM_PREF_I            		/* System Preference per NAM               */
NV_HOME_SID_NID_I           				259		;NV_HOME_SID_NID_I           		/* "Home" SID/NID list                      */
NV_OTAPA_ENABLED_I          				260		;NV_OTAPA_ENABLED_I          		/* Whether OTAPA is enabled per NAM*/ /*260*/
NV_NAM_LOCK_I               				261		;NV_NAM_LOCK_I               		/* SPASM protection per NAM                 */
NV_IMSI_T_S1_I              				262		;NV_IMSI_T_S1_I              		/* True IMSI - MIN1                         */
NV_IMSI_T_S2_I              				263		;NV_IMSI_T_S2_I              		/* True IMSI - MIN2                         */
NV_IMSI_T_MCC_I             				264		;NV_IMSI_T_MCC_I             		/* True IMSI - MCC                          */
NV_IMSI_T_11_12_I           				265		;NV_IMSI_T_11_12_I           		/* True IMSI - 11th & 12th digits           */
NV_IMSI_T_ADDR_NUM_I        				266		;NV_IMSI_T_ADDR_NUM_I        		/* True IMSI - Addr num                     */
NV_UP_ALERTS_I              				267		;NV_UP_ALERTS_I              		/* Unwired Planet alert records             */
NV_UP_IDLE_TIMER_I          				268		;NV_UP_IDLE_TIMER_I          		/* Idle time timer                          */
NV_SMS_UTC_I                				269		;NV_SMS_UTC_I                		/* Specifies format of SMS time display     */
NV_ROAM_RINGER_I            				270		;NV_ROAM_RINGER_I            		/* Specifies roam ringer on or off  */ /*270*/
NV_RENTAL_TIMER_I           				271		;NV_RENTAL_TIMER_I           		/* The rental timer item                    */
NV_RENTAL_TIMER_INC_I       				272		;NV_RENTAL_TIMER_INC_I       		/* The rental timer increment value         */
NV_RENTAL_CNT_I             				273		;NV_RENTAL_CNT_I             		/* The rental counter                       */
NV_RENTAL_TIMER_ENABLED_I   				274		;NV_RENTAL_TIMER_ENABLED_I   		/* Enables/disables the rental timer        */
NV_FULL_SYSTEM_PREF_I       				275		;NV_FULL_SYSTEM_PREF_I       		/* Controls system pref display options     */
NV_BORSCHT_RINGER_FREQ_I    				276		;NV_BORSCHT_RINGER_FREQ_I    		/* Ringer freq used for BORSCHT port (RJ-11)*/
NV_PAYPHONE_ENABLE_I        				277		;NV_PAYPHONE_ENABLE_I        		/* Enable/disable payphone support          */
NV_DSP_ANSWER_DET_ENABLE_I  				278		;NV_DSP_ANSWER_DET_ENABLE_I  		/* Enable/disable dsp answer detection      */
NV_EVRC_PRI_I               				279		;NV_EVRC_PRI_I               		/* EVRC/13K priority: EVRC first 13K first */
NV_AFAX_CLASS_20_I          				280		;NV_AFAX_CLASS_20_I          		/* Obsolete item                    */ /*280*/
NV_V52_CONTROL_I            				281		;NV_V52_CONTROL_I            		/* V52 control option                       */
NV_CARRIER_INFO_I           				282		;NV_CARRIER_INFO_I           		/* Bitmap and ASCII name info for carrier   */
NV_AFAX_I                   				283		;NV_AFAX_I                   		/* Analog FAX type: end to end or class 2.0 */
NV_SIO_PWRDWN_I             				284		;NV_SIO_PWRDWN_I             		/* Distinguishes old/new UART hardware      */
NV_PREF_VOICE_SO_I          				285		;NV_PREF_VOICE_SO_I          		/* EVRC voice service options               */
NV_VRHFK_ENABLED_I          				286		;NV_VRHFK_ENABLED_I          		/* Voice recognition hands free kit enabled */
NV_VRHFK_VOICE_ANSWER_I     				287		;NV_VRHFK_VOICE_ANSWER_I     		/* Voice recognition voice answer           */
NV_PDM1_VS_FREQ_I           				288		;NV_PDM1_VS_FREQ_I           		/* For RF Cal use                           */
NV_PDM2_VS_FREQ_I           				289		;NV_PDM2_VS_FREQ_I           		/* For RF Cal use                           */
NV_SMS_AUTO_DELETE_I        				290		;NV_SMS_AUTO_DELETE_I        		/* SMS auto-deletion enabled status */ /*290*/
NV_SRDA_ENABLED_I           				291		;NV_SRDA_ENABLED_I           		/* Silent redial enabled status             */
NV_OUTPUT_UI_KEYS_I         				292		;NV_OUTPUT_UI_KEYS_I         		/* Enable-disable sending UI keystrokes     */
NV_POL_REV_TIMEOUT_I        				293		;NV_POL_REV_TIMEOUT_I        		/* Timeout for polarity reversal            */
NV_SI_TEST_DATA_1_I         				294		;NV_SI_TEST_DATA_1_I         		/* First stack-checker diagnostic buffer    */
NV_SI_TEST_DATA_2_I         				295		;NV_SI_TEST_DATA_2_I         		/* Second stack-checker diagnostic buffer   */
NV_SPC_CHANGE_ENABLED_I     				296		;NV_SPC_CHANGE_ENABLED_I     		/* Enable-disable OTASP SPC change          */
NV_DATA_MDR_MODE_I          				297		;NV_DATA_MDR_MODE_I          		/* Select the MDR mode                      */
NV_DATA_PKT_ORIG_STR_I      				298		;NV_DATA_PKT_ORIG_STR_I      		/* Dial string for originating packet calls */
NV_UP_KEY_I                 				299		;NV_UP_KEY_I                 		/* Unwired Planet access key item           */
NV_DATA_AUTO_PACKET_DETECTION_I 			300		;NV_DATA_AUTO_PACKET_DETECTION_I 	/* Packet data configuration item       */
NV_AUTO_VOLUME_ENABLED_I    				301		;NV_AUTO_VOLUME_ENABLED_I    		/* Enable-disable auto volume               */
NV_WILDCARD_SID_I           				302		;NV_WILDCARD_SID_I           		/* Allow wildcard SID                       */
NV_ROAM_MSG_I               				303		;NV_ROAM_MSG_I               		/* Downloadable roaming messages            */
NV_OTKSL_FLAG_I             				304		;NV_OTKSL_FLAG_I             		/* OTKSL Flag                               */
NV_BROWSER_TYPE_I           				305		;NV_BROWSER_TYPE_I           		/* Browser identifier                       */ 
NV_SMS_REMINDER_TONE_I      				306		;NV_SMS_REMINDER_TONE_I      		/* Reminder tone is on or off               */
NV_UBROWSER_I               				307		;NV_UBROWSER_I               		/* Micro browser data                       */
NV_BTF_ADJUST_I             				308		;NV_BTF_ADJUST_I             		/* BTF adjustment value                     */
NV_FULL_PREF_MODE_I         				309		;NV_FULL_PREF_MODE_I         		/* Controls pref display options            */
NV_UP_BROWSER_WARN_I        				310		;NV_UP_BROWSER_WARN_I        		/* Confirmation screen option       */ /*310*/
NV_FM_HDET_ADC_RANGE_I      				311		;NV_FM_HDET_ADC_RANGE_I      		/* ADC range for HDET sampling (analog)     */
NV_CDMA_HDET_ADC_RANGE_I    				312		;NV_CDMA_HDET_ADC_RANGE_I    		/* ADC range for HDET sampling (CDMA)       */
NV_PN_ID_I                  				313		;NV_PN_ID_I                  		/* PN code selection                        */
NV_USER_ZONE_ENABLED_I      				314		;NV_USER_ZONE_ENABLED_I      		/* Enable-disable User Zone table           */
NV_USER_ZONE_I              				315		;NV_USER_ZONE_I              		/* User Zone table                          */
NV_PAP_DATA_I               				316		;NV_PAP_DATA_I               		/* Password Authentication Protocol data    */
NV_DATA_DEFAULT_PROFILE_I   				317		;NV_DATA_DEFAULT_PROFILE_I   		/* Default user AT command profile          */
NV_PAP_USER_ID_I            				318		;NV_PAP_USER_ID_I            		/* User_ID for Password Auth. Protocol      */
NV_PAP_PASSWORD_I           				319		;NV_PAP_PASSWORD_I           		/* Actual password for PAP                  */
NV_STA_TBYE_I               				320		;NV_STA_TBYE_I               		/* Num wakeup samples below thrshld */ /*320*/
NV_STA_MIN_THR_I            				321		;NV_STA_MIN_THR_I            		/* Threshold for Rx+Ec/Io (RSSI) trigger    */
NV_STA_MIN_RX_I             				322		;NV_STA_MIN_RX_I             		/* Threshold for Rx trigger                 */
NV_STA_MIN_ECIO_I           				323		;NV_STA_MIN_ECIO_I           		/* Threshold for Rx-Only idle trigger       */
NV_STA_PRI_I                				324		;NV_STA_PRI_I                		/* Switch to AMPS PRI setting               */
NV_PCS_RX_LIN_OFF_0_I       				325		;NV_PCS_RX_LIN_OFF_0_I       		/* PCS Rx linearizer offset                 */
NV_PCS_RX_LIN_SLP_I         				326		;NV_PCS_RX_LIN_SLP_I         		/* PCS Rx linearizer slope                  */
NV_PCS_RX_COMP_VS_FREQ_I    				327		;NV_PCS_RX_COMP_VS_FREQ_I    		/* PCS Rx gain comp vs frequency            */
NV_PCS_TX_COMP_VS_FREQ_I    				328		;NV_PCS_TX_COMP_VS_FREQ_I    		/* PCS Tx gain comp vs frequency            */
NV_PCS_TX_LIN_MASTER_OFF_0_I				329		;NV_PCS_TX_LIN_MASTER_OFF_0_I		/* PCS Tx linearizer master offset          */
NV_PCS_TX_LIN_MASTER_SLP_I  				330		;NV_PCS_TX_LIN_MASTER_SLP_I  		/* PCS Tx linearizer master slope   */ /*330*/
NV_PCS_TX_LIN_VS_TEMP_I     				331		;NV_PCS_TX_LIN_VS_TEMP_I     		/* PCS Tx linearizer trim vs temp           */
NV_PCS_TX_LIM_VS_TEMP_I     				332		;NV_PCS_TX_LIM_VS_TEMP_I     		/* PCS Tx power limit vs temperature        */
NV_PCS_TX_LIM_VS_FREQ_I     				333		;NV_PCS_TX_LIM_VS_FREQ_I     		/* PCS Tx power limit vs frequency          */
NV_PCS_EXP_HDET_VS_AGC_I    				334		;NV_PCS_EXP_HDET_VS_AGC_I    		/* PCS expected HDET reading vs AGC PDM     */
NV_PCS_HDET_OFF_I           				335		;NV_PCS_HDET_OFF_I           		/* ADC HDET reading offset                  */
NV_PCS_HDET_SPN_I           				336		;NV_PCS_HDET_SPN_I           		/* ADC HDET reading span                    */
NV_PCS_R1_RISE_I            				337		;NV_PCS_R1_RISE_I            		/* TX pwr lvl at which PA is stepped up     */
NV_PCS_R1_FALL_I            				338		;NV_PCS_R1_FALL_I            		/* TX pwr lvl at which PA is stepped down   */
NV_PCS_R2_RISE_I            				339		;NV_PCS_R2_RISE_I            		/* TX pwr lvl at which PA is stepped up     */
NV_PCS_R2_FALL_I            				340		;NV_PCS_R2_FALL_I            		/* TX pwr lvl at which PA stpd down */ /*340*/
NV_PCS_R3_RISE_I            				341		;NV_PCS_R3_RISE_I            		/* TX pwr lvl at which PA is stepped up     */
NV_PCS_R3_FALL_I            				342		;NV_PCS_R3_FALL_I            		/* TX pwr lvl at which PA is stepped down   */
NV_PCS_PA_RANGE_STEP_CAL_I  				343		;NV_PCS_PA_RANGE_STEP_CAL_I  		/* Calibrate PA Range gain step             */
NV_PCS_PDM1_VS_FREQ_I       				344		;NV_PCS_PDM1_VS_FREQ_I       		/* PDM1 vs frequency compensation table     */
NV_PCS_PDM2_VS_FREQ_I       				345		;NV_PCS_PDM2_VS_FREQ_I       		/* PDM2 vs frequency compensation table     */
NV_PCS_LNA_RANGE_POL_I      				346		;NV_PCS_LNA_RANGE_POL_I      		/* Polarity of LNA range control signal     */
NV_PCS_LNA_RANGE_RISE_I     				347		;NV_PCS_LNA_RANGE_RISE_I     		/* Rx pwr lvl for: LNA bypass               */
NV_PCS_LNA_RANGE_FALL_I     				348		;NV_PCS_LNA_RANGE_FALL_I     		/* Rx pwr lvl for: LNA turned on            */
NV_PCS_LNA_RANGE_OFFSET_I   				349		;NV_PCS_LNA_RANGE_OFFSET_I   		/* Rx pwr lvl offset when LNA is bypassed   */
NV_PCS_RX_LIN_VS_TEMP_I     				350		;NV_PCS_RX_LIN_VS_TEMP_I     		/* PCS Rx linearizer vs temperature */ /*350*/
NV_PCS_ADJ_FACTOR_I         				351		;NV_PCS_ADJ_FACTOR_I         		/* PCS adjustment factor                    */
NV_PCS_PA_RANGE_VS_TEMP_I   				352		;NV_PCS_PA_RANGE_VS_TEMP_I   		/* Changes in PA_RANGE_STEP over temp       */
NV_PCS_PDM1_VS_TEMP_I       				353		;NV_PCS_PDM1_VS_TEMP_I       		/* TX temperature compensation using PDM1   */
NV_PCS_PDM2_VS_TEMP_I       				354		;NV_PCS_PDM2_VS_TEMP_I       		/* TX temperature compensation using PDM2   */
NV_PCS_RX_SLP_VS_TEMP_I     				355		;NV_PCS_RX_SLP_VS_TEMP_I     		/* Slope of RX linearizer over temperature  */
NV_PCS_TX_SLP_VS_TEMP_I     				356		;NV_PCS_TX_SLP_VS_TEMP_I     		/* Slope of TX linearizer over temperature  */
NV_PCS_RX_AGC_MINMAX_I      				357		;NV_PCS_RX_AGC_MINMAX_I      		/* Receiver AGC min-max                     */
NV_PA_OFFSETS_I                                         358             ;NV_PA_OFFSETS_I                         
NV_CDMA_TX_LIN_MASTER_I     				359		;NV_CDMA_TX_LIN_MASTER_I     		/* Obsolete tx linearizer item              */
NV_VEXT_I                                               360           	;NV_VEXT_I                               /*360*/
NV_VLCD_ADC_CNT_I                                       361             ;NV_VLCD_ADC_CNT_I                       
NV_VLCD_DRVR_CNT_I                                      362             ;NV_VLCD_DRVR_CNT_I                      
NV_VREF_ADJ_PDM_CNT_I                                   363             ;NV_VREF_ADJ_PDM_CNT_I                   
NV_IBAT_PER_LSB_I                                       364             ;NV_IBAT_PER_LSB_I                       
NV_IEXT_I                                               365             ;NV_IEXT_I                               
NV_IEXT_THR_I                                           366             ;NV_IEXT_THR_I                           
NV_CDMA_TX_LIN_MASTER0_I                                367             ;NV_CDMA_TX_LIN_MASTER0_I                
NV_CDMA_TX_LIN_MASTER1_I                                368             ;NV_CDMA_TX_LIN_MASTER1_I                
NV_CDMA_TX_LIN_MASTER2_I                                369             ;NV_CDMA_TX_LIN_MASTER2_I                
NV_CDMA_TX_LIN_MASTER3_I                                370           	;NV_CDMA_TX_LIN_MASTER3_I                /*370*/
NV_TIME_FMT_SELECTION_I                                 371             ;NV_TIME_FMT_SELECTION_I                 
NV_SMS_BC_SERVICE_TABLE_SIZE_I                          372             ;NV_SMS_BC_SERVICE_TABLE_SIZE_I          
NV_SMS_BC_SERVICE_TABLE_I                               373             ;NV_SMS_BC_SERVICE_TABLE_I               
NV_SMS_BC_CONFIG_I                                      374             ;NV_SMS_BC_CONFIG_I                      
NV_SMS_BC_USER_PREF_I                                   375             ;NV_SMS_BC_USER_PREF_I                   
NV_LNA_RANGE_2_RISE_I                                   376             ;NV_LNA_RANGE_2_RISE_I                   
NV_LNA_RANGE_2_FALL_I                                   377             ;NV_LNA_RANGE_2_FALL_I                   
NV_LNA_RANGE_12_OFFSET_I                                378             ;NV_LNA_RANGE_12_OFFSET_I                
NV_NONBYPASS_TIMER_I                                    379             ;NV_NONBYPASS_TIMER_I                    
NV_BYPASS_TIMER_I                                       380           	;NV_BYPASS_TIMER_I                       /*380*/
NV_IM_LEVEL1_I                                          381             ;NV_IM_LEVEL1_I                          
NV_IM_LEVEL2_I                                          382             ;NV_IM_LEVEL2_I                          
NV_CDMA_LNA_OFFSET_VS_FREQ_I                            383             ;NV_CDMA_LNA_OFFSET_VS_FREQ_I            
NV_CDMA_LNA_12_OFFSET_VS_FREQ_I                         384             ;NV_CDMA_LNA_12_OFFSET_VS_FREQ_I         
NV_AGC_PHASE_OFFSET_I                                   385             ;NV_AGC_PHASE_OFFSET_I                   
NV_RX_AGC_MIN_11_I                                      386             ;NV_RX_AGC_MIN_11_I                      
NV_PCS_LNA_RANGE_2_RISE_I                               387             ;NV_PCS_LNA_RANGE_2_RISE_I               
NV_PCS_LNA_RANGE_2_FALL_I                               388             ;NV_PCS_LNA_RANGE_2_FALL_I               
NV_PCS_LNA_RANGE_12_OFFSET_I                            389             ;NV_PCS_LNA_RANGE_12_OFFSET_I            
NV_PCS_NONBYPASS_TIMER_I                                390           	;NV_PCS_NONBYPASS_TIMER_I                /*390*/
NV_PCS_BYPASS_TIMER_I                                   391             ;NV_PCS_BYPASS_TIMER_I                   
NV_PCS_IM_LEVEL1_I                                      392             ;NV_PCS_IM_LEVEL1_I                      
NV_PCS_IM_LEVEL2_I                                      393             ;NV_PCS_IM_LEVEL2_I                      
NV_PCS_CDMA_LNA_OFFSET_VS_FREQ_I                        394             ;NV_PCS_CDMA_LNA_OFFSET_VS_FREQ_I        
NV_PCS_CDMA_LNA_12_OFFSET_VS_FREQ_I                     395             ;NV_PCS_CDMA_LNA_12_OFFSET_VS_FREQ_I     
NV_PCS_AGC_PHASE_OFFSET_I                               396             ;NV_PCS_AGC_PHASE_OFFSET_I               
NV_PCS_RX_AGC_MIN_11_I                                  397             ;NV_PCS_RX_AGC_MIN_11_I                  
NV_RUIM_CHV_1_I                 			398		;NV_RUIM_CHV_1_I                 	 /* Card holder verification 1 for R-UIM */
NV_RUIM_CHV_2_I                 			399		;NV_RUIM_CHV_2_I                 	 /* Card holder verification 2 for R-UIM */
NV_GPS1_CAPABILITIES_I          			400		;NV_GPS1_CAPABILITIES_I          	 /* GPS One Capabilities */
NV_GPS1_PDE_ADDRESS_I           			401		;NV_GPS1_PDE_ADDRESS_I           	 /* GPS One PDE TCP Address */ 
NV_GPS1_ALLOWED_I   					402		;NV_GPS1_ALLOWED_I   			 /* GPS One Position Determination Services Lock-out */
NV_GPS1_PDE_TRANSPORT_I        				403		;NV_GPS1_PDE_TRANSPORT_I        	 	/* GPS One Preferred transport mechanism */
NV_GPS1_MOBILE_CALC_I                                   404             ;NV_GPS1_MOBILE_CALC_I                    
NV_PREF_FOR_RC_I        				405		;NV_PREF_FOR_RC_I        		 /* IS2000 CAI radio configuration RC preference */
NV_DS_DEFAULT_BAUD_I             			406		;NV_DS_DEFAULT_BAUD_I             	 /* DATA SERVICES default SIO baud rate */  
NV_DIAG_DEFAULT_BAUD_I                    		407		;NV_DIAG_DEFAULT_BAUD_I                   /* DIAG default SIO baud rate */                
NV_SIO_DEV_MAP_MENU_ITEM_I                              408             ;NV_SIO_DEV_MAP_MENU_ITEM_I               
NV_TTY_I                				409		;NV_TTY_I                		 /* Specifies whether TTY is enabled or disabled */
NV_PA_RANGE_OFFSETS_I                                   410             ;NV_PA_RANGE_OFFSETS_I                    
NV_TX_COMP0_I  						411		;NV_TX_COMP0_I  			 	/* For temp. and freq. compensation of the Tx linearizer */  
NV_MM_SDAC_LVL_I                  			412		;NV_MM_SDAC_LVL_I                  	 /* Stereo DAC Multimedia volume level */
NV_BEEP_SDAC_LVL_I                  			413		;NV_BEEP_SDAC_LVL_I                  	 /* Stereo DAC key beep volume level */
NV_SDAC_LVL_I                                		414		;NV_SDAC_LVL_I                            /* Stereo DAC volume level */
NV_MM_LVL_I                          			415		;NV_MM_LVL_I                          	 /* Handset Multimedia volume level */  
NV_MM_LVL_SHADOW_I                   			416		;NV_MM_LVL_SHADOW_I                   	 /* Headset Multimedia volume level */
NV_MM_SPEAKER_LVL_I                      		417		;NV_MM_SPEAKER_LVL_I                      /* HFK Multimedia volume level */
NV_MM_PLAY_MODE_I                               	418		;NV_MM_PLAY_MODE_I                        /* Multimedia play mode */
NV_MM_REPEAT_MODE_I                           		419		;NV_MM_REPEAT_MODE_I                      /* Multimedia repeat mode */
NV_TX_COMP1_I  						420		;NV_TX_COMP1_I  			 	/* For temp. and freq. compensation of the Tx linearizer */  
NV_TX_COMP2_I  						421		;NV_TX_COMP2_I  			 	/* For temp. and freq. compensation of the Tx linearizer */  
NV_TX_COMP3_I  						422		;NV_TX_COMP3_I  			 	/* For temp. and freq. compensation of the Tx linearizer */
NV_PRIMARY_DNS_I           				423		;NV_PRIMARY_DNS_I           		 /* Contains the IP Address of the DNS Server */  
NV_SECONDARY_DNS_I                                      424             ;NV_SECONDARY_DNS_I                       
NV_DIAG_PORT_SELECT_I             	 		425		;NV_DIAG_PORT_SELECT_I             	 /* Info for DIAG boot port selection */
NV_GPS1_PDE_PORT_I        				426		;NV_GPS1_PDE_PORT_I        		 /* Listening port associated with PDE address */
NV_MM_RINGER_FILE_I       				427		;NV_MM_RINGER_FILE_I       		 /* Multimedia ringer filename */
NV_MM_STORAGE_DEVICE_I    				428		;NV_MM_STORAGE_DEVICE_I    		 /* Multimedia file location */
NV_DATA_SCRM_ENABLED_I 					429		;NV_DATA_SCRM_ENABLED_I 		 	/* Enables/disables the mobile's ability to SCRM */
NV_RUIM_SMS_STATUS_I                                    430        	;NV_RUIM_SMS_STATUS_I                             
NV_PCS_TX_LIN_MASTER0_I        				431		;NV_PCS_TX_LIN_MASTER0_I        	 	/* PCS Tx linearizer with internal PA=00 */
NV_PCS_TX_LIN_MASTER1_I        				432		;NV_PCS_TX_LIN_MASTER1_I        	 	/* PCS Tx linearizer with internal PA=01 */
NV_PCS_TX_LIN_MASTER2_I        				433		;NV_PCS_TX_LIN_MASTER2_I        	 	/* PCS Tx linearizer with internal PA=10 */
NV_PCS_TX_LIN_MASTER3_I        				434		;NV_PCS_TX_LIN_MASTER3_I        	 	/* PCS Tx linearizer with internal PA=11 */
NV_PCS_PA_RANGE_OFFSETS_I                       	435		;NV_PCS_PA_RANGE_OFFSETS_I                /* PCS PA range offsets */
NV_PCS_TX_COMP0_I        				436		;NV_PCS_TX_COMP0_I        		 /* PCS transmit frequency compensation table 0 */  
NV_PCS_TX_COMP1_I        				437		;NV_PCS_TX_COMP1_I        		 /* PCS transmit frequency compensation table 1 */  
NV_PCS_TX_COMP2_I        				438		;NV_PCS_TX_COMP2_I        		 /* PCS transmit frequency compensation table 2 */  
NV_PCS_TX_COMP3_I        				439		;NV_PCS_TX_COMP3_I        		 /* PCS transmit frequency compensation table 3 */
NV_DIAG_RESTART_CONFIG_I                                440             ;NV_DIAG_RESTART_CONFIG_I                 
NV_BAND_PREF_I   					441		;NV_BAND_PREF_I   			 /* Stores the band-class preference on a per NAM basis */
NV_ROAM_PREF_I      					442		;NV_ROAM_PREF_I      			 /* Stores the roaming preference on a per NAM basis */
NV_GPS1_GPS_RF_DELAY_I                          	443		;NV_GPS1_GPS_RF_DELAY_I                   /* GPS RF Signal Delay */
NV_GPS1_CDMA_RF_DELAY_I                         	444		;NV_GPS1_CDMA_RF_DELAY_I                  /* CDMA RF Signal Delay */
NV_PCS_ENC_BTF_I                                        445             ;NV_PCS_ENC_BTF_I                         
NV_CDMA_ENC_BTF_I                                       446             ;NV_CDMA_ENC_BTF_I                        
NV_BD_ADDR_I               				447		;NV_BD_ADDR_I               		 /* Holds the Bluetooth address of the mobile */
NV_SUBPCG_PA_WARMUP_DELAY_I				448		;NV_SUBPCG_PA_WARMUP_DELAY_I            
NV_GPS1_GPS_RF_LOSS_I                                   449             ;NV_GPS1_GPS_RF_LOSS_I
NV_DATA_TRTL_ENABLED_I                                  450             ;NV_DATA_TRTL_ENABLED_I                  
NV_AMPS_BACKSTOP_ENABLED_I       			451		;NV_AMPS_BACKSTOP_ENABLED_I       	/* AMPS backstop system enabled status */
NV_GPS1_LOCK_I                                   	452		;NV_GPS1_LOCK_I                          /* GPS One lock status */ 
NV_FTM_MODE_I    					453		;NV_FTM_MODE_I    			/* Determines boot up mode of a factory testmode phone */
NV_DS_DEFAULT_BAUDRATE_I                                454             ;NV_DS_DEFAULT_BAUDRATE_I                
NV_DIAG_DEFAULT_BAUDRATE_I                              455             ;NV_DIAG_DEFAULT_BAUDRATE_I              
NV_JCDMA_DS_F92_I                  			456		;NV_JCDMA_DS_F92_I                  	/* Stores JCDMA F92 option selected  */
NV_IMEI_I                                               457             ;NV_IMEI_I                               
NV_IMEI_CHKSUM_I                                        458             ;NV_IMEI_CHKSUM_I                        
NV_DS_QCMIP_I                        			459		;NV_DS_QCMIP_I                        	/* The mode for Mobile IP behavior */
NV_DS_MIP_RETRIES_I                                     460             ;NV_DS_MIP_RETRIES_I                     
NV_DS_MIP_RETRY_INT_I                                   461             ;NV_DS_MIP_RETRY_INT_I                   
NV_DS_MIP_PRE_RE_RRQ_TIME_I                             462             ;NV_DS_MIP_PRE_RE_RRQ_TIME_I             
NV_DS_MIP_NUM_PROF_I        				463		;NV_DS_MIP_NUM_PROF_I        		/* Number of Mobile IP user profiles stored */
NV_DS_MIP_ACTIVE_PROF_I  				464		;NV_DS_MIP_ACTIVE_PROF_I  		/* The currently active Mobile IP user profile */
NV_DS_MIP_GEN_USER_PROF_I                               465             ;NV_DS_MIP_GEN_USER_PROF_I               
NV_DS_MIP_SS_USER_PROF_I                                466             ;NV_DS_MIP_SS_USER_PROF_I                
NV_HDR_CON_SUSPEND_I                                    467             ;NV_HDR_CON_SUSPEND_I                    
NV_HDR_PRE_CC_CYC_ENABLED_I                             468             ;NV_HDR_PRE_CC_CYC_ENABLED_I             
NV_HDR_PRE_CC_CYC_I                                     469             ;NV_HDR_PRE_CC_CYC_I                     
NV_HDR_SRCH_PARAMS_I                                    470             ;NV_HDR_SRCH_PARAMS_I                    
NV_HDRSMP_KEEP_ALIVE_START_I                            471             ;NV_HDRSMP_KEEP_ALIVE_START_I            
NV_HDRSMP_KEEP_ALIVE_SENT_I                             472             ;NV_HDRSMP_KEEP_ALIVE_SENT_I             
NV_HDRSMP_KEEP_ALIVE_REQ_INT_I                          473             ;NV_HDRSMP_KEEP_ALIVE_REQ_INT_I          
NV_HDRAMP_ADDRESS_DATA_I                                474             ;NV_HDRAMP_ADDRESS_DATA_I                
NV_HDRSCP_SESSION_STATUS_I                              475             ;NV_HDRSCP_SESSION_STATUS_I              
NV_HDRSCP_TOKEN_I                                       476             ;NV_HDRSCP_TOKEN_I                       
NV_HDRSCP_PROTOCOL_SUBTYPE_I                            477             ;NV_HDRSCP_PROTOCOL_SUBTYPE_I            
NV_HDRAMP_DUAL_EXPIRE_TIME_I                            478             ;NV_HDRAMP_DUAL_EXPIRE_TIME_I            
NV_HDRSTREAM_CURR_STREAM_CFG_I                          479             ;NV_HDRSTREAM_CURR_STREAM_CFG_I          
NV_HDR_SET_MNGMT_SAME_CHAN_I                            480             ;NV_HDR_SET_MNGMT_SAME_CHAN_I            
NV_HDR_SET_MNGMT_DIFF_CHAN_I                            481             ;NV_HDR_SET_MNGMT_DIFF_CHAN_I            
NV_HDRLUP_UNSOLICITED_ENABLED_I                         482             ;NV_HDRLUP_UNSOLICITED_ENABLED_I         
NV_HDRAMAC_INITIAL_CONFIG_I                             483             ;NV_HDRAMAC_INITIAL_CONFIG_I             
NV_HDRAMAC_POWER_PARAMS_I                               484             ;NV_HDRAMAC_POWER_PARAMS_I               
NV_HDRFMAC_DRC_GATING_I                                 485             ;NV_HDRFMAC_DRC_GATING_I                 
NV_HDRFMAC_HANDOFF_DELAYS_I                             486             ;NV_HDRFMAC_HANDOFF_DELAYS_I             
NV_HDRRMAC_POWER_PARAMS_I                               487             ;NV_HDRRMAC_POWER_PARAMS_I               
NV_HDRRMAC_RATE_PARAMS_I                                488             ;NV_HDRRMAC_RATE_PARAMS_I                
NV_HDRSLP_RESET_SEQNO_I                                 489             ;NV_HDRSLP_RESET_SEQNO_I                 
NV_PWR_BACKOFF_VS_VOLT_MED_I                            490             ;NV_PWR_BACKOFF_VS_VOLT_MED_I            	/*490*/
NV_PWR_BACKOFF_VS_VOLT_LOW_I                            491             ;NV_PWR_BACKOFF_VS_VOLT_LOW_I            
NV_PA_BACKOFF_VOLTS_I                                   492             ;NV_PA_BACKOFF_VOLTS_I                   
NV_VBATT_MIN_MAX_I                                      493             ;NV_VBATT_MIN_MAX_I                      
NV_DS_MIP_MN_HA_TIME_DELTA_I                            494             ;NV_DS_MIP_MN_HA_TIME_DELTA_I            
NV_DS_MIP_QC_DRS_OPT_I                                  495             ;NV_DS_MIP_QC_DRS_OPT_I                  
NV_ANT2_CDMA_RX_LIN_OFF_0_I                             496             ;NV_ANT2_CDMA_RX_LIN_OFF_0_I             
NV_ANT2_CDMA_RX_LIN_SLP_I                               497             ;NV_ANT2_CDMA_RX_LIN_SLP_I               
NV_ANT2_CDMA_RX_COMP_VS_FREQ_I                          498             ;NV_ANT2_CDMA_RX_COMP_VS_FREQ_I          
NV_ANT2_CDMA_RX_LIN_VS_TEMP_I                           499             ;NV_ANT2_CDMA_RX_LIN_VS_TEMP_I           
NV_ANT2_CDMA_RX_SLP_VS_TEMP_I                           500             ;NV_ANT2_CDMA_RX_SLP_VS_TEMP_I           
NV_ANT2_LNA_RANGE_OFFSET_I                              501             ;NV_ANT2_LNA_RANGE_OFFSET_I              
NV_ANT2_LNA_RANGE_12_OFFSET_I                           502             ;NV_ANT2_LNA_RANGE_12_OFFSET_I           
NV_ANT2_CDMA_LNA_OFFSET_VS_FREQ_I                       503             ;NV_ANT2_CDMA_LNA_OFFSET_VS_FREQ_I       
NV_ANT2_CDMA_LNA_12_OFFSET_VS_FREQ_I                    504             ;NV_ANT2_CDMA_LNA_12_OFFSET_VS_FREQ_I    
NV_ANT2_PCS_RX_LIN_OFF_0_I                              505             ;NV_ANT2_PCS_RX_LIN_OFF_0_I              
NV_ANT2_PCS_RX_LIN_SLP_I                                506             ;NV_ANT2_PCS_RX_LIN_SLP_I                
NV_ANT2_PCS_RX_COMP_VS_FREQ_I                           507             ;NV_ANT2_PCS_RX_COMP_VS_FREQ_I           
NV_ANT2_PCS_RX_LIN_VS_TEMP_I                            508             ;NV_ANT2_PCS_RX_LIN_VS_TEMP_I            
NV_ANT2_PCS_RX_SLP_VS_TEMP_I                            509             ;NV_ANT2_PCS_RX_SLP_VS_TEMP_I            
NV_ANT2_PCS_LNA_RANGE_OFFSET_I                          510             ;NV_ANT2_PCS_LNA_RANGE_OFFSET_I          
NV_ANT2_PCS_LNA_RANGE_12_OFFSET_I                       511             ;NV_ANT2_PCS_LNA_RANGE_12_OFFSET_I      		 
NV_ANT2_PCS_CDMA_LNA_OFFSET_VS_FREQ_I                   512             ;NV_ANT2_PCS_CDMA_LNA_OFFSET_VS_FREQ_I  		 
NV_ANT2_PCS_CDMA_LNA_12_OFFSET_VS_FREQ_I                513             ;NV_ANT2_PCS_CDMA_LNA_12_OFFSET_VS_FREQ_I
NV_WCDMA_RX_LIN_I                                       514             ;NV_WCDMA_RX_LIN_I                       
NV_WCDMA_RX_COMP_VS_FREQ_I                              515             ;NV_WCDMA_RX_COMP_VS_FREQ_I              
NV_WCDMA_RX_LIN_VS_TEMP_I                               516             ;NV_WCDMA_RX_LIN_VS_TEMP_I               
NV_WCDMA_RX_SLP_VS_TEMP_I                               517             ;NV_WCDMA_RX_SLP_VS_TEMP_I               
NV_WCDMA_LNA_RANGE_POL_I                                518             ;NV_WCDMA_LNA_RANGE_POL_I                
NV_WCDMA_LNA_RANGE_RISE_I                               519             ;NV_WCDMA_LNA_RANGE_RISE_I               
NV_WCDMA_LNA_RANGE_FALL_I                               520             ;NV_WCDMA_LNA_RANGE_FALL_I               
NV_WCDMA_IM_LEVEL_I                                     521             ;NV_WCDMA_IM_LEVEL_I                     
NV_WCDMA_NONBYPASS_TIMER_I                              522             ;NV_WCDMA_NONBYPASS_TIMER_I              
NV_WCDMA_BYPASS_TIMER_I                                 523             ;NV_WCDMA_BYPASS_TIMER_I                 
NV_WCDMA_LNA_RANGE_OFFSET_I                             524             ;NV_WCDMA_LNA_RANGE_OFFSET_I             
NV_WCDMA_LNA_OFFSET_VS_FREQ_I                           525             ;NV_WCDMA_LNA_OFFSET_VS_FREQ_I           
NV_WCDMA_RX_AGC_MIN_I                                   526             ;NV_WCDMA_RX_AGC_MIN_I                   
NV_WCDMA_RX_AGC_MAX_I                                   527             ;NV_WCDMA_RX_AGC_MAX_I                   
NV_WCDMA_AGC_PHASE_OFFSET_I                             528             ;NV_WCDMA_AGC_PHASE_OFFSET_I             
NV_WCDMA_TX_LIN_MASTER_0_I                              529             ;NV_WCDMA_TX_LIN_MASTER_0_I              
NV_WCDMA_TX_LIN_MASTER_1_I                              530             ;NV_WCDMA_TX_LIN_MASTER_1_I              
NV_WCDMA_TX_COMP_VS_FREQ_0_I                            531             ;NV_WCDMA_TX_COMP_VS_FREQ_0_I            
NV_WCDMA_TX_COMP_VS_FREQ_1_I                            532             ;NV_WCDMA_TX_COMP_VS_FREQ_1_I            
NV_WCDMA_TX_LIN_VS_TEMP_0_I                             533             ;NV_WCDMA_TX_LIN_VS_TEMP_0_I             
NV_WCDMA_TX_LIN_VS_TEMP_1_I                             534             ;NV_WCDMA_TX_LIN_VS_TEMP_1_I             
NV_WCDMA_TX_SLP_VS_TEMP_0_I                             535             ;NV_WCDMA_TX_SLP_VS_TEMP_0_I             
NV_WCDMA_TX_SLP_VS_TEMP_1_I                             536             ;NV_WCDMA_TX_SLP_VS_TEMP_1_I             
NV_WCDMA_R1_RISE_I                                      537             ;NV_WCDMA_R1_RISE_I                      
NV_WCDMA_R1_FALL_I                                      538             ;NV_WCDMA_R1_FALL_I                      
NV_WCDMA_TX_LIM_VS_TEMP_I                               539             ;NV_WCDMA_TX_LIM_VS_TEMP_I               
NV_WCDMA_TX_LIM_VS_FREQ_I                               540             ;NV_WCDMA_TX_LIM_VS_FREQ_I               
NV_WCDMA_ADJ_FACTOR_I                                   541             ;NV_WCDMA_ADJ_FACTOR_I                   
NV_WCDMA_EXP_HDET_VS_AGC_I                              542             ;NV_WCDMA_EXP_HDET_VS_AGC_I              
NV_WCDMA_HDET_OFF_I                                     543             ;NV_WCDMA_HDET_OFF_I                     
NV_WCDMA_HDET_SPN_I                                     544             ;NV_WCDMA_HDET_SPN_I                     
NV_WCDMA_ENC_BTF_I                                      545             ;NV_WCDMA_ENC_BTF_I                      
NV_DS_MIP_2002BIS_MN_HA_AUTH_I                          546             ;NV_DS_MIP_2002BIS_MN_HA_AUTH_I          
NV_DIAL_TONE_I						547  		;NV_DIAL_TONE_I				/*563*/
NV_HOWLER_TONE_I                                        548             ;NV_HOWLER_TONE_I                        
NV_NO_SERVICE_TONE_I                                    549             ;NV_NO_SERVICE_TONE_I                    
NV_OUTGOING_CALL_RESTRICTION_TONE_I                     550             ;NV_OUTGOING_CALL_RESTRICTION_TONE_I     
NV_ONE_MINUTE_ALERT_TONE_I                              551             ;NV_ONE_MINUTE_ALERT_TONE_I              
NV_LOW_BATTERY_ALERT_TONE_I                             552             ;NV_LOW_BATTERY_ALERT_TONE_I             
NV_V_MAIL_TONE_I	      				553		;NV_V_MAIL_TONE_I	      		/*???*/
NV_WAKE_UP_TONE_I                                       554             ;NV_WAKE_UP_TONE_I                       
NV_ALERT_TONE_I                                         555             ;NV_ALERT_TONE_I                         
NV_BUSY_TONE_I                                          556             ;NV_BUSY_TONE_I                          
NV_TONE_ONE_I                                           557             ;NV_TONE_ONE_I                           
NV_TONE_TWO_I                                           558             ;NV_TONE_TWO_I                           
NV_TONE_THREE_I                                         559             ;NV_TONE_THREE_I                         
NV_ALARM_I                                              560             ;NV_ALARM_I                              
NV_ALARM_TIME_I                                         561             ;NV_ALARM_TIME_I                         
NV_OUTGOING_RES_I                                       562             ;NV_OUTGOING_RES_I                       
NV_INTERNATIONAL_RES_I                                  563             ;NV_INTERNATIONAL_RES_I                  
NV_INCOMING_RES_I                                       564             ;NV_INCOMING_RES_I                       
NV_LONG_DISTANCE_RES_I                                  565             ;NV_LONG_DISTANCE_RES_I                  
NV_CLEAR_MEMORY_I                                       566             ;NV_CLEAR_MEMORY_I                       
NV_RESET_PHONE_I                                        567             ;NV_RESET_PHONE_I                        
NV_AUTO_SEND_TIME_I                                     568             ;NV_AUTO_SEND_TIME_I                     
NV_ALERT_TYPE_I                                         569             ;NV_ALERT_TYPE_I                         
NV_LANGUAGE_SELECT_I                                    570             ;NV_LANGUAGE_SELECT_I                    
NV_FLASH_TIME_MIN_I                                     571             ;NV_FLASH_TIME_MIN_I                     
NV_FLASH_TIME_MAX_I                                     572             ;NV_FLASH_TIME_MAX_I                     
NV_FIRST_DIGIT_TIME_I                                   573             ;NV_FIRST_DIGIT_TIME_I                   
NV_APM_24_TIME_I                                        574             ;NV_APM_24_TIME_I                        
NV_ALARM_TONE_I                                         575             ;NV_ALARM_TONE_I                         
NV_DAILY_ONETIME_I                                      576             ;NV_DAILY_ONETIME_I                      
NV_ALARM_DURATION_I                                     577             ;NV_ALARM_DURATION_I                     
NV_ONETIME_CHECK_I                                      578             ;NV_ONETIME_CHECK_I                      
NV_LIFE_TIMER_ALERT_G_I                                 579             ;NV_LIFE_TIMER_ALERT_G_I                 
NV_SEND_SMS_I                                           580             ;NV_SEND_SMS_I                           
NV_CNI_IDX_I                                            581             ;NV_CNI_IDX_I                            
NV_SEND_SMS_IDX_I                                       582             ;NV_SEND_SMS_IDX_I                       
NV_SMS_LOCK_I                                           583             ;NV_SMS_LOCK_I                           
NV_SMS_ALERT_I                                          584             ;NV_SMS_ALERT_I                          
NV_CNI_I                                                585             ;NV_CNI_I                                
NV_CONFIRM_SMS_I                                        586             ;NV_CONFIRM_SMS_I                        
NV_DS_COM_PORT_SEL_I                                    587             ;NV_DS_COM_PORT_SEL_I                    
NV_DS_SPEED_SEL_I                                       588             ;NV_DS_SPEED_SEL_I                       
NV_DS_RECEIVE_MODE_SEL_I                                589             ;NV_DS_RECEIVE_MODE_SEL_I                
NV_HOT_LINE_I                                           590             ;NV_HOT_LINE_I                           
NV_VOICEMAIL_DIAL_NUMBER_I                              591             ;NV_VOICEMAIL_DIAL_NUMBER_I
NV_DIAL_TONE_VOL_I                                      592             ;NV_DIAL_TONE_VOL_I                      
NV_ALERT_TONE_VOL_I                                     593             ;NV_ALERT_TONE_VOL_I                     
NV_HOWLER_TONE_VOL_I                                    594             ;NV_HOWLER_TONE_VOL_I                    
NV_START_TONE_VOL_I                                     595             ;NV_START_TONE_VOL_I                     
NV_RES_OUT_TONE_VOL_I                                   596             ;NV_RES_OUT_TONE_VOL_I                   
NV_VMAIL_TONE_VOL_I                                     597             ;NV_VMAIL_TONE_VOL_I                     
NV_ONEMIN_ALERT_TONE_VOL_I                              598             ;NV_ONEMIN_ALERT_TONE_VOL_I              
NV_LOWBATT_TONE_VOL_I                                   599             ;NV_LOWBATT_TONE_VOL_I                   
NV_FCOMP_TONE_VOL_I                                     600             ;NV_FCOMP_TONE_VOL_I                     
NV_BUSY_TONE_VOL_I                                      601             ;NV_BUSY_TONE_VOL_I                      
NV_IN_USE_UNITS_I                                       602             ;NV_IN_USE_UNITS_I                       
NV_IN_USE_TOTAL_UNITS_I                                 603             ;NV_IN_USE_TOTAL_UNITS_I                 
NV_PHONE_TOTAL_UNITS_I                                  604             ;NV_PHONE_TOTAL_UNITS_I
NV_CONNECT_BEEP_I					605		; beep select
NV_COUNTRY_SELECT_I  					606		; country function select
NV_MISSED_IDX_I	  					607		;	
NV_MISSED_I						608		;	
NV_PRIVACY_BEEP_I					609 		;
NV_SMS_ACK_I 						610		;
NV_HSPN_IND_I 						611		;
NV_ICCID_I						612		;
NV_ROMSIM_I           					613		;
NV_MAX_I                                                614             ;NV_MAX_I