NV_FM_RSSI_I,95,ReadWrite,<BYTE,Minimum Analog RSSI adjustment>#<BYTE,Maximum Analog RSSI adjustment>#
NV_CDMA_RX_COMP_VS_FREQ_I,129,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_CDMA_RX_LIN_OFF_0_I,127,ReadWrite,<BYTE,CDMA mode RX linearizer offset>#
NV_CDMA_RX_LIN_SLP_I,128,ReadWrite,<BYTE,Array[0]>#<BYTE,Array[1]>#<BYTE,Array[2]>#<BYTE,Array[3]>#<BYTE,Array[4]>#<BYTE,Array[5]>#<BYTE,Array[6]>#<BYTE,Array[7]>#<BYTE,Array[8]>#<BYTE,Array[9]>#<BYTE,Array[10]>#<BYTE,Array[11]>#<BYTE,Array[12]>#<BYTE,Array[13]>#<BYTE,Array[14]>#<BYTE,Array[15]>#
NV_CDMA_TX_COMP_VS_FREQ_I,130,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_CDMA_TX_LIN_MASTER_OFF_0_I,132,ReadWrite,<WORD,CDMA TX linearizer master offset>#
NV_CDMA_TX_LIN_MASTER_SLP_I,133,ReadWrite,<BYTE,Array[0]>#<BYTE,Array[1]>#<BYTE,Array[2]>#<BYTE,Array[3]>#<BYTE,Array[4]>#<BYTE,Array[5]>#<BYTE,Array[6]>#<BYTE,Array[7]>#<BYTE,Array[8]>#<BYTE,Array[9]>#<BYTE,Array[10]>#<BYTE,Array[11]>#<BYTE,Array[12]>#<BYTE,Array[13]>#<BYTE,Array[14]>#<BYTE,Array[15]>#<BYTE,Array[16]>#<BYTE,Array[17]>#<BYTE,Array[18]>#<BYTE,Array[19]>#<BYTE,Array[20]>#<BYTE,Array[21]>#<BYTE,Array[22]>#<BYTE,Array[23]>#<BYTE,Array[24]>#<BYTE,Array[25]>#<BYTE,Array[26]>#<BYTE,Array[27]>#<BYTE,Array[28]>#<BYTE,Array[29]>#<BYTE,Array[30]>#<BYTE,Array[31]>#<BYTE,Array[32]>#<BYTE,Array[33]>#<BYTE,Array[34]>#<BYTE,Array[35]>#
NV_CDMA_TX_LIM_VS_TEMP_I,136,ReadWrite,<BYTE,Array[0]>#<BYTE,Array[1]>#<BYTE,Array[2]>#<BYTE,Array[3]>#<BYTE,Array[4]>#<BYTE,Array[5]>#<BYTE,Array[6]>#<BYTE,Array[7]>#
NV_HDET_OFF_I,143,ReadWrite,<BYTE,ADC HDET reading offset>#
NV_HDET_SPN_I,144,ReadWrite,<BYTE,ADC HDET reading span>#
NV_CDMA_ERR_SLP_VS_HDET_I,140,ReadWrite,<BYTE,Array[0]>#<BYTE,Array[1]>#<BYTE,Array[2]>#<BYTE,Array[3]>#<BYTE,Array[4]>#<BYTE,Array[5]>#<BYTE,Array[6]>#<BYTE,Array[7]>#
NV_CDMA_EXP_HDET_VS_AGC_I,139,ReadWrite,<BYTE,Array[0]>#<BYTE,Array[1]>#<BYTE,Array[2]>#<BYTE,Array[3]>#<BYTE,Array[4]>#<BYTE,Array[5]>#<BYTE,Array[6]>#<BYTE,Array[7]>#<BYTE,Array[8]>#<BYTE,Array[9]>#<BYTE,Array[10]>#<BYTE,Array[11]>#<BYTE,Array[12]>#<BYTE,Array[13]>#<BYTE,Array[14]>#<BYTE,Array[15]>#
NV_CDMA_TX_LIM_VS_FREQ_I,138,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_CDMA_TX_LIN_VS_TEMP_I,134,ReadWrite,<BYTE,Array[0]>#<BYTE,Array[1]>#<BYTE,Array[2]>#<BYTE,Array[3]>#<BYTE,Array[4]>#<BYTE,Array[5]>#<BYTE,Array[6]>#<BYTE,Array[7]>#
NV_THERM_I,141,ReadWrite,<BYTE,Minimum>#<BYTE,Maximum>#
NV_R1_RISE_I,149,ReadWrite,<BYTE,R1 rise>#
NV_R1_FALL_I,150,ReadWrite,<BYTE,R1 fall>#
NV_R2_RISE_I,151,ReadWrite,<BYTE,R2 rise>#
NV_R2_FALL_I,152,ReadWrite,<BYTE,R2 fall>#
NV_R3_RISE_I,153,ReadWrite,<BYTE,R3 rise>#
NV_R3_FALL_I,154,ReadWrite,<BYTE,R3 fall>#
NV_LNA_RANGE_POL_I,156,ReadWrite,<BYTE,LNA range polarity>#
NV_LNA_RANGE_RISE_I,157,ReadWrite,<SIGNED_BYTE,LNA range rise>#
NV_LNA_RANGE_FALL_I,158,ReadWrite,<SIGNED_BYTE,LNA range fall>#
NV_LNA_RANGE_OFFSET_I,159,ReadWrite,<WORD,LNA range offset>#
NV_CDMA_TX_COMP_VS_VOLT_I,131,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#
NV_CDMA_TX_LIM_VS_VOLT_I,137,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#
NV_CDMA_TX_LIN_VS_VOLT_I,135,ReadWrite,<BYTE,Array[0]>#<BYTE,Array[1]>#<BYTE,Array[2]>#<BYTE,Array[3]>#<BYTE,Array[4]>#<BYTE,Array[5]>#<BYTE,Array[6]>#<BYTE,Array[7]>#
NV_RF_CONFIG_I,148,ReadWrite,<BYTE,RF configuration>#
NV_VBATT_PA_I,142,ReadWrite,<BYTE,Minimum>#<BYTE,Maximum>#
NV_PA_RANGE_STEP_CAL_I,155,ReadWrite,<BYTE,PA range step calibration>#
NV_PDM2_I,246,ReadWrite,<BYTE,PDM2>#
NV_PDM1_I,251,ReadWrite,<BYTE,PDM1>#
NV_PDM1_VS_TEMP_I,253,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#
NV_PDM2_VS_TEMP_I,254,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#
NV_PDM1_VS_FREQ_I,288,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_PDM2_VS_FREQ_I,289,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_FM_AGC_SET_VS_PWR_I,121,ReadWrite,<BYTE,Array[0]>#<BYTE,Array[1]>#<BYTE,Array[2]>#<BYTE,Array[3]>#<BYTE,Array[4]>#<BYTE,Array[5]>#<BYTE,Array[6]>#<BYTE,Array[7]>#<BYTE,Array[8]>#<BYTE,Array[9]>#<BYTE,Array[10]>#<BYTE,Array[11]>#<BYTE,Array[12]>#<BYTE,Array[13]>#<BYTE,Array[14]>#<BYTE,Array[15]>#
NV_FM_EXP_HDET_VS_PWR_I,124,ReadWrite,<BYTE,Array[0]>#<BYTE,Array[1]>#<BYTE,Array[2]>#<BYTE,Array[3]>#<BYTE,Array[4]>#<BYTE,Array[5]>#<BYTE,Array[6]>#<BYTE,Array[7]>#<BYTE,Array[8]>#<BYTE,Array[9]>#<BYTE,Array[10]>#<BYTE,Array[11]>#<BYTE,Array[12]>#<BYTE,Array[13]>#<BYTE,Array[14]>#<BYTE,Array[15]>#
NV_FM_ERR_SLP_VS_PWR_I,125,ReadWrite,<BYTE,Array[0]>#<BYTE,Array[1]>#<BYTE,Array[2]>#<BYTE,Array[3]>#<BYTE,Array[4]>#<BYTE,Array[5]>#<BYTE,Array[6]>#<BYTE,Array[7]>#<BYTE,Array[8]>#<BYTE,Array[9]>#<BYTE,Array[10]>#<BYTE,Array[11]>#<BYTE,Array[12]>#<BYTE,Array[13]>#<BYTE,Array[14]>#<BYTE,Array[15]>#
NV_VBATT_I,90,ReadWrite,<BYTE,Minimum>#<BYTE,Maximum>#
NV_FM_AGC_SET_VS_FREQ_I,122,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_FM_AGC_ADJ_VS_FREQ_I,146,ReadWrite,<BYTE,Array[0]>#<BYTE,Array[1]>#<BYTE,Array[2]>#<BYTE,Array[3]>#<BYTE,Array[4]>#<BYTE,Array[5]>#<BYTE,Array[6]>#<BYTE,Array[7]>#<BYTE,Array[8]>#<BYTE,Array[9]>#<BYTE,Array[10]>#<BYTE,Array[11]>#<BYTE,Array[12]>#<BYTE,Array[13]>#<BYTE,Array[14]>#<BYTE,Array[15]>#
NV_FM_FREQ_SENSE_GAIN_I,126,ReadWrite,<BYTE,FM frequency sense gain>#
NV_FM_AGC_ADJ_VS_TEMP_I,147,ReadWrite,<BYTE,Array[0]>#<BYTE,Array[1]>#<BYTE,Array[2]>#<BYTE,Array[3]>#<BYTE,Array[4]>#<BYTE,Array[5]>#<BYTE,Array[6]>#<BYTE,Array[7]>#
NV_FM_AGC_SET_VS_TEMP_I,123,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#
NV_FM_AGC_I,194,ReadWrite,<BYTE,Minimum>#<BYTE,Maximum>#
NV_FM_LNA_CTL_I,190,ReadWrite,<BYTE,Minimum>#<BYTE,Maximum>#
NV_HW_CONFIG_I,198,ReadWrite,<DWORD,Hardware configuration>#
NV_CDMA_RX_LIN_VS_TEMP_I,199,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#
NV_CDMA_ADJ_FACTOR_I,200,ReadWrite,<BYTE,CDMA adjustment factor>#
NV_CDMA_RX_SLP_VS_TEMP_I,202,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#
NV_CDMA_TX_SLP_VS_TEMP_I,203,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#
NV_PA_RANGE_VS_TEMP_I,204,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#
NV_FM_EXP_HDET_VS_TEMP_I,206,ReadWrite,<BYTE,Array[0]>#<BYTE,Array[1]>#<BYTE,Array[2]>#<BYTE,Array[3]>#<BYTE,Array[4]>#<BYTE,Array[5]>#<BYTE,Array[6]>#<BYTE,Array[7]>#
NV_LCD_I,72,ReadWrite,<BYTE,Handset brightness>#
NV_RX_AGC_MINMAX_I,247,ReadWrite,<BYTE,Minimum>#<BYTE,Maximum>#
NV_FR_TEMP_OFFSET_I,92,ReadWrite,<BYTE,Array[0]>#<BYTE,Array[1]>#<BYTE,Array[2]>#<BYTE,Array[3]>#<BYTE,Array[4]>#<BYTE,Array[5]>#<BYTE,Array[6]>#<BYTE,Array[7]>#<BYTE,Array[8]>#<BYTE,Array[9]>#<BYTE,Array[10]>#<BYTE,Array[11]>#<BYTE,Array[12]>#<BYTE,Array[13]>#<BYTE,Array[14]>#<BYTE,Array[15]>#<BYTE,Array[16]>#<BYTE,Array[17]>#<BYTE,Array[18]>#<BYTE,Array[19]>#<BYTE,Array[20]>#<BYTE,Array[21]>#<BYTE,Array[22]>#<BYTE,Array[23]>#<BYTE,Array[24]>#<BYTE,Array[25]>#<BYTE,Array[26]>#<BYTE,Array[27]>#<BYTE,Array[28]>#<BYTE,Array[29]>#<BYTE,Array[30]>#<BYTE,Array[31]>#<BYTE,Array[32]>#<BYTE,Array[33]>#<BYTE,Array[34]>#<BYTE,Array[35]>#<BYTE,Array[36]>#<BYTE,Array[37]>#<BYTE,Array[38]>#<BYTE,Array[39]>#<BYTE,Array[40]>#<BYTE,Array[41]>#<BYTE,Array[42]>#<BYTE,Array[43]>#<BYTE,Array[44]>#<BYTE,Array[45]>#<BYTE,Array[46]>#<BYTE,Array[47]>#<BYTE,Array[48]>#<BYTE,Array[49]>#<BYTE,Array[50]>#<BYTE,Array[51]>#<BYTE,Array[52]>#<BYTE,Array[53]>#<BYTE,Array[54]>#<BYTE,Array[55]>#<BYTE,Array[56]>#<BYTE,Array[57]>#<BYTE,Array[58]>#<BYTE,Array[59]>#<BYTE,Array[60]>#<BYTE,Array[61]>#<BYTE,Array[62]>#<BYTE,Array[63]>#
NV_FM_HDET_ADC_RANGE_I,311,ReadWrite,<BYTE,Array[1]>#<BYTE,Array[2]>#<BYTE,Array[3]>#<BYTE,Array[4]>#<BYTE,Array[5]>#<BYTE,Array[6]>#
NV_CDMA_HDET_ADC_RANGE_I,312,ReadWrite,<BYTE,CDMA HDET range VS amc>#
NV_PCS_RX_LIN_OFF_0_I,325,ReadWrite,<BYTE,PCS RX linearizer offset>#
NV_PCS_RX_LIN_SLP_I,326,ReadWrite,<BYTE,Array[0]>#<BYTE,Array[1]>#<BYTE,Array[2]>#<BYTE,Array[3]>#<BYTE,Array[4]>#<BYTE,Array[5]>#<BYTE,Array[6]>#<BYTE,Array[7]>#<BYTE,Array[8]>#<BYTE,Array[9]>#<BYTE,Array[10]>#<BYTE,Array[11]>#<BYTE,Array[12]>#<BYTE,Array[13]>#<BYTE,Array[14]>#<BYTE,Array[15]>#
NV_PCS_RX_COMP_VS_FREQ_I,327,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_PCS_TX_COMP_VS_FREQ_I,328,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_PCS_TX_LIN_MASTER_OFF_0_I,329,ReadWrite,<WORD,PCS TX linearizer master offset>#
NV_PCS_TX_LIN_MASTER_SLP_I,330,ReadWrite,<BYTE,Array[0]>#<BYTE,Array[1]>#<BYTE,Array[2]>#<BYTE,Array[3]>#<BYTE,Array[4]>#<BYTE,Array[5]>#<BYTE,Array[6]>#<BYTE,Array[7]>#<BYTE,Array[8]>#<BYTE,Array[9]>#<BYTE,Array[10]>#<BYTE,Array[11]>#<BYTE,Array[12]>#<BYTE,Array[13]>#<BYTE,Array[14]>#<BYTE,Array[15]>#<BYTE,Array[16]>#<BYTE,Array[17]>#<BYTE,Array[18]>#<BYTE,Array[19]>#<BYTE,Array[20]>#<BYTE,Array[21]>#<BYTE,Array[22]>#<BYTE,Array[23]>#<BYTE,Array[24]>#<BYTE,Array[25]>#<BYTE,Array[26]>#<BYTE,Array[27]>#<BYTE,Array[28]>#<BYTE,Array[29]>#<BYTE,Array[30]>#<BYTE,Array[31]>#
NV_PCS_TX_LIN_VS_TEMP_I,331,ReadWrite,<BYTE,Array[0]>#<BYTE,Array[1]>#<BYTE,Array[2]>#<BYTE,Array[3]>#<BYTE,Array[4]>#<BYTE,Array[5]>#<BYTE,Array[6]>#<BYTE,Array[7]>#
NV_PCS_TX_LIM_VS_TEMP_I,332,ReadWrite,<BYTE,Array[1]>#<BYTE,Array[1]>#<BYTE,Array[2]>#<BYTE,Array[3]>#<BYTE,Array[4]>#<BYTE,Array[5]>#<BYTE,Array[6]>#<BYTE,Array[7]>#
NV_PCS_TX_LIM_VS_FREQ_I,333,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_PCS_EXP_HDET_VS_AGC_I,334,ReadWrite,<BYTE,Array[0]>#<BYTE,Array[1]>#<BYTE,Array[2]>#<BYTE,Array[3]>#<BYTE,Array[4]>#<BYTE,Array[5]>#<BYTE,Array[6]>#<BYTE,Array[7]>#<BYTE,Array[8]>#<BYTE,Array[9]>#<BYTE,Array[10]>#<BYTE,Array[11]>#<BYTE,Array[12]>#<BYTE,Array[13]>#<BYTE,Array[14]>#<BYTE,Array[15]>#
NV_PCS_HDET_OFF_I,335,ReadWrite,<BYTE,PCS ADC HDET reading offset>#
NV_PCS_HDET_SPN_I,336,ReadWrite,<BYTE,PCS ADC HDET reading span>#
NV_PCS_R1_RISE_I,337,ReadWrite,<BYTE,PCS R1 rise>#
NV_PCS_R1_FALL_I,338,ReadWrite,<BYTE,PCS R1 fall>#
NV_PCS_R2_RISE_I,339,ReadWrite,<BYTE,PCS R2 rise>#
NV_PCS_R2_FALL_I,340,ReadWrite,<BYTE,PCS R2 fall>#
NV_PCS_R3_RISE_I,341,ReadWrite,<BYTE,PCS R3 rise>#
NV_PCS_R3_FALL_I,342,ReadWrite,<BYTE,PCS R3 fall>#
NV_PCS_PA_RANGE_STEP_CAL_I,343,ReadWrite,<BYTE,PCS PA range step calibraion>#
NV_PCS_PDM1_VS_FREQ_I,344,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_PCS_PDM2_VS_FREQ_I,345,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_PCS_LNA_RANGE_POL_I,346,ReadWrite,<BYTE,PCS LNA range polarity>#
NV_PCS_LNA_RANGE_RISE_I,347,ReadWrite,<SIGNED_BYTE,PCS LNA range rise>#
NV_PCS_LNA_RANGE_FALL_I,348,ReadWrite,<SIGNED_BYTE,PCS LNA range fall>#
NV_PCS_LNA_RANGE_OFFSET_I,349,ReadWrite,<WORD,PCS LNA range offset>#
NV_PCS_RX_LIN_VS_TEMP_I,350,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#
NV_PCS_ADJ_FACTOR_I,351,ReadWrite,<BYTE,PCS adjustment factor>#
NV_PCS_PA_RANGE_VS_TEMP_I,352,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#
NV_PCS_PDM1_VS_TEMP_I,353,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#
NV_PCS_PDM2_VS_TEMP_I,354,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#
NV_PCS_RX_SLP_VS_TEMP_I,355,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#
NV_PCS_TX_SLP_VS_TEMP_I,356,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#
NV_PCS_RX_AGC_MINMAX_I,357,ReadWrite,<BYTE,Minimum>#<BYTE,Maximum>#
NV_VEXT_I,360,ReadWrite,<BYTE,Minimum>#<BYTE,Maximum>#
NV_VLCD_ADC_CNT_I,361,ReadWrite,<BYTE,VLCD ADC CNT>#
NV_VLCD_DRVR_CNT_I,362,ReadWrite,<BYTE,VLCD_DRVR_CNT>#
NV_VREF_ADJ_PDM_CNT_I,363,ReadWrite,<BYTE,VREF_ADJ_PDM_CNT>#
NV_IBAT_PER_LSB_I,364,ReadWrite,<BYTE,Minimum>#<BYTE,Maximum>#
NV_IEXT_I,365,ReadWrite,<BYTE,Minimum>#<BYTE,Maximum>#
NV_IEXT_THR_I,366,ReadWrite,<BYTE,IEXT_THR>#
NV_LNA_RANGE_2_RISE_I,376,ReadWrite,<SIGNED_BYTE,Receive power level to bypass the second LNA>#
NV_LNA_RANGE_2_FALL_I,377,ReadWrite,<SIGNED_BYTE,Receive power level to turn on the second LNA>#
NV_LNA_RANGE_12_OFFSET_I,378,ReadWrite,<SIGNED_WORD,Offset added to Receive power when the first ande second LNAs are bypassed>#
NV_NONBYPASS_TIMER_I,379,ReadWrite,<BYTE,Duration of non-bypass state in multiples of 52us(3-bits)>#
NV_BYPASS_TIMER_I,380,ReadWrite,<BYTE,Duration of bypass state in multiples of 6.6us>#
NV_IM_LEVEL1_I,381,ReadWrite,<BYTE,LNA1 InterMod antijamming threshold power level>#
NV_IM_LEVEL2_I,382,ReadWrite,<BYTE,LNA2 InterMod antijamming threshold power level>#
NV_CDMA_LNA_OFFSET_VS_FREQ_I,383,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_CDMA_LNA_12_OFFSET_VS_FREQ_I,384,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_AGC_PHASE_OFFSET_I,385,ReadWrite,<BYTE,Phase rotation setting for LNA_DECISION 01 and 11>#
NV_RX_AGC_MIN_11_I,386,ReadWrite,<BYTE,Minimum>#<BYTE,Maximum>#
NV_CDMA_TX_LIN_MASTER0_I,367,ReadWrite,<SIGNED_WORD,Offset>#<BYTE,Slope[0]>#<BYTE,Slope[1]>#<BYTE,Slope[2]>#<BYTE,Slope[3]>#<BYTE,Slope[4]>#<BYTE,Slope[5]>#<BYTE,Slope[6]>#<BYTE,Slope[7]>#<BYTE,Slope[8]>#<BYTE,Slope[9]>#<BYTE,Slope[10]>#<BYTE,Slope[11]>#<BYTE,Slope[12]>#<BYTE,Slope[13]>#<BYTE,Slope[14]>#<BYTE,Slope[15]>#<BYTE,Slope[16]>#<BYTE,Slope[17]>#<BYTE,Slope[18]>#<BYTE,Slope[19]>#<BYTE,Slope[20]>#<BYTE,Slope[21]>#<BYTE,Slope[22]>#<BYTE,Slope[23]>#<BYTE,Slope[24]>#<BYTE,Slope[25]>#<BYTE,Slope[26]>#<BYTE,Slope[27]>#<BYTE,Slope[28]>#<BYTE,Slope[29]>#<BYTE,Slope[30]>#<BYTE,Slope[31]>#<BYTE,Slope[32]>#<BYTE,Slope[33]>#<BYTE,Slope[34]>#<BYTE,Slope[35]>#
NV_CDMA_TX_LIN_MASTER1_I,368,ReadWrite,<SIGNED_WORD,Offset>#<BYTE,Slope[0]>#<BYTE,Slope[1]>#<BYTE,Slope[2]>#<BYTE,Slope[3]>#<BYTE,Slope[4]>#<BYTE,Slope[5]>#<BYTE,Slope[6]>#<BYTE,Slope[7]>#<BYTE,Slope[8]>#<BYTE,Slope[9]>#<BYTE,Slope[10]>#<BYTE,Slope[11]>#<BYTE,Slope[12]>#<BYTE,Slope[13]>#<BYTE,Slope[14]>#<BYTE,Slope[15]>#<BYTE,Slope[16]>#<BYTE,Slope[17]>#<BYTE,Slope[18]>#<BYTE,Slope[19]>#<BYTE,Slope[20]>#<BYTE,Slope[21]>#<BYTE,Slope[22]>#<BYTE,Slope[23]>#<BYTE,Slope[24]>#<BYTE,Slope[25]>#<BYTE,Slope[26]>#<BYTE,Slope[27]>#<BYTE,Slope[28]>#<BYTE,Slope[29]>#<BYTE,Slope[30]>#<BYTE,Slope[31]>#<BYTE,Slope[32]>#<BYTE,Slope[33]>#<BYTE,Slope[34]>#<BYTE,Slope[35]>#
NV_CDMA_TX_LIN_MASTER2_I,369,ReadWrite,<SIGNED_WORD,Offset>#<BYTE,Slope[0]>#<BYTE,Slope[1]>#<BYTE,Slope[2]>#<BYTE,Slope[3]>#<BYTE,Slope[4]>#<BYTE,Slope[5]>#<BYTE,Slope[6]>#<BYTE,Slope[7]>#<BYTE,Slope[8]>#<BYTE,Slope[9]>#<BYTE,Slope[10]>#<BYTE,Slope[11]>#<BYTE,Slope[12]>#<BYTE,Slope[13]>#<BYTE,Slope[14]>#<BYTE,Slope[15]>#<BYTE,Slope[16]>#<BYTE,Slope[17]>#<BYTE,Slope[18]>#<BYTE,Slope[19]>#<BYTE,Slope[20]>#<BYTE,Slope[21]>#<BYTE,Slope[22]>#<BYTE,Slope[23]>#<BYTE,Slope[24]>#<BYTE,Slope[25]>#<BYTE,Slope[26]>#<BYTE,Slope[27]>#<BYTE,Slope[28]>#<BYTE,Slope[29]>#<BYTE,Slope[30]>#<BYTE,Slope[31]>#<BYTE,Slope[32]>#<BYTE,Slope[33]>#<BYTE,Slope[34]>#<BYTE,Slope[35]>#
NV_CDMA_TX_LIN_MASTER3_I,370,ReadWrite,<SIGNED_WORD,Offset>#<BYTE,Slope[0]>#<BYTE,Slope[1]>#<BYTE,Slope[2]>#<BYTE,Slope[3]>#<BYTE,Slope[4]>#<BYTE,Slope[5]>#<BYTE,Slope[6]>#<BYTE,Slope[7]>#<BYTE,Slope[8]>#<BYTE,Slope[9]>#<BYTE,Slope[10]>#<BYTE,Slope[11]>#<BYTE,Slope[12]>#<BYTE,Slope[13]>#<BYTE,Slope[14]>#<BYTE,Slope[15]>#<BYTE,Slope[16]>#<BYTE,Slope[17]>#<BYTE,Slope[18]>#<BYTE,Slope[19]>#<BYTE,Slope[20]>#<BYTE,Slope[21]>#<BYTE,Slope[22]>#<BYTE,Slope[23]>#<BYTE,Slope[24]>#<BYTE,Slope[25]>#<BYTE,Slope[26]>#<BYTE,Slope[27]>#<BYTE,Slope[28]>#<BYTE,Slope[29]>#<BYTE,Slope[30]>#<BYTE,Slope[31]>#<BYTE,Slope[32]>#<BYTE,Slope[33]>#<BYTE,Slope[34]>#<BYTE,Slope[35]>#
NV_PA_RANGE_OFFSETS_I,410,ReadWrite,<SIGNED_WORD,PA range offset[0]>#<SIGNED_WORD,PA range offset[1]>#<SIGNED_WORD,PA range offset[2]>#<SIGNED_WORD,PA range offset[3]>#
NV_TX_COMP0_I,411,ReadWrite,<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[0]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[1]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[2]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[3]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[4]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[5]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[6]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[8]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[9]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[10]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[11]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[12]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[13]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[14]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[15]>#
NV_TX_COMP1_I,420,ReadWrite,<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[0]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[1]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[2]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[3]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[4]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[5]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[6]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[8]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[9]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[10]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[11]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[12]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[13]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[14]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[15]>#
NV_TX_COMP2_I,421,ReadWrite,<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[0]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[1]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[2]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[3]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[4]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[5]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[6]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[8]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[9]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[10]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[11]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[12]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[13]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[14]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[15]>#
NV_TX_COMP3_I,422,ReadWrite,<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[0]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[1]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[2]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[3]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[4]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[5]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[6]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[8]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[9]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[10]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[11]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[12]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[13]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[14]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[15]>#
NV_PCS_LNA_RANGE_2_RISE_I,387,ReadWrite,<SIGNED_BYTE,Receive power level to bypass the second LNA>#
NV_PCS_LNA_RANGE_2_FALL_I,388,ReadWrite,<SIGNED_BYTE,Receive power level to turn on the second LNA>#
NV_PCS_LNA_RANGE_12_OFFSET_I,389,ReadWrite,<SIGNED_WORD,Offset added to receive power when the first and second LNAs are bypassed>#
NV_PCS_NONBYPASS_TIMER_I,390,ReadWrite,<BYTE,Duration of nonbypass state in multiples of 52us>#
NV_PCS_BYPASS_TIMER_I,391,ReadWrite,<BYTE,Duration of bypass state in multiples of 6.6us>#
NV_PCS_IM_LEVEL1_I,392,ReadWrite,<BYTE,LNA1 InterMod antijamming threshold power level>#
NV_PCS_IM_LEVEL2_I,393,ReadWrite,<BYTE,LNA2 InterMod antijamming threshold power level>#
NV_PCS_CDMA_LNA_OFFSET_VS_FREQ_I,394,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_PCS_CDMA_LNA_12_OFFSET_VS_FREQ_I,395,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_PCS_AGC_PHASE_OFFSET_I,396,ReadWrite,<BYTE,Phase rotation setting for LNA_DECISION 01 and 11>#
NV_PCS_RX_AGC_MIN_11_I,397,ReadWrite,<BYTE,Minimum>#<BYTE,Maximum>#
NV_PCS_TX_LIN_MASTER0_I,431,ReadWrite,<SIGNED_WORD,Offset>#<BYTE,Slope[0]>#<BYTE,Slope[1]>#<BYTE,Slope[2]>#<BYTE,Slope[3]>#<BYTE,Slope[4]>#<BYTE,Slope[5]>#<BYTE,Slope[6]>#<BYTE,Slope[7]>#<BYTE,Slope[8]>#<BYTE,Slope[9]>#<BYTE,Slope[10]>#<BYTE,Slope[11]>#<BYTE,Slope[12]>#<BYTE,Slope[13]>#<BYTE,Slope[14]>#<BYTE,Slope[15]>#<BYTE,Slope[16]>#<BYTE,Slope[17]>#<BYTE,Slope[18]>#<BYTE,Slope[19]>#<BYTE,Slope[20]>#<BYTE,Slope[21]>#<BYTE,Slope[22]>#<BYTE,Slope[23]>#<BYTE,Slope[24]>#<BYTE,Slope[25]>#<BYTE,Slope[26]>#<BYTE,Slope[27]>#<BYTE,Slope[28]>#<BYTE,Slope[29]>#<BYTE,Slope[30]>#<BYTE,Slope[31]>#<BYTE,Slope[32]>#<BYTE,Slope[33]>#<BYTE,Slope[34]>#<BYTE,Slope[35]>#
NV_PCS_TX_LIN_MASTER1_I,432,ReadWrite,<SIGNED_WORD,Offset>#<BYTE,Slope[0]>#<BYTE,Slope[1]>#<BYTE,Slope[2]>#<BYTE,Slope[3]>#<BYTE,Slope[4]>#<BYTE,Slope[5]>#<BYTE,Slope[6]>#<BYTE,Slope[7]>#<BYTE,Slope[8]>#<BYTE,Slope[9]>#<BYTE,Slope[10]>#<BYTE,Slope[11]>#<BYTE,Slope[12]>#<BYTE,Slope[13]>#<BYTE,Slope[14]>#<BYTE,Slope[15]>#<BYTE,Slope[16]>#<BYTE,Slope[17]>#<BYTE,Slope[18]>#<BYTE,Slope[19]>#<BYTE,Slope[20]>#<BYTE,Slope[21]>#<BYTE,Slope[22]>#<BYTE,Slope[23]>#<BYTE,Slope[24]>#<BYTE,Slope[25]>#<BYTE,Slope[26]>#<BYTE,Slope[27]>#<BYTE,Slope[28]>#<BYTE,Slope[29]>#<BYTE,Slope[30]>#<BYTE,Slope[31]>#<BYTE,Slope[32]>#<BYTE,Slope[33]>#<BYTE,Slope[34]>#<BYTE,Slope[35]>#
NV_PCS_TX_LIN_MASTER2_I,433,ReadWrite,<SIGNED_WORD,Offset>#<BYTE,Slope[0]>#<BYTE,Slope[1]>#<BYTE,Slope[2]>#<BYTE,Slope[3]>#<BYTE,Slope[4]>#<BYTE,Slope[5]>#<BYTE,Slope[6]>#<BYTE,Slope[7]>#<BYTE,Slope[8]>#<BYTE,Slope[9]>#<BYTE,Slope[10]>#<BYTE,Slope[11]>#<BYTE,Slope[12]>#<BYTE,Slope[13]>#<BYTE,Slope[14]>#<BYTE,Slope[15]>#<BYTE,Slope[16]>#<BYTE,Slope[17]>#<BYTE,Slope[18]>#<BYTE,Slope[19]>#<BYTE,Slope[20]>#<BYTE,Slope[21]>#<BYTE,Slope[22]>#<BYTE,Slope[23]>#<BYTE,Slope[24]>#<BYTE,Slope[25]>#<BYTE,Slope[26]>#<BYTE,Slope[27]>#<BYTE,Slope[28]>#<BYTE,Slope[29]>#<BYTE,Slope[30]>#<BYTE,Slope[31]>#<BYTE,Slope[32]>#<BYTE,Slope[33]>#<BYTE,Slope[34]>#<BYTE,Slope[35]>#
NV_PCS_TX_LIN_MASTER3_I,434,ReadWrite,<SIGNED_WORD,Offset>#<BYTE,Slope[0]>#<BYTE,Slope[1]>#<BYTE,Slope[2]>#<BYTE,Slope[3]>#<BYTE,Slope[4]>#<BYTE,Slope[5]>#<BYTE,Slope[6]>#<BYTE,Slope[7]>#<BYTE,Slope[8]>#<BYTE,Slope[9]>#<BYTE,Slope[10]>#<BYTE,Slope[11]>#<BYTE,Slope[12]>#<BYTE,Slope[13]>#<BYTE,Slope[14]>#<BYTE,Slope[15]>#<BYTE,Slope[16]>#<BYTE,Slope[17]>#<BYTE,Slope[18]>#<BYTE,Slope[19]>#<BYTE,Slope[20]>#<BYTE,Slope[21]>#<BYTE,Slope[22]>#<BYTE,Slope[23]>#<BYTE,Slope[24]>#<BYTE,Slope[25]>#<BYTE,Slope[26]>#<BYTE,Slope[27]>#<BYTE,Slope[28]>#<BYTE,Slope[29]>#<BYTE,Slope[30]>#<BYTE,Slope[31]>#<BYTE,Slope[32]>#<BYTE,Slope[33]>#<BYTE,Slope[34]>#<BYTE,Slope[35]>#
NV_PCS_PA_RANGE_OFFSETS_I,435,ReadWrite,<SIGNED_WORD,Array[0]>#<SIGNED_WORD,Array[1]>#<SIGNED_WORD,Array[2]>#<SIGNED_WORD,Array[3]>#
NV_PCS_TX_COMP0_I,436,ReadWrite,<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[0]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[1]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[2]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[3]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[4]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[5]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[6]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[8]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[9]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[10]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[11]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[12]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[13]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[14]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[15]>#
NV_PCS_TX_COMP1_I,437,ReadWrite,<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[0]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[1]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[2]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[3]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[4]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[5]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[6]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[8]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[9]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[10]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[11]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[12]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[13]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[14]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[15]>#
NV_PCS_TX_COMP2_I,438,ReadWrite,<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[0]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[1]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[2]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[3]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[4]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[5]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[6]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[8]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[9]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[10]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[11]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[12]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[13]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[14]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[15]>#
NV_PCS_TX_COMP3_I,439,ReadWrite,<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[0]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[1]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[2]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[3]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[4]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[5]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[6]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[8]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[9]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[10]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[11]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[12]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[13]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[14]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[15]>#
NV_GPS1_GPS_RF_DELAY_I,443,ReadWrite,<WORD,GPS RF delay>#
NV_GPS1_CDMA_RF_DELAY_I,444,ReadWrite,<WORD,CDMA RF delay>#
NV_PCS_ENC_BTF_I,445,ReadWrite,<DWORD,PCS ENC BTF>#
NV_CDMA_ENC_BTF_I,446,ReadWrite,<DWORD,CDMA ENC BTF>#
NV_SUBPCG_PA_WARMUP_DELAY_I,448,ReadWrite,<WORD,SUBPCG PA warm up delay>#
NV_GPS1_GPS_RF_LOSS_I,449,ReadWrite,<BYTE,GPS RF loss>#
NV_WCDMA_RX_LIN_I,514,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#
NV_WCDMA_RX_COMP_VS_FREQ_I,515,ReadWrite,<SIGNED_BYTE,Aarray[0]>#<SIGNED_BYTE,Aarray[1]>#<SIGNED_BYTE,Aarray[2]>#<SIGNED_BYTE,Aarray[3]>#<SIGNED_BYTE,Aarray[4]>#<SIGNED_BYTE,Aarray[5]>#<SIGNED_BYTE,Aarray[6]>#<SIGNED_BYTE,Aarray[7]>#<SIGNED_BYTE,Aarray[8]>#<SIGNED_BYTE,Aarray[9]>#<SIGNED_BYTE,Aarray[10]>#<SIGNED_BYTE,Aarray[11]>#<SIGNED_BYTE,Aarray[12]>#<SIGNED_BYTE,Aarray[13]>#<SIGNED_BYTE,Aarray[14]>#<SIGNED_BYTE,Aarray[15]>#
NV_WCDMA_RX_LIN_VS_TEMP_I,516,ReadWrite,<SIGNED_BYTE,Aarray[0]>#<SIGNED_BYTE,Aarray[1]>#<SIGNED_BYTE,Aarray[2]>#<SIGNED_BYTE,Aarray[3]>#<SIGNED_BYTE,Aarray[4]>#<SIGNED_BYTE,Aarray[5]>#<SIGNED_BYTE,Aarray[6]>#<SIGNED_BYTE,Aarray[7]>#
NV_WCDMA_RX_SLP_VS_TEMP_I,517,ReadWrite,<SIGNED_BYTE,Aarray[0]>#<SIGNED_BYTE,Aarray[1]>#<SIGNED_BYTE,Aarray[2]>#<SIGNED_BYTE,Aarray[3]>#<SIGNED_BYTE,Aarray[4]>#<SIGNED_BYTE,Aarray[5]>#<SIGNED_BYTE,Aarray[6]>#<SIGNED_BYTE,Aarray[7]>#
NV_WCDMA_LNA_RANGE_POL_I,518,ReadWrite,<BYTE,LNA range pol>#
NV_WCDMA_LNA_RANGE_RISE_I,519,ReadWrite,<SIGNED_WORD,LNA range rise>#
NV_WCDMA_LNA_RANGE_FALL_I,520,ReadWrite,<SIGNED_WORD,LNA range fall>#
NV_WCDMA_IM_LEVEL_I,521,ReadWrite,<SIGNED_WORD,IM level>#
NV_WCDMA_NONBYPASS_TIMER_I,522,ReadWrite,<BYTE,Non-bypass timer>#
NV_WCDMA_BYPASS_TIMER_I,523,ReadWrite,<WORD,Bypass timer>#
NV_WCDMA_LNA_RANGE_OFFSET_I,524,ReadWrite,<SIGNED_WORD,LNA range offset>#
NV_WCDMA_LNA_OFFSET_VS_FREQ_I,525,ReadWrite,<SIGNED_BYTE,Aarray[0]>#<SIGNED_BYTE,Aarray[1]>#<SIGNED_BYTE,Aarray[2]>#<SIGNED_BYTE,Aarray[3]>#<SIGNED_BYTE,Aarray[4]>#<SIGNED_BYTE,Aarray[5]>#<SIGNED_BYTE,Aarray[6]>#<SIGNED_BYTE,Aarray[7]>#<SIGNED_BYTE,Aarray[8]>#<SIGNED_BYTE,Aarray[9]>#<SIGNED_BYTE,Aarray[10]>#<SIGNED_BYTE,Aarray[11]>#<SIGNED_BYTE,Aarray[12]>#<SIGNED_BYTE,Aarray[13]>#<SIGNED_BYTE,Aarray[14]>#<SIGNED_BYTE,Aarray[15]>#
NV_WCDMA_RX_AGC_MIN_I,526,ReadWrite,<SIGNED_WORD,RX agc min>#
NV_WCDMA_RX_AGC_MAX_I,527,ReadWrite,<SIGNED_WORD,RX agc max>#
NV_WCDMA_AGC_PHASE_OFFSET_I,528,ReadWrite,<BYTE,Agc phase offset>#
NV_WCDMA_TX_LIN_MASTER_0_I,529,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#<WORD,Array[30]>#<WORD,Array[31]>#<WORD,Array[32]>#<WORD,Array[33]>#<WORD,Array[34]>#<WORD,Array[35]>#
NV_WCDMA_TX_LIN_MASTER_1_I,530,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#<WORD,Array[30]>#<WORD,Array[31]>#<WORD,Array[32]>#<WORD,Array[33]>#<WORD,Array[34]>#<WORD,Array[35]>#
NV_WCDMA_TX_COMP_VS_FREQ_0_I,531,ReadWrite,<SIGNED_BYTE,Aarray[0]>#<SIGNED_BYTE,Aarray[1]>#<SIGNED_BYTE,Aarray[2]>#<SIGNED_BYTE,Aarray[3]>#<SIGNED_BYTE,Aarray[4]>#<SIGNED_BYTE,Aarray[5]>#<SIGNED_BYTE,Aarray[6]>#<SIGNED_BYTE,Aarray[7]>#<SIGNED_BYTE,Aarray[8]>#<SIGNED_BYTE,Aarray[9]>#<SIGNED_BYTE,Aarray[10]>#<SIGNED_BYTE,Aarray[11]>#<SIGNED_BYTE,Aarray[12]>#<SIGNED_BYTE,Aarray[13]>#<SIGNED_BYTE,Aarray[14]>#<SIGNED_BYTE,Aarray[15]>#
NV_WCDMA_TX_COMP_VS_FREQ_1_I,532,ReadWrite,<SIGNED_BYTE,Aarray[0]>#<SIGNED_BYTE,Aarray[1]>#<SIGNED_BYTE,Aarray[2]>#<SIGNED_BYTE,Aarray[3]>#<SIGNED_BYTE,Aarray[4]>#<SIGNED_BYTE,Aarray[5]>#<SIGNED_BYTE,Aarray[6]>#<SIGNED_BYTE,Aarray[7]>#<SIGNED_BYTE,Aarray[8]>#<SIGNED_BYTE,Aarray[9]>#<SIGNED_BYTE,Aarray[10]>#<SIGNED_BYTE,Aarray[11]>#<SIGNED_BYTE,Aarray[12]>#<SIGNED_BYTE,Aarray[13]>#<SIGNED_BYTE,Aarray[14]>#<SIGNED_BYTE,Aarray[15]>#
NV_WCDMA_TX_LIN_VS_TEMP_0_I,533,ReadWrite,<SIGNED_BYTE,Aarray[0]>#<SIGNED_BYTE,Aarray[1]>#<SIGNED_BYTE,Aarray[2]>#<SIGNED_BYTE,Aarray[3]>#<SIGNED_BYTE,Aarray[4]>#<SIGNED_BYTE,Aarray[5]>#<SIGNED_BYTE,Aarray[6]>#<SIGNED_BYTE,Aarray[7]>#
NV_WCDMA_TX_LIN_VS_TEMP_1_I,534,ReadWrite,<SIGNED_BYTE,Aarray[0]>#<SIGNED_BYTE,Aarray[1]>#<SIGNED_BYTE,Aarray[2]>#<SIGNED_BYTE,Aarray[3]>#<SIGNED_BYTE,Aarray[4]>#<SIGNED_BYTE,Aarray[5]>#<SIGNED_BYTE,Aarray[6]>#<SIGNED_BYTE,Aarray[7]>#
NV_WCDMA_TX_SLP_VS_TEMP_0_I,535,ReadWrite,<SIGNED_BYTE,Aarray[0]>#<SIGNED_BYTE,Aarray[1]>#<SIGNED_BYTE,Aarray[2]>#<SIGNED_BYTE,Aarray[3]>#<SIGNED_BYTE,Aarray[4]>#<SIGNED_BYTE,Aarray[5]>#<SIGNED_BYTE,Aarray[6]>#<SIGNED_BYTE,Aarray[7]>#
NV_WCDMA_TX_SLP_VS_TEMP_1_I,536,ReadWrite,<SIGNED_BYTE,Aarray[0]>#<SIGNED_BYTE,Aarray[1]>#<SIGNED_BYTE,Aarray[2]>#<SIGNED_BYTE,Aarray[3]>#<SIGNED_BYTE,Aarray[4]>#<SIGNED_BYTE,Aarray[5]>#<SIGNED_BYTE,Aarray[6]>#<SIGNED_BYTE,Aarray[7]>#
NV_WCDMA_R1_RISE_I,537,ReadWrite,<WORD,R1 rise>#
NV_WCDMA_R1_FALL_I,538,ReadWrite,<WORD,R1 fall>#
NV_WCDMA_TX_LIM_VS_TEMP_I,539,ReadWrite,<BYTE,Aarray[0]>#<BYTE,Aarray[1]>#<BYTE,Aarray[2]>#<BYTE,Aarray[3]>#<BYTE,Aarray[4]>#<BYTE,Aarray[5]>#<BYTE,Aarray[6]>#<BYTE,Aarray[7]>#
NV_WCDMA_TX_LIM_VS_FREQ_I,540,ReadWrite,<SIGNED_WORD,Array[0]>#<SIGNED_WORD,Array[1]>#<SIGNED_WORD,Array[2]>#<SIGNED_WORD,Array[3]>#<SIGNED_WORD,Array[4]>#<SIGNED_WORD,Array[5]>#<SIGNED_WORD,Array[6]>#<SIGNED_WORD,Array[7]>#<SIGNED_WORD,Array[8]>#<SIGNED_WORD,Array[9]>#<SIGNED_WORD,Array[10]>#<SIGNED_WORD,Array[11]>#<SIGNED_WORD,Array[12]>#<SIGNED_WORD,Array[13]>#<SIGNED_WORD,Array[14]>#<SIGNED_WORD,Array[15]>#
NV_WCDMA_ADJ_FACTOR_I,541,ReadWrite,<BYTE,ADJ factor>#
NV_WCDMA_EXP_HDET_VS_AGC_I,542,ReadWrite,<BYTE,Aarray[0]>#<BYTE,Aarray[1]>#<BYTE,Aarray[2]>#<BYTE,Aarray[3]>#<BYTE,Aarray[4]>#<BYTE,Aarray[5]>#<BYTE,Aarray[6]>#<BYTE,Aarray[7]>#<BYTE,Aarray[8]>#<BYTE,Aarray[9]>#<BYTE,Aarray[10]>#<BYTE,Aarray[11]>#<BYTE,Aarray[12]>#<BYTE,Aarray[13]>#<BYTE,Aarray[14]>#<BYTE,Aarray[15]>#
NV_WCDMA_HDET_OFF_I,543,ReadWrite,<BYTE,HDET off>#
NV_WCDMA_HDET_SPN_I,544,ReadWrite,<BYTE,HDET spn>#
NV_WCDMA_ENC_BTF_I,545,ReadWrite,<DWORD,ENC BTF>#
NV_ANT2_CDMA_RX_LIN_OFF_0_I,496,ReadWrite,<BYTE,ANT2_CDMA_RX_LIN_OFF>#
NV_ANT2_CDMA_RX_LIN_SLP_I,497,ReadWrite,<BYTE,Aarray[0]>#<BYTE,Aarray[1]>#<BYTE,Aarray[2]>#<BYTE,Aarray[3]>#<BYTE,Aarray[4]>#<BYTE,Aarray[5]>#<BYTE,Aarray[6]>#<BYTE,Aarray[7]>#<BYTE,Aarray[8]>#<BYTE,Aarray[9]>#<BYTE,Aarray[10]>#<BYTE,Aarray[11]>#<BYTE,Aarray[12]>#<BYTE,Aarray[13]>#<BYTE,Aarray[14]>#<BYTE,Aarray[15]>#
NV_ANT2_CDMA_RX_COMP_VS_FREQ_I,498,ReadWrite,<SIGNED_BYTE,Aarray[0]>#<SIGNED_BYTE,Aarray[1]>#<SIGNED_BYTE,Aarray[2]>#<SIGNED_BYTE,Aarray[3]>#<SIGNED_BYTE,Aarray[4]>#<SIGNED_BYTE,Aarray[5]>#<SIGNED_BYTE,Aarray[6]>#<SIGNED_BYTE,Aarray[7]>#<SIGNED_BYTE,Aarray[8]>#<SIGNED_BYTE,Aarray[9]>#<SIGNED_BYTE,Aarray[10]>#<SIGNED_BYTE,Aarray[11]>#<SIGNED_BYTE,Aarray[12]>#<SIGNED_BYTE,Aarray[13]>#<SIGNED_BYTE,Aarray[14]>#<SIGNED_BYTE,Aarray[15]>#
NV_ANT2_CDMA_RX_LIN_VS_TEMP_I,499,ReadWrite,<SIGNED_BYTE,Aarray[0]>#<SIGNED_BYTE,Aarray[1]>#<SIGNED_BYTE,Aarray[2]>#<SIGNED_BYTE,Aarray[3]>#<SIGNED_BYTE,Aarray[4]>#<SIGNED_BYTE,Aarray[5]>#<SIGNED_BYTE,Aarray[6]>#<SIGNED_BYTE,Aarray[7]>#
NV_ANT2_CDMA_RX_SLP_VS_TEMP_I,500,ReadWrite,<SIGNED_BYTE,Aarray[0]>#<SIGNED_BYTE,Aarray[1]>#<SIGNED_BYTE,Aarray[2]>#<SIGNED_BYTE,Aarray[3]>#<SIGNED_BYTE,Aarray[4]>#<SIGNED_BYTE,Aarray[5]>#<SIGNED_BYTE,Aarray[6]>#<SIGNED_BYTE,Aarray[7]>#
NV_ANT2_LNA_RANGE_OFFSET_I,501,ReadWrite,<WORD,LNA range offset>#
NV_ANT2_LNA_RANGE_12_OFFSET_I,502,ReadWrite,<SIGNED_WORD,LNA range 12 offset>#
NV_ANT2_CDMA_LNA_OFFSET_VS_FREQ_I,503,ReadWrite,<SIGNED_BYTE,Aarray[0]>#<SIGNED_BYTE,Aarray[1]>#<SIGNED_BYTE,Aarray[2]>#<SIGNED_BYTE,Aarray[3]>#<SIGNED_BYTE,Aarray[4]>#<SIGNED_BYTE,Aarray[5]>#<SIGNED_BYTE,Aarray[6]>#<SIGNED_BYTE,Aarray[7]>#<SIGNED_BYTE,Aarray[8]>#<SIGNED_BYTE,Aarray[9]>#<SIGNED_BYTE,Aarray[10]>#<SIGNED_BYTE,Aarray[11]>#<SIGNED_BYTE,Aarray[12]>#<SIGNED_BYTE,Aarray[13]>#<SIGNED_BYTE,Aarray[14]>#<SIGNED_BYTE,Aarray[15]>#
NV_ANT2_CDMA_LNA_12_OFFSET_VS_FREQ_I,504,ReadWrite,<SIGNED_BYTE,Aarray[0]>#<SIGNED_BYTE,Aarray[1]>#<SIGNED_BYTE,Aarray[2]>#<SIGNED_BYTE,Aarray[3]>#<SIGNED_BYTE,Aarray[4]>#<SIGNED_BYTE,Aarray[5]>#<SIGNED_BYTE,Aarray[6]>#<SIGNED_BYTE,Aarray[7]>#<SIGNED_BYTE,Aarray[8]>#<SIGNED_BYTE,Aarray[9]>#<SIGNED_BYTE,Aarray[10]>#<SIGNED_BYTE,Aarray[11]>#<SIGNED_BYTE,Aarray[12]>#<SIGNED_BYTE,Aarray[13]>#<SIGNED_BYTE,Aarray[14]>#<SIGNED_BYTE,Aarray[15]>#
NV_ANT2_PCS_RX_LIN_OFF_0_I,505,ReadWrite,<BYTE,PCS RX lin off>#
NV_ANT2_PCS_RX_LIN_SLP_I,506,ReadWrite,<BYTE,Aarray[0]>#<BYTE,Aarray[1]>#<BYTE,Aarray[2]>#<BYTE,Aarray[3]>#<BYTE,Aarray[4]>#<BYTE,Aarray[5]>#<BYTE,Aarray[6]>#<BYTE,Aarray[7]>#<BYTE,Aarray[8]>#<BYTE,Aarray[9]>#<BYTE,Aarray[10]>#<BYTE,Aarray[11]>#<BYTE,Aarray[12]>#<BYTE,Aarray[13]>#<BYTE,Aarray[14]>#<BYTE,Aarray[15]>#
NV_ANT2_PCS_RX_COMP_VS_FREQ_I,507,ReadWrite,<SIGNED_BYTE,Aarray[0]>#<SIGNED_BYTE,Aarray[1]>#<SIGNED_BYTE,Aarray[2]>#<SIGNED_BYTE,Aarray[3]>#<SIGNED_BYTE,Aarray[4]>#<SIGNED_BYTE,Aarray[5]>#<SIGNED_BYTE,Aarray[6]>#<SIGNED_BYTE,Aarray[7]>#<SIGNED_BYTE,Aarray[8]>#<SIGNED_BYTE,Aarray[9]>#<SIGNED_BYTE,Aarray[10]>#<SIGNED_BYTE,Aarray[11]>#<SIGNED_BYTE,Aarray[12]>#<SIGNED_BYTE,Aarray[13]>#<SIGNED_BYTE,Aarray[14]>#<SIGNED_BYTE,Aarray[15]>#
NV_ANT2_PCS_RX_LIN_VS_TEMP_I,508,ReadWrite,<SIGNED_BYTE,Aarray[0]>#<SIGNED_BYTE,Aarray[1]>#<SIGNED_BYTE,Aarray[2]>#<SIGNED_BYTE,Aarray[3]>#<SIGNED_BYTE,Aarray[4]>#<SIGNED_BYTE,Aarray[5]>#<SIGNED_BYTE,Aarray[6]>#<SIGNED_BYTE,Aarray[7]>#
NV_ANT2_PCS_RX_SLP_VS_TEMP_I,509,ReadWrite,<SIGNED_BYTE,Aarray[0]>#<SIGNED_BYTE,Aarray[1]>#<SIGNED_BYTE,Aarray[2]>#<SIGNED_BYTE,Aarray[3]>#<SIGNED_BYTE,Aarray[4]>#<SIGNED_BYTE,Aarray[5]>#<SIGNED_BYTE,Aarray[6]>#<SIGNED_BYTE,Aarray[7]>#
NV_ANT2_PCS_LNA_RANGE_OFFSET_I,510,ReadWrite,<WORD,PCS LNA range offset>#
NV_ANT2_PCS_LNA_RANGE_12_OFFSET_I,511,ReadWrite,<SIGNED_WORD,PCS LAN range 12 offset>#
NV_ANT2_PCS_CDMA_LNA_OFFSET_VS_FREQ_I,512,ReadWrite,<SIGNED_BYTE,Aarray[0]>#<SIGNED_BYTE,Aarray[1]>#<SIGNED_BYTE,Aarray[2]>#<SIGNED_BYTE,Aarray[3]>#<SIGNED_BYTE,Aarray[4]>#<SIGNED_BYTE,Aarray[5]>#<SIGNED_BYTE,Aarray[6]>#<SIGNED_BYTE,Aarray[7]>#<SIGNED_BYTE,Aarray[8]>#<SIGNED_BYTE,Aarray[9]>#<SIGNED_BYTE,Aarray[10]>#<SIGNED_BYTE,Aarray[11]>#<SIGNED_BYTE,Aarray[12]>#<SIGNED_BYTE,Aarray[13]>#<SIGNED_BYTE,Aarray[14]>#<SIGNED_BYTE,Aarray[15]>#
NV_ANT2_PCS_CDMA_LNA_12_OFFSET_VS_FREQ_I,513,ReadWrite,<SIGNED_BYTE,Aarray[0]>#<SIGNED_BYTE,Aarray[1]>#<SIGNED_BYTE,Aarray[2]>#<SIGNED_BYTE,Aarray[3]>#<SIGNED_BYTE,Aarray[4]>#<SIGNED_BYTE,Aarray[5]>#<SIGNED_BYTE,Aarray[6]>#<SIGNED_BYTE,Aarray[7]>#<SIGNED_BYTE,Aarray[8]>#<SIGNED_BYTE,Aarray[9]>#<SIGNED_BYTE,Aarray[10]>#<SIGNED_BYTE,Aarray[11]>#<SIGNED_BYTE,Aarray[12]>#<SIGNED_BYTE,Aarray[13]>#<SIGNED_BYTE,Aarray[14]>#<SIGNED_BYTE,Aarray[15]>#
NV_TEST_CODE_VER_I,567,Read,<BYTE,Aarray[0]>#<BYTE,Aarray[1]>#<BYTE,Aarray[2]>#<BYTE,Aarray[3]>#<BYTE,Aarray[4]>#<BYTE,Aarray[5]>#<BYTE,Aarray[6]>#<BYTE,Aarray[7]>#
NV_SYS_SW_VER_I,568,Read,<BYTE,Aarray[0]>#<BYTE,Aarray[1]>#<BYTE,Aarray[2]>#<BYTE,Aarray[3]>#<BYTE,Aarray[4]>#<BYTE,Aarray[5]>#<BYTE,Aarray[6]>#<BYTE,Aarray[7]>#
NV_RF_CAL_VER_I,569,Read,<BYTE,Aarray[0]>#<BYTE,Aarray[1]>#<BYTE,Aarray[2]>#<BYTE,Aarray[3]>#<BYTE,Aarray[4]>#<BYTE,Aarray[5]>#<BYTE,Aarray[6]>#<BYTE,Aarray[7]>#
NV_RF_CONFIG_VER_I,570,Read,<BYTE,Aarray[0]>#<BYTE,Aarray[1]>#<BYTE,Aarray[2]>#<BYTE,Aarray[3]>#<BYTE,Aarray[4]>#<BYTE,Aarray[5]>#<BYTE,Aarray[6]>#<BYTE,Aarray[7]>#
NV_RF_CAL_DATE_I,571,ReadTime,<DWORD,RF Cal date>#
NV_RF_NV_LOADED_DATE_I,572,ReadWriteTime,<DWORD,RF NV Loaded date>#
NV_RF_CAL_DAT_FILE_I,573,Read,<BYTE,Aarray[0]>#<BYTE,Aarray[1]>#<BYTE,Aarray[2]>#<BYTE,Aarray[3]>#<BYTE,Aarray[4]>#<BYTE,Aarray[5]>#<BYTE,Aarray[6]>#<BYTE,Aarray[7]>#<BYTE,Aarray[8]>#
NV_AGC_VALUE_3_MIN_I,587,ReadWrite,<SIGNED_BYTE,AGC value 3 min>#
NV_AGC_VALUE_4_MIN_I,588,ReadWrite,<SIGNED_BYTE,AGC value 4 min>#
NV_TX_GAIN_ATTEN_LIMIT_I,589,ReadWrite,<SIGNED_WORD,TX gain atten limit>#
NV_CDMA_LNA_3_FALL_I,590,ReadWrite,<SIGNED_BYTE,CDMA LNA 3 fall>#
NV_CDMA_LNA_3_OFFSET_I,591,ReadWrite,<SIGNED_WORD,CDMA LNA 3 offset>#
NV_CDMA_LNA_3_RISE_I,592,ReadWrite,<SIGNED_BYTE,CDMA LNA 3 rise>#
NV_CDMA_LNA_3_OFFSET_VS_FREQ_I,593,ReadWrite,<SIGNED_BYTE,Aarray[0]>#<SIGNED_BYTE,Aarray[1]>#<SIGNED_BYTE,Aarray[2]>#<SIGNED_BYTE,Aarray[3]>#<SIGNED_BYTE,Aarray[4]>#<SIGNED_BYTE,Aarray[5]>#<SIGNED_BYTE,Aarray[6]>#<SIGNED_BYTE,Aarray[7]>#<SIGNED_BYTE,Aarray[8]>#<SIGNED_BYTE,Aarray[9]>#<SIGNED_BYTE,Aarray[10]>#<SIGNED_BYTE,Aarray[11]>#<SIGNED_BYTE,Aarray[12]>#<SIGNED_BYTE,Aarray[13]>#<SIGNED_BYTE,Aarray[14]>#<SIGNED_BYTE,Aarray[15]>#
NV_PCS_LNA_3_FALL_I,594,ReadWrite,<SIGNED_BYTE,PCS LNA 3 fall>#
NV_PCS_LNA_3_OFFSET_I,595,ReadWrite,<SIGNED_WORD,PCS LNA 3 offset>#
NV_PCS_LNA_3_RISE_I,596,ReadWrite,<SIGNED_BYTE,PCS LNA 3 rise>#
NV_PCS_LNA_3_OFFSET_VS_FREQ_I,597,ReadWrite,<SIGNED_BYTE,Aarray[0]>#<SIGNED_BYTE,Aarray[1]>#<SIGNED_BYTE,Aarray[2]>#<SIGNED_BYTE,Aarray[3]>#<SIGNED_BYTE,Aarray[4]>#<SIGNED_BYTE,Aarray[5]>#<SIGNED_BYTE,Aarray[6]>#<SIGNED_BYTE,Aarray[7]>#<SIGNED_BYTE,Aarray[8]>#<SIGNED_BYTE,Aarray[9]>#<SIGNED_BYTE,Aarray[10]>#<SIGNED_BYTE,Aarray[11]>#<SIGNED_BYTE,Aarray[12]>#<SIGNED_BYTE,Aarray[13]>#<SIGNED_BYTE,Aarray[14]>#<SIGNED_BYTE,Aarray[15]>#
NV_CDMA_LNA_4_FALL_I,598,ReadWrite,<SIGNED_BYTE,CDMA LNA 4 fall>#
NV_CDMA_LNA_4_OFFSET_I,599,ReadWrite,<SIGNED_WORD,CDMA LNA 4 offset>#
NV_CDMA_LNA_4_RISE_I,600,ReadWrite,<SIGNED_BYTE,CDMA LNA 4 rise>#
NV_CDMA_LNA_4_OFFSET_VS_FREQ_I,601,ReadWrite,<SIGNED_BYTE,Aarray[0]>#<SIGNED_BYTE,Aarray[1]>#<SIGNED_BYTE,Aarray[2]>#<SIGNED_BYTE,Aarray[3]>#<SIGNED_BYTE,Aarray[4]>#<SIGNED_BYTE,Aarray[5]>#<SIGNED_BYTE,Aarray[6]>#<SIGNED_BYTE,Aarray[7]>#<SIGNED_BYTE,Aarray[8]>#<SIGNED_BYTE,Aarray[9]>#<SIGNED_BYTE,Aarray[10]>#<SIGNED_BYTE,Aarray[11]>#<SIGNED_BYTE,Aarray[12]>#<SIGNED_BYTE,Aarray[13]>#<SIGNED_BYTE,Aarray[14]>#<SIGNED_BYTE,Aarray[15]>#
NV_PCS_LNA_4_FALL_I,602,ReadWrite,<SIGNED_BYTE,PCS LNA 4 fall>#
NV_PCS_LNA_4_OFFSET_I,603,ReadWrite,<SIGNED_WORD,PCS LNA 4 offset>#
NV_PCS_LNA_4_RISE_I,604,ReadWrite,<SIGNED_BYTE,PCS LNA 4 rise>#
NV_PCS_LNA_4_OFFSET_VS_FREQ_I,605,ReadWrite,<SIGNED_BYTE,Aarray[0]>#<SIGNED_BYTE,Aarray[1]>#<SIGNED_BYTE,Aarray[2]>#<SIGNED_BYTE,Aarray[3]>#<SIGNED_BYTE,Aarray[4]>#<SIGNED_BYTE,Aarray[5]>#<SIGNED_BYTE,Aarray[6]>#<SIGNED_BYTE,Aarray[7]>#<SIGNED_BYTE,Aarray[8]>#<SIGNED_BYTE,Aarray[9]>#<SIGNED_BYTE,Aarray[10]>#<SIGNED_BYTE,Aarray[11]>#<SIGNED_BYTE,Aarray[12]>#<SIGNED_BYTE,Aarray[13]>#<SIGNED_BYTE,Aarray[14]>#<SIGNED_BYTE,Aarray[15]>#
NV_DFM_LNA_FALL_I,606,ReadWrite,<SIGNED_BYTE,DFM LNA fall>#
NV_DFM_LNA_OFFSET_I,607,ReadWrite,<SIGNED_WORD,DFM LNA offset>#
NV_DFM_LNA_RISE_I,608,ReadWrite,<SIGNED_BYTE,DFM LNA rise>#
NV_DFM_LNA_OFFSET_VS_FREQ_I,609,ReadWrite,<SIGNED_BYTE,Aarray[0]>#<SIGNED_BYTE,Aarray[1]>#<SIGNED_BYTE,Aarray[2]>#<SIGNED_BYTE,Aarray[3]>#<SIGNED_BYTE,Aarray[4]>#<SIGNED_BYTE,Aarray[5]>#<SIGNED_BYTE,Aarray[6]>#<SIGNED_BYTE,Aarray[7]>#<SIGNED_BYTE,Aarray[8]>#<SIGNED_BYTE,Aarray[9]>#<SIGNED_BYTE,Aarray[10]>#<SIGNED_BYTE,Aarray[11]>#<SIGNED_BYTE,Aarray[12]>#<SIGNED_BYTE,Aarray[13]>#<SIGNED_BYTE,Aarray[14]>#<SIGNED_BYTE,Aarray[15]>#
NV_CDMA_IM2_I_VALUE_I,687,ReadWrite,<BYTE,IM2 I value>#
NV_PCS_IM2_I_VALUE_I,688,ReadWrite,<BYTE,IM2 I value>#
NV_CDMA_IM2_Q_VALUE_I,689,ReadWrite,<BYTE,IM2 Q value>#
NV_PCS_IM2_Q_VALUE_I,690,ReadWrite,<BYTE,IM2 Q value>#
NV_FM_VGA_GAIN_OFFSET_I,692,ReadWrite,<SIGNED_WORD,Offset>#
NV_CDMA_VGA_GAIN_OFFSET_I,693,ReadWrite,<SIGNED_WORD,Offset>#
NV_PCS_VGA_GAIN_OFFSET_I,694,ReadWrite,<SIGNED_WORD,Offset>#
NV_FM_VGA_GAIN_OFFSET_VS_FREQ_I,695,ReadWrite,<SIGNED_BYTE,Aarray[0]>#<SIGNED_BYTE,Aarray[1]>#<SIGNED_BYTE,Aarray[2]>#<SIGNED_BYTE,Aarray[3]>#<SIGNED_BYTE,Aarray[4]>#<SIGNED_BYTE,Aarray[5]>#<SIGNED_BYTE,Aarray[6]>#<SIGNED_BYTE,Aarray[7]>#<SIGNED_BYTE,Aarray[8]>#<SIGNED_BYTE,Aarray[9]>#<SIGNED_BYTE,Aarray[10]>#<SIGNED_BYTE,Aarray[11]>#<SIGNED_BYTE,Aarray[12]>#<SIGNED_BYTE,Aarray[13]>#<SIGNED_BYTE,Aarray[14]>#<SIGNED_BYTE,Aarray[15]>#
NV_CDMA_VGA_GAIN_OFFSET_VS_FREQ_I,696,ReadWrite,<SIGNED_BYTE,Aarray[0]>#<SIGNED_BYTE,Aarray[1]>#<SIGNED_BYTE,Aarray[2]>#<SIGNED_BYTE,Aarray[3]>#<SIGNED_BYTE,Aarray[4]>#<SIGNED_BYTE,Aarray[5]>#<SIGNED_BYTE,Aarray[6]>#<SIGNED_BYTE,Aarray[7]>#<SIGNED_BYTE,Aarray[8]>#<SIGNED_BYTE,Aarray[9]>#<SIGNED_BYTE,Aarray[10]>#<SIGNED_BYTE,Aarray[11]>#<SIGNED_BYTE,Aarray[12]>#<SIGNED_BYTE,Aarray[13]>#<SIGNED_BYTE,Aarray[14]>#<SIGNED_BYTE,Aarray[15]>#
NV_PCS_VGA_GAIN_OFFSET_VS_FREQ_I,697,ReadWrite,<SIGNED_BYTE,Aarray[0]>#<SIGNED_BYTE,Aarray[1]>#<SIGNED_BYTE,Aarray[2]>#<SIGNED_BYTE,Aarray[3]>#<SIGNED_BYTE,Aarray[4]>#<SIGNED_BYTE,Aarray[5]>#<SIGNED_BYTE,Aarray[6]>#<SIGNED_BYTE,Aarray[7]>#<SIGNED_BYTE,Aarray[8]>#<SIGNED_BYTE,Aarray[9]>#<SIGNED_BYTE,Aarray[10]>#<SIGNED_BYTE,Aarray[11]>#<SIGNED_BYTE,Aarray[12]>#<SIGNED_BYTE,Aarray[13]>#<SIGNED_BYTE,Aarray[14]>#<SIGNED_BYTE,Aarray[15]>#
NV_FM_VGA_GAIN_OFFSET_VS_TEMP_I,698,ReadWrite,<SIGNED_WORD,Aarray[0]>#<SIGNED_WORD,Aarray[1]>#<SIGNED_WORD,Aarray[2]>#<SIGNED_WORD,Aarray[3]>#<SIGNED_WORD,Aarray[4]>#<SIGNED_WORD,Aarray[5]>#<SIGNED_WORD,Aarray[6]>#<SIGNED_WORD,Aarray[7]>#<SIGNED_WORD,Aarray[8]>#<SIGNED_WORD,Aarray[9]>#<SIGNED_WORD,Aarray[10]>#<SIGNED_WORD,Aarray[11]>#<SIGNED_WORD,Aarray[12]>#<SIGNED_WORD,Aarray[13]>#<SIGNED_WORD,Aarray[14]>#<SIGNED_WORD,Aarray[15]>#
NV_CDMA_VGA_GAIN_OFFSET_VS_TEMP_I,699,ReadWrite,<SIGNED_WORD,Aarray[0]>#<SIGNED_WORD,Aarray[1]>#<SIGNED_WORD,Aarray[2]>#<SIGNED_WORD,Aarray[3]>#<SIGNED_WORD,Aarray[4]>#<SIGNED_WORD,Aarray[5]>#<SIGNED_WORD,Aarray[6]>#<SIGNED_WORD,Aarray[7]>#<SIGNED_WORD,Aarray[8]>#<SIGNED_WORD,Aarray[9]>#<SIGNED_WORD,Aarray[10]>#<SIGNED_WORD,Aarray[11]>#<SIGNED_WORD,Aarray[12]>#<SIGNED_WORD,Aarray[13]>#<SIGNED_WORD,Aarray[14]>#<SIGNED_WORD,Aarray[15]>#
NV_PCS_VGA_GAIN_OFFSET_VS_TEMP_I,700,ReadWrite,<SIGNED_WORD,Aarray[0]>#<SIGNED_WORD,Aarray[1]>#<SIGNED_WORD,Aarray[2]>#<SIGNED_WORD,Aarray[3]>#<SIGNED_WORD,Aarray[4]>#<SIGNED_WORD,Aarray[5]>#<SIGNED_WORD,Aarray[6]>#<SIGNED_WORD,Aarray[7]>#<SIGNED_WORD,Aarray[8]>#<SIGNED_WORD,Aarray[9]>#<SIGNED_WORD,Aarray[10]>#<SIGNED_WORD,Aarray[11]>#<SIGNED_WORD,Aarray[12]>#<SIGNED_WORD,Aarray[13]>#<SIGNED_WORD,Aarray[14]>#<SIGNED_WORD,Aarray[15]>#
NV_FM_MIS_COMP_A_OFFSET_I,701,ReadWrite,<SIGNED_DWORD,Offset>#
NV_DIGITAL_MIS_COMP_A_OFFSET_I,702,ReadWrite,<SIGNED_DWORD,Offset>#
NV_FM_MIS_COMP_B_OFFSET_I,704,ReadWrite,<SIGNED_DWORD,Offset>#
NV_DIGITAL_MIS_COMP_B_OFFSET_I,705,ReadWrite,<SIGNED_DWORD,Offset>#
NV_IM_LEVEL3_I,585,ReadWrite,<SIGNED_BYTE,IM level 3>#
NV_IM_LEVEL4_I,586,ReadWrite,<SIGNED_BYTE,IM level 4>#
NV_DFM_AGC_ACC_MIN_1_I,610,ReadWrite,<BYTE,DFM AGC ACC MIN 1>#
NV_DFM_AGC_IM_GAIN_I,611,ReadWrite,<BYTE,DFM AGC IM gain >#
NV_DFM_AGC_DC_GAIN_I,612,ReadWrite,<BYTE,DFM AGC DC gain >#
NV_DFM_IM_LEVEL1_I,613,ReadWrite,<SIGNED_BYTE,DFM IM level 1>#
NV_GPS_FG_TRK_OFFSET_SCALER_I,614,ReadWrite,<BYTE,Trk offset scaler>#
NV_DIGITAL_FG_TRK_OFFSET_SCALER_I,615,ReadWrite,<BYTE,Trk offset scaler>#
NV_FM_FG_TRK_OFFSET_SCALER_I,616,ReadWrite,<BYTE,Trk offset scaler>#
NV_DFM_LNA_S0_PHASE_OFFSET_I,617,ReadWrite,<WORD,Phase offset>#
NV_DFM_LNA_S1_PHASE_OFFSET_I,618,ReadWrite,<WORD,Phase offset>#
NV_CDMA_RXF_CG_IOFFSET_I,619,ReadWrite,<DWORD,RXF CG Offset>#
NV_PCS_RXF_CG_IOFFSET_I,620,ReadWrite,<DWORD,RXF CG Offset>#
NV_FM_RXF_CG_IOFFSET_I,621,ReadWrite,<DWORD,RXF CG Offset>#
NV_GPS_RXF_CG_IOFFSET_I,622,ReadWrite,<DWORD,RXF CG Offset>#
NV_CDMA_RXF_CG_QOFFSET_I,623,ReadWrite,<DWORD,RXF CG Offset>#
NV_PCS_RXF_CG_QOFFSET_I,624,ReadWrite,<DWORD,RXF CG Offset>#
NV_FM_RXF_CG_QOFFSET_I,625,ReadWrite,<DWORD,RXF CG Offset>#
NV_GPS_RXF_CG_QOFFSET_I,626,ReadWrite,<DWORD,RXF CG Offset>#
NV_CDMA_RXF_FG_IOFFSET_I,627,ReadWrite,<DWORD,RXF CG Offset>#
NV_PCS_RXF_FG_IOFFSET_I,628,ReadWrite,<DWORD,RXF CG Offset>#
NV_FM_RXF_FG_IOFFSET_I,629,ReadWrite,<DWORD,RXF CG Offset>#
NV_GPS_RXF_FG_IOFFSET_I,630,ReadWrite,<DWORD,RXF CG Offset>#
NV_CDMA_RXF_FG_QOFFSET_I,631,ReadWrite,<DWORD,RXF CG Offset>#
NV_PCS_RXF_FG_QOFFSET_I,632,ReadWrite,<DWORD,RXF CG Offset>#
NV_FM_RXF_FG_QOFFSET_I,633,ReadWrite,<DWORD,RXF CG Offset>#
NV_GPS_RXF_FG_QOFFSET_I,634,ReadWrite,<DWORD,RXF CG Offset>#
NV_CDMA_DACC_EST_IOFFSET_I,635,ReadWrite,<DWORD,RXF CG Offset>#
NV_PCS_DACC_EST_IOFFSET_I,636,ReadWrite,<DWORD,RXF CG Offset>#
NV_FM_DACC_EST_IOFFSET_I,637,ReadWrite,<DWORD,RXF CG Offset>#
NV_GPS_DACC_EST_IOFFSET_I,638,ReadWrite,<DWORD,RXF CG Offset>#
NV_CDMA_DACC_EST_QOFFSET_I,639,ReadWrite,<DWORD,RXF CG Offset>#
NV_PCS_DACC_EST_QOFFSET_I,640,ReadWrite,<DWORD,RXF CG Offset>#
NV_FM_DACC_EST_QOFFSET_I,641,ReadWrite,<DWORD,RXF CG Offset>#
NV_GPS_DACC_EST_QOFFSET_I,642,ReadWrite,<DWORD,RXF CG Offset>#
NV_CDMA_DACC_IACCUM0_I,643,ReadWrite,<BYTE,DACC Accum>#
NV_PCS_DACC_IACCUM0_I,644,ReadWrite,<BYTE,DACC Accum>#
NV_FM_DACC_IACCUM0_I,645,ReadWrite,<BYTE,DACC Accum>#
NV_GPS_DACC_IACCUM0_I,646,ReadWrite,<BYTE,DACC Accum>#
NV_CDMA_DACC_IACCUM1_I,647,ReadWrite,<BYTE,DACC Accum>#
NV_PCS_DACC_IACCUM1_I,648,ReadWrite,<BYTE,DACC Accum>#
NV_FM_DACC_IACCUM1_I,649,ReadWrite,<BYTE,DACC Accum>#
NV_GPS_DACC_IACCUM1_I,650,ReadWrite,<BYTE,DACC Accum>#
NV_CDMA_DACC_IACCUM2_I,651,ReadWrite,<BYTE,DACC Accum>#
NV_PCS_DACC_IACCUM2_I,652,ReadWrite,<BYTE,DACC Accum>#
NV_FM_DACC_IACCUM2_I,653,ReadWrite,<BYTE,DACC Accum>#
NV_GPS_DACC_IACCUM2_I,654,ReadWrite,<BYTE,DACC Accum>#
NV_CDMA_DACC_IACCUM3_I,655,ReadWrite,<BYTE,DACC Accum>#
NV_PCS_DACC_IACCUM3_I,656,ReadWrite,<BYTE,DACC Accum>#
NV_FM_DACC_IACCUM3_I,657,ReadWrite,<BYTE,DACC Accum>#
NV_GPS_DACC_IACCUM3_I,658,ReadWrite,<BYTE,DACC Accum>#
NV_CDMA_DACC_IACCUM4_I,659,ReadWrite,<BYTE,DACC Accum>#
NV_PCS_DACC_IACCUM4_I,660,ReadWrite,<BYTE,DACC Accum>#
NV_FM_DACC_IACCUM4_I,661,ReadWrite,<BYTE,DACC Accum>#
NV_GPS_DACC_IACCUM4_I,662,ReadWrite,<BYTE,DACC Accum>#
NV_CDMA_DACC_QACCUM0_I,663,ReadWrite,<BYTE,DACC Accum>#
NV_PCS_DACC_QACCUM0_I,664,ReadWrite,<BYTE,DACC Accum>#
NV_FM_DACC_QACCUM0_I,665,ReadWrite,<BYTE,DACC Accum>#
NV_GPS_DACC_QACCUM0_I,666,ReadWrite,<BYTE,DACC Accum>#
NV_CDMA_DACC_QACCUM1_I,667,ReadWrite,<BYTE,DACC Accum>#
NV_PCS_DACC_QACCUM1_I,668,ReadWrite,<BYTE,DACC Accum>#
NV_FM_DACC_QACCUM1_I,669,ReadWrite,<BYTE,DACC Accum>#
NV_GPS_DACC_QACCUM1_I,670,ReadWrite,<BYTE,DACC Accum>#
NV_CDMA_DACC_QACCUM2_I,671,ReadWrite,<BYTE,DACC Accum>#
NV_PCS_DACC_QACCUM2_I,672,ReadWrite,<BYTE,DACC Accum>#
NV_FM_DACC_QACCUM2_I,673,ReadWrite,<BYTE,DACC Accum>#
NV_GPS_DACC_QACCUM2_I,674,ReadWrite,<BYTE,DACC Accum>#
NV_CDMA_DACC_QACCUM3_I,675,ReadWrite,<BYTE,DACC Accum>#
NV_PCS_DACC_QACCUM3_I,676,ReadWrite,<BYTE,DACC Accum>#
NV_FM_DACC_QACCUM3_I,677,ReadWrite,<BYTE,DACC Accum>#
NV_GPS_DACC_QACCUM3_I,678,ReadWrite,<BYTE,DACC Accum>#
NV_CDMA_DACC_QACCUM4_I,679,ReadWrite,<BYTE,DACC Accum>#
NV_PCS_DACC_QACCUM4_I,680,ReadWrite,<BYTE,DACC Accum>#
NV_FM_DACC_QACCUM4_I,681,ReadWrite,<BYTE,DACC Accum>#
NV_GPS_DACC_QACCUM4_I,682,ReadWrite,<BYTE,DACC Accum>#
NV_CDMA_DACC_GAIN_MULT_I,683,ReadWrite,<BYTE,Gain mult>#
NV_PCS_DACC_GAIN_MULT_I,684,ReadWrite,<BYTE,Gain mult>#
NV_FM_DACC_GAIN_MULT_I,685,ReadWrite,<BYTE,Gain mult>#
NV_GPS_DACC_GAIN_MULT_I,686,ReadWrite,<BYTE,Gain mult>#
NV_RTC_TIME_ADJUST_I,691,ReadWrite,<BYTE,Time adjust>#
NV_GPS_MIS_COMP_A_OFFSET_I,703,ReadWrite,<SIGNED_DWORD,Offset>#
NV_GPS_MIS_COMP_B_OFFSET_I,706,ReadWrite,<SIGNED_DWORD,Offset>#
NV_PCS_IM_LEVEL3_I,715,ReadWrite,<SIGNED_BYTE,IM level 3>#
NV_PCS_IM_LEVEL4_I,716,ReadWrite,<SIGNED_BYTE,IM level 4>#
NV_PCS_AGC_VALUE_3_MIN_I,717,ReadWrite,<SIGNED_BYTE,AGC value 3 min>#
NV_PCS_AGC_VALUE_4_MIN_I,718,ReadWrite,<SIGNED_BYTE,AGC value 4 min>#
NV_GSM_CAL_ARFCN_I,724,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#
NV_DCS_CAL_ARFCN_I,725,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#
NV_GSM_RX_GAIN_RANGE_1_FREQ_COMP_I,726,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#
NV_GSM_RX_GAIN_RANGE_2_FREQ_COMP_I,727,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#
NV_GSM_RX_GAIN_RANGE_3_FREQ_COMP_I,728,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#
NV_GSM_RX_GAIN_RANGE_4_FREQ_COMP_I,729,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#
NV_DCS_RX_GAIN_RANGE_1_FREQ_COMP_I,730,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#
NV_DCS_RX_GAIN_RANGE_2_FREQ_COMP_I,731,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#
NV_DCS_RX_GAIN_RANGE_3_FREQ_COMP_I,732,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#
NV_DCS_RX_GAIN_RANGE_4_FREQ_COMP_I,733,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#
NV_GSM_TRK_LO_ADJ_PDM_INIT_VAL_I,734,ReadWrite,<WORD,PDM init val>#
NV_GSM_TRK_LO_ADJ_PDM_GAIN_SLOPE_I,735,ReadWrite,<WORD,PDM gain slope>#
NV_GSM_TX_BURST_RAMP_UP_INDEX_00_I,740,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_GSM_TX_BURST_RAMP_UP_INDEX_01_I,741,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_GSM_TX_BURST_RAMP_UP_INDEX_02_I,742,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_GSM_TX_BURST_RAMP_UP_INDEX_03_I,743,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_GSM_TX_BURST_RAMP_UP_INDEX_04_I,744,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_GSM_TX_BURST_RAMP_UP_INDEX_05_I,745,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_GSM_TX_BURST_RAMP_UP_INDEX_06_I,746,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_GSM_TX_BURST_RAMP_UP_INDEX_07_I,747,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_GSM_TX_BURST_RAMP_UP_INDEX_08_I,748,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_GSM_TX_BURST_RAMP_UP_INDEX_09_I,749,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_GSM_TX_BURST_RAMP_UP_INDEX_10_I,750,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_GSM_TX_BURST_RAMP_UP_INDEX_11_I,751,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_GSM_TX_BURST_RAMP_UP_INDEX_12_I,752,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_GSM_TX_BURST_RAMP_UP_INDEX_13_I,753,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_GSM_TX_BURST_RAMP_UP_INDEX_14_I,754,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_GSM_TX_BURST_RAMP_DOWN_INDEX_00_I,755,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_GSM_TX_BURST_RAMP_DOWN_INDEX_01_I,756,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_GSM_TX_BURST_RAMP_DOWN_INDEX_02_I,757,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_GSM_TX_BURST_RAMP_DOWN_INDEX_03_I,758,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_GSM_TX_BURST_RAMP_DOWN_INDEX_04_I,759,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_GSM_TX_BURST_RAMP_DOWN_INDEX_05_I,760,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_GSM_TX_BURST_RAMP_DOWN_INDEX_06_I,761,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_GSM_TX_BURST_RAMP_DOWN_INDEX_07_I,762,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_GSM_TX_BURST_RAMP_DOWN_INDEX_08_I,763,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_GSM_TX_BURST_RAMP_DOWN_INDEX_09_I,764,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_GSM_TX_BURST_RAMP_DOWN_INDEX_10_I,765,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_GSM_TX_BURST_RAMP_DOWN_INDEX_11_I,766,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_GSM_TX_BURST_RAMP_DOWN_INDEX_12_I,767,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_GSM_TX_BURST_RAMP_DOWN_INDEX_13_I,768,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_GSM_TX_BURST_RAMP_DOWN_INDEX_14_I,769,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_DCS_TX_BURST_RAMP_UP_INDEX_00_I,770,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_DCS_TX_BURST_RAMP_UP_INDEX_01_I,771,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_DCS_TX_BURST_RAMP_UP_INDEX_02_I,772,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_DCS_TX_BURST_RAMP_UP_INDEX_03_I,773,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_DCS_TX_BURST_RAMP_UP_INDEX_04_I,774,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_DCS_TX_BURST_RAMP_UP_INDEX_05_I,775,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_DCS_TX_BURST_RAMP_UP_INDEX_06_I,776,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_DCS_TX_BURST_RAMP_UP_INDEX_07_I,777,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_DCS_TX_BURST_RAMP_UP_INDEX_08_I,778,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_DCS_TX_BURST_RAMP_UP_INDEX_09_I,779,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_DCS_TX_BURST_RAMP_UP_INDEX_10_I,780,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_DCS_TX_BURST_RAMP_UP_INDEX_11_I,781,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_DCS_TX_BURST_RAMP_UP_INDEX_12_I,782,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_DCS_TX_BURST_RAMP_UP_INDEX_13_I,783,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_DCS_TX_BURST_RAMP_UP_INDEX_14_I,784,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_DCS_TX_BURST_RAMP_UP_INDEX_15_I,785,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_DCS_TX_BURST_RAMP_DOWN_INDEX_00_I,786,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_DCS_TX_BURST_RAMP_DOWN_INDEX_01_I,787,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_DCS_TX_BURST_RAMP_DOWN_INDEX_02_I,788,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_DCS_TX_BURST_RAMP_DOWN_INDEX_03_I,789,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_DCS_TX_BURST_RAMP_DOWN_INDEX_04_I,790,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_DCS_TX_BURST_RAMP_DOWN_INDEX_05_I,791,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_DCS_TX_BURST_RAMP_DOWN_INDEX_06_I,792,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_DCS_TX_BURST_RAMP_DOWN_INDEX_07_I,793,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_DCS_TX_BURST_RAMP_DOWN_INDEX_08_I,794,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_DCS_TX_BURST_RAMP_DOWN_INDEX_09_I,795,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_DCS_TX_BURST_RAMP_DOWN_INDEX_10_I,796,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_DCS_TX_BURST_RAMP_DOWN_INDEX_11_I,797,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_DCS_TX_BURST_RAMP_DOWN_INDEX_12_I,798,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_DCS_TX_BURST_RAMP_DOWN_INDEX_13_I,799,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_DCS_TX_BURST_RAMP_DOWN_INDEX_14_I,800,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_DCS_TX_BURST_RAMP_DOWN_INDEX_15_I,801,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#
NV_GSM_PA_GAIN_SLOPE_I,802,ReadWrite,<BYTE,Array[0]>#<BYTE,Array[1]>#<BYTE,Array[2]>#<BYTE,Array[3]>#<BYTE,Array[4]>#<BYTE,Array[5]>#<BYTE,Array[6]>#<BYTE,Array[7]>#<BYTE,Array[8]>#<BYTE,Array[9]>#<BYTE,Array[10]>#<BYTE,Array[11]>#<BYTE,Array[12]>#<BYTE,Array[13]>#<BYTE,Array[14]>#
NV_DCS_PA_GAIN_SLOPE_I,803,ReadWrite,<BYTE,Array[0]>#<BYTE,Array[1]>#<BYTE,Array[2]>#<BYTE,Array[3]>#<BYTE,Array[4]>#<BYTE,Array[5]>#<BYTE,Array[6]>#<BYTE,Array[7]>#<BYTE,Array[8]>#<BYTE,Array[9]>#<BYTE,Array[10]>#<BYTE,Array[11]>#<BYTE,Array[12]>#<BYTE,Array[13]>#<BYTE,Array[14]>#<BYTE,Array[15]>#
NV_GSM_TX_FREQ_COMP_I,804,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#
NV_DCS_TX_FREQ_COMP_I,805,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_GSM_VBATT_HI_PA_COMP_I,806,ReadWrite,<BYTE,VBATT HI PA comp>#
NV_GSM_VBATT_LO_PA_COMP_I,807,ReadWrite,<BYTE,VBATT LO PA comp>#
NV_DCS_VBATT_HI_PA_COMP_I,808,ReadWrite,<BYTE,VBATT HI PA comp>#
NV_DCS_VBATT_LO_PA_COMP_I,809,ReadWrite,<BYTE,VBATT LO PA comp>#
NV_VBATT_3200_MV_ADC_I,810,ReadWrite,<WORD,3200 MV ADC>#
NV_VBATT_3700_MV_ADC_I,811,ReadWrite,<WORD,3700 MV ADC>#
NV_VBATT_4200_MV_ADC_I,812,ReadWrite,<WORD,4200 MV ADC>#
NV_GSM_PRECHARGE_I,813,ReadWrite,<WORD,GSM pre-charge>#
NV_DCS_PRECHARGE_I,814,ReadWrite,<WORD,DCS pre-charge>#
NV_GSM_PRECHARGE_DUR_I,815,ReadWrite,<WORD,GSM pre-charge dur>#
NV_DCS_PRECHARGE_DUR_I,816,ReadWrite,<WORD,DCS pre-charge dur>#
NV_DIGITAL_PLL_LOCK_TIMER_I,817,ReadWrite,<BYTE,Digitial PLL lock Timer>#
NV_GSM_PA_START_TIME_OFFSET_I,819,ReadWrite,<SIGNED_BYTE,GSM PA start time offset>#
NV_GSM_PA_STOP_TIME_OFFSET_I,820,ReadWrite,<SIGNED_BYTE,GSM PA stop time offset>#
NV_DCS_PA_START_TIME_OFFSET_I,821,ReadWrite,<SIGNED_BYTE,DCS PA start time offset>#
NV_DCS_PA_STOP_TIME_OFFSET_I,822,ReadWrite,<SIGNED_BYTE,DCS PA stop time offset>#
NV_CDMA_IM2_TRANSCONDUCTOR_VALUE_I,837,ReadWrite,<BYTE,Transconductor value>#
NV_PCS_IM2_TRANSCONDUCTOR_VALUE_I,838,ReadWrite,<BYTE,Transconductor value>#
NV_LNA_NON_BYPASS_TIMER_0_I,839,ReadWrite,<WORD,Non-bypass timer>#
NV_LNA_NON_BYPASS_TIMER_1_I,840,ReadWrite,<WORD,Non-bypass timer>#
NV_LNA_NON_BYPASS_TIMER_2_I,841,ReadWrite,<WORD,Non-bypass timer>#
NV_LNA_NON_BYPASS_TIMER_3_I,842,ReadWrite,<WORD,Non-bypass timer>#
NV_LNA_BYPASS_TIMER_0_I,843,ReadWrite,<WORD,Bypass timer>#
NV_LNA_BYPASS_TIMER_1_I,844,ReadWrite,<WORD,Bypass timer>#
NV_LNA_BYPASS_TIMER_2_I,845,ReadWrite,<WORD,Bypass timer>#
NV_LNA_BYPASS_TIMER_3_I,846,ReadWrite,<WORD,Bypass timer>#
NV_WCDMA_VGA_GAIN_OFFSET_I,856,ReadWrite,<SIGNED_WORD,VGA gain offset>#
NV_WCDMA_VGA_GAIN_OFFSET_VS_FREQ_I,857,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_WCDMA_VGA_GAIN_OFFSET_VS_TEMP_I,858,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#
NV_WCDMA_LNA_RANGE_RISE_2_I,859,ReadWrite,<SIGNED_WORD,LNA range rise 2>#
NV_WCDMA_LNA_RANGE_RISE_3_I,860,ReadWrite,<SIGNED_WORD,LNA range rise 3>#
NV_WCDMA_LNA_RANGE_FALL_2_I,861,ReadWrite,<SIGNED_WORD,LNA range fall 2>#
NV_WCDMA_LNA_RANGE_FALL_3_I,862,ReadWrite,<SIGNED_WORD,LNA range fall 3>#
NV_WCDMA_IM_LEVEL_2_I,863,ReadWrite,<SIGNED_WORD,IM level 2>#
NV_WCDMA_IM_LEVEL_3_I,864,ReadWrite,<SIGNED_WORD,IM level 3>#
NV_WCDMA_LNA_RANGE_OFFSET_2_I,865,ReadWrite,<SIGNED_WORD,LNA range offset 2>#
NV_WCDMA_LNA_RANGE_OFFSET_3_I,866,ReadWrite,<SIGNED_WORD,LNA range offset 3>#
NV_WCDMA_LNA_OFFSET_VS_FREQ_2_I,867,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_WCDMA_LNA_OFFSET_VS_FREQ_3_I,868,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_WCDMA_IM2_I_VALUE_I,869,ReadWrite,<BYTE,I value>#
NV_WCDMA_IM2_Q_VALUE_I,870,ReadWrite,<BYTE,Q value>#
NV_WCDMA_IM2_TRANSCONDUCTOR_VALUE_I,871,ReadWrite,<BYTE,Transconductore>#
NV_WCDMA_RX_AGC_MIN_2_I,872,ReadWrite,<SIGNED_WORD,RX AGC min 2>#
NV_WCDMA_RX_AGC_MIN_3_I,873,ReadWrite,<SIGNED_WORD,RX AGC min 3>#
NV_WCDMA_VBATT_I,874,ReadWrite,<BYTE,Array[0]>#<BYTE,Array[1]>#
NV_WCDMA_THERM_I,875,ReadWrite,<BYTE,Array[0]>#<BYTE,Array[1]>#
NV_WCDMA_MAX_TX_POWER_I,876,ReadWrite,<SIGNED_BYTE,Max TX power>#
NV_FM_PA_MAC_HIGH_I,877,ReadWrite,<BYTE,FM PA MAC high>#
NV_CDMA_DYNAMIC_RANGE_I,878,ReadWrite,<SIGNED_WORD,CDMA dynamic range>#
NV_CDMA_MIN_RX_RSSI_I,879,ReadWrite,<SIGNED_WORD,CDMA min RX rssi>#
NV_TX_WARMUP_I,884,ReadWrite,<WORD,TX warm up>#
NV_UE_IMEI_I,550,ReadWrite,<BYTE,Array[0]>#<BYTE,Array[1]>#<BYTE,Array[2]>#<BYTE,Array[3]>#<BYTE,Array[4]>#<BYTE,Array[5]>#<BYTE,Array[6]>#<BYTE,Array[7]>#<BYTE,Array[8]>#
NV_CDMA_P1_RISE_FALL_OFF_I,901,ReadWrite,<BYTE,Array[0]>#<BYTE,Array[1]>#<BYTE,Array[2]>#<BYTE,Array[3]>#<BYTE,Array[4]>#<BYTE,Array[5]>#<BYTE,Array[6]>#<BYTE,Array[7]>#
NV_PCS_P1_RISE_FALL_OFF_I,902,ReadWrite,<BYTE,Array[0]>#<BYTE,Array[1]>#<BYTE,Array[2]>#<BYTE,Array[3]>#<BYTE,Array[4]>#<BYTE,Array[5]>#<BYTE,Array[6]>#<BYTE,Array[7]>#
NV_FTM_MODE,453,ReadWrite,<BYTE,FTM mode>#
NV_C1_CDMA_LNA_OFFSET_I,948,ReadWrite,<SIGNED_WORD,Offset>#
NV_C1_CDMA_LNA_OFFSET_VS_FREQ_I,949,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C1_PCS_LNA_OFFSET_I,950,ReadWrite,<SIGNED_WORD,Offset>#
NV_C1_PCS_LNA_OFFSET_VS_FREQ_I,951,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C1_CDMA_LNA_2_OFFSET_I,952,ReadWrite,<SIGNED_WORD,Offset>#
NV_C1_CDMA_LNA_2_OFFSET_VS_FREQ_I,953,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C1_PCS_LNA_2_OFFSET_I,954,ReadWrite,<SIGNED_WORD,Offset>#
NV_C1_PCS_LNA_2_OFFSET_VS_FREQ_I,955,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C1_CDMA_LNA_3_OFFSET_I,956,ReadWrite,<SIGNED_WORD,Offset>#
NV_C1_CDMA_LNA_3_OFFSET_VS_FREQ_I,957,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C1_PCS_LNA_3_OFFSET_I,958,ReadWrite,<SIGNED_WORD,Offset>#
NV_C1_PCS_LNA_3_OFFSET_VS_FREQ_I,959,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C1_CDMA_LNA_4_OFFSET_I,960,ReadWrite,<SIGNED_WORD,Offset>#
NV_C1_CDMA_LNA_4_OFFSET_VS_FREQ_I,961,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C1_PCS_LNA_4_OFFSET_I,962,ReadWrite,<SIGNED_WORD,Offset>#
NV_C1_PCS_LNA_4_OFFSET_VS_FREQ_I,963,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C1_CDMA_P1_RISE_FALL_OFFSET_I,964,ReadWrite,<BYTE,Array[0]>#<BYTE,Array[1]>#<BYTE,Array[2]>#<BYTE,Array[3]>#<BYTE,Array[4]>#<BYTE,Array[5]>#<BYTE,Array[6]>#<BYTE,Array[7]>#
NV_C1_PCS_P1_RISE_FALL_OFFSET_I,965,ReadWrite,<BYTE,Array[0]>#<BYTE,Array[1]>#<BYTE,Array[2]>#<BYTE,Array[3]>#<BYTE,Array[4]>#<BYTE,Array[5]>#<BYTE,Array[6]>#<BYTE,Array[7]>#
NV_C1_RX_AGC_VALUE_1_MINMAX_I,966,ReadWrite,<BYTE,Min>#<BYTE,Max>#
NV_C1_RX_AGC_VALUE_2_MINMAX_I,967,ReadWrite,<BYTE,Min>#<BYTE,Max>#
NV_C1_RX_AGC_VALUE_3_MINMAX_I,968,ReadWrite,<BYTE,Min>#<BYTE,Max>#
NV_C1_RX_AGC_VALUE_4_MINMAX_I,969,ReadWrite,<BYTE,Min>#<BYTE,Max>#
NV_C0_RX_AGC_VREF_VAL_I,970,ReadWrite,<BYTE,VREF value or the difference between the base and switched values>#
NV_C1_RX_AGC_VREF_VAL_I,971,ReadWrite,<BYTE,VREF value or the difference between the base and switched values>#
NV_C0_GRP_DELAY_ADJ_I,972,ReadWrite,<BYTE,Define Group Delay Adjust>#
NV_C1_GRP_DELAY_ADJ_I,973,ReadWrite,<BYTE,Define Group Delay Adjust>#
NV_C1_CDMA_VGA_GAIN_OFFSET_I,974,ReadWrite,<SIGNED_WORD,13-bit 2's complement for Digital VGA gain offset>#
NV_C1_CDMA_VGA_GAIN_OFFSET_VS_FREQ_I,975,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C1_CDMA_VGA_GAIN_OFFSET_VS_TEMP_I,976,ReadWrite,<SIGNED_WORD,Array[0]>#<SIGNED_WORD,Array[1]>#<SIGNED_WORD,Array[2]>#<SIGNED_WORD,Array[3]>#<SIGNED_WORD,Array[4]>#<SIGNED_WORD,Array[5]>#<SIGNED_WORD,Array[6]>#<SIGNED_WORD,Array[7]>#
NV_C1_PCS_VGA_GAIN_OFFSET_I,977,ReadWrite,<SIGNED_WORD,13 bits complement interger for Digital VGA gain offset>#
NV_C1_PCS_VGA_GAIN_OFFSET_VS_FREQ_I,978,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C1_PCS_VGA_GAIN_OFFSET_VS_TEMP_I,979,ReadWrite,<SIGNED_WORD,Array[0]>#<SIGNED_WORD,Array[1]>#<SIGNED_WORD,Array[2]>#<SIGNED_WORD,Array[3]>#<SIGNED_WORD,Array[4]>#<SIGNED_WORD,Array[5]>#<SIGNED_WORD,Array[6]>#<SIGNED_WORD,Array[7]>#
NV_C1_DIGITAL_MIS_COMP_A_OFFSET_I,980,ReadWrite,<SIGNED_DWORD,In-phase coefficient for mismatch compensation>#
NV_C1_GPS_MIS_COMP_A_OFFSET_I,981,ReadWrite,<SIGNED_DWORD,In-phase coefficient for mismatch compensation>#
NV_C1_DIGITAL_MIS_COMP_B_OFFSET_I,982,ReadWrite,<SIGNED_DWORD,In-phase coefficient for mismatch compensation>#
NV_C1_GPS_MIS_COMP_B_OFFSET_I,983,ReadWrite,<SIGNED_DWORD,In-phase coefficient for mismatch compensation>#
NV_C1_CDMA_DACC_IACCUM0_I,984,ReadWrite,<BYTE,Internal Only>#
NV_C1_PCS_DACC_IACCUM0_I,985,ReadWrite,<BYTE,Internal Only>#
NV_C1_GPS_DACC_IACCUM0_I,986,ReadWrite,<BYTE,Internal Only>#
NV_C1_CDMA_DACC_IACCUM1_I,987,ReadWrite,<BYTE,Internal Only>#
NV_C1_PCS_DACC_IACCUM1_I,988,ReadWrite,<BYTE,Internal Only>#
NV_C1_GPS_DACC_IACCUM1_I,989,ReadWrite,<BYTE,Internal Only>#
NV_C1_CDMA_DACC_IACCUM2_I,990,ReadWrite,<BYTE,Internal Only>#
NV_C1_PCS_DACC_IACCUM2_I,991,ReadWrite,<BYTE,Internal Only>#
NV_C1_GPS_DACC_IACCUM2_I,992,ReadWrite,<BYTE,Internal Only>#
NV_C1_CDMA_DACC_IACCUM3_I,993,ReadWrite,<BYTE,Internal Only>#
NV_C1_PCS_DACC_IACCUM3_I,994,ReadWrite,<BYTE,Internal Only>#
NV_C1_GPS_DACC_IACCUM3_I,995,ReadWrite,<BYTE,Internal Only>#
NV_C1_CDMA_DACC_IACCUM4_I,996,ReadWrite,<BYTE,Internal Only>#
NV_C1_PCS_DACC_IACCUM4_I,997,ReadWrite,<BYTE,Internal Only>#
NV_C1_GPS_DACC_IACCUM4_I,998,ReadWrite,<BYTE,Internal Only>#
NV_C1_CDMA_DACC_QACCUM0_I,999,ReadWrite,<BYTE,Internal Only>#
NV_C1_PCS_DACC_QACCUM0_I,1000,ReadWrite,<BYTE,Internal Only>#
NV_C1_GPS_DACC_QACCUM0_I,1001,ReadWrite,<BYTE,Internal Only>#
NV_C1_CDMA_DACC_QACCUM1_I,1002,ReadWrite,<BYTE,Internal Only>#
NV_C1_PCS_DACC_QACCUM1_I,1003,ReadWrite,<BYTE,Internal Only>#
NV_C1_GPS_DACC_QACCUM1_I,1004,ReadWrite,<BYTE,Internal Only>#
NV_C1_CDMA_DACC_QACCUM2_I,1005,ReadWrite,<BYTE,Internal Only>#
NV_C1_PCS_DACC_QACCUM2_I,1006,ReadWrite,<BYTE,Internal Only>#
NV_C1_GPS_DACC_QACCUM2_I,1007,ReadWrite,<BYTE,Internal Only>#
NV_C1_CDMA_DACC_QACCUM3_I,1008,ReadWrite,<BYTE,Internal Only>#
NV_C1_PCS_DACC_QACCUM3_I,1009,ReadWrite,<BYTE,Internal Only>#
NV_C1_GPS_DACC_QACCUM3_I,1010,ReadWrite,<BYTE,Internal Only>#
NV_C1_CDMA_DACC_QACCUM4_I,1011,ReadWrite,<BYTE,Internal Only>#
NV_C1_PCS_DACC_QACCUM4_I,1012,ReadWrite,<BYTE,Internal Only>#
NV_C1_GPS_DACC_QACCUM4_I,1013,ReadWrite,<BYTE,Internal Only>#
NV_CDMA_RX_DIVERSITY_CTRL_I,1018,ReadWrite,<WORD,Diversity Overwrite Value>#
NV_C1_CDMA_IM2_Q_VALUE_I,1020,ReadWrite,<BYTE,Q Value>#
NV_C1_PCS_IM2_Q_VALUE_I,1021,ReadWrite,<BYTE,Q Value>#
NV_C1_CDMA_IM2_I_VALUE_I,1022,ReadWrite,<BYTE,I Value>#
NV_C1_PCS_IM2_I_VALUE_I,1023,ReadWrite,<BYTE,I Value>#
NV_C1_CDMA_IM2_TRANSCONDUCTOR_VALUE_I,1024,ReadWrite,<BYTE,Transconductor Value>#
NV_C1_PCS_IM2_TRANSCONDUCTOR_VALUE_I,1025,ReadWrite,<BYTE,Transconductor Value>#
NV_C1_CDMA_LNA_1_RISE_I,1033,ReadWrite,<BYTE,C1 CDMA LNA 1 rise>#
NV_C1_CDMA_LNA_1_FALL_I,1041,ReadWrite,<BYTE,C1 CDMA LNA 1 fall>#
NV_C1_PCS_LNA_1_RISE_I,1037,ReadWrite,<BYTE,C1 PCS LNA 1 rise>#
NV_C1_PCS_LNA_1_FALL_I,1045,ReadWrite,<BYTE,C1 PCS LNA 1 fall>#
NV_C1_CDMA_LNA_2_RISE_I,1034,ReadWrite,<BYTE,C1 CDMA LNA 2 rise>#
NV_C1_CDMA_LNA_2_FALL_I,1042,ReadWrite,<BYTE,C1 CDMA LNA 2 fall>#
NV_C1_PCS_LNA_2_RISE_I,1038,ReadWrite,<BYTE,C1 PCS LNA 2 rise>#
NV_C1_PCS_LNA_2_FALL_I,1046,ReadWrite,<BYTE,C1 PCS LNA 2 fall>#
NV_C1_CDMA_LNA_3_RISE_I,1035,ReadWrite,<BYTE,C1 CDMA LNA 3 rise>#
NV_C1_CDMA_LNA_3_FALL_I,1043,ReadWrite,<BYTE,C1 CDMA LNA 3 fall>#
NV_C1_PCS_LNA_3_RISE_I,1039,ReadWrite,<BYTE,C1 PCS LNA 3 rise>#
NV_C1_PCS_LNA_3_FALL_I,1047,ReadWrite,<BYTE,C1 PCS LNA 3 fall>#
NV_C1_CDMA_LNA_4_RISE_I,1036,ReadWrite,<BYTE,C1 CDMA LNA 4 rise>#
NV_C1_CDMA_LNA_4_FALL_I,1044,ReadWrite,<BYTE,C1 CDMA LNA 4 fall>#
NV_C1_PCS_LNA_4_RISE_I,1040,ReadWrite,<BYTE,C1 PCS LNA 4 rise>#
NV_C1_CDMA_IM_LEVEL1_I,1049,ReadWrite,<BYTE,C1 CDMA IM level 1>#
NV_C1_PCS_IM_LEVEL1_I,1053,ReadWrite,<BYTE,C1 PCS IM level1>#
NV_C1_CDMA_IM_LEVEL2_I,1050,ReadWrite,<BYTE,C1 CDMA IM level 2>#
NV_C1_PCS_IM_LEVEL2_I,1054,ReadWrite,<BYTE,C1 PCS IM level 2>#
NV_C1_CDMA_IM_LEVEL3_I,1051,ReadWrite,<BYTE,C1 CDMA IM level 3>#
NV_C1_PCS_IM_LEVEL3_I,1055,ReadWrite,<BYTE,C1 PCS IM level 3>#
NV_C1_CDMA_IM_LEVEL4_I,1052,ReadWrite,<BYTE,C1 CDMA IM level 4>#
NV_C1_PCS_IM_LEVEL4_I,1056,ReadWrite,<BYTE,C1 PCS IM level 4>#
NV_GSM_1900_CAL_ARFCN_I,1057,ReadWrite,<SIGNED_WORD,Array[0]>#<SIGNED_WORD,Array[1]>#<SIGNED_WORD,Array[2]>#<SIGNED_WORD,Array[3]>#<SIGNED_WORD,Array[4]>#<SIGNED_WORD,Array[5]>#<SIGNED_WORD,Array[6]>#<SIGNED_WORD,Array[7]>#<SIGNED_WORD,Array[8]>#<SIGNED_WORD,Array[9]>#<SIGNED_WORD,Array[10]>#<SIGNED_WORD,Array[11]>#<SIGNED_WORD,Array[12]>#<SIGNED_WORD,Array[13]>#<SIGNED_WORD,Array[14]>#<SIGNED_WORD,Array[15]>#
NV_GSM_1900_RX_GAIN_RANGE_1_FREQ_COMP_I,1058,ReadWrite,<SIGNED_WORD,Array[0]>#<SIGNED_WORD,Array[1]>#<SIGNED_WORD,Array[2]>#<SIGNED_WORD,Array[3]>#<SIGNED_WORD,Array[4]>#<SIGNED_WORD,Array[5]>#<SIGNED_WORD,Array[6]>#<SIGNED_WORD,Array[7]>#<SIGNED_WORD,Array[8]>#<SIGNED_WORD,Array[9]>#<SIGNED_WORD,Array[10]>#<SIGNED_WORD,Array[11]>#<SIGNED_WORD,Array[12]>#<SIGNED_WORD,Array[13]>#<SIGNED_WORD,Array[14]>#<SIGNED_WORD,Array[15]>#
NV_GSM_1900_RX_GAIN_RANGE_2_FREQ_COMP_I,1059,ReadWrite,<SIGNED_WORD,Array[0]>#<SIGNED_WORD,Array[1]>#<SIGNED_WORD,Array[2]>#<SIGNED_WORD,Array[3]>#<SIGNED_WORD,Array[4]>#<SIGNED_WORD,Array[5]>#<SIGNED_WORD,Array[6]>#<SIGNED_WORD,Array[7]>#<SIGNED_WORD,Array[8]>#<SIGNED_WORD,Array[9]>#<SIGNED_WORD,Array[10]>#<SIGNED_WORD,Array[11]>#<SIGNED_WORD,Array[12]>#<SIGNED_WORD,Array[13]>#<SIGNED_WORD,Array[14]>#<SIGNED_WORD,Array[15]>#
NV_GSM_1900_RX_GAIN_RANGE_3_FREQ_COMP_I,1060,ReadWrite,<SIGNED_WORD,Array[0]>#<SIGNED_WORD,Array[1]>#<SIGNED_WORD,Array[2]>#<SIGNED_WORD,Array[3]>#<SIGNED_WORD,Array[4]>#<SIGNED_WORD,Array[5]>#<SIGNED_WORD,Array[6]>#<SIGNED_WORD,Array[7]>#<SIGNED_WORD,Array[8]>#<SIGNED_WORD,Array[9]>#<SIGNED_WORD,Array[10]>#<SIGNED_WORD,Array[11]>#<SIGNED_WORD,Array[12]>#<SIGNED_WORD,Array[13]>#<SIGNED_WORD,Array[14]>#<SIGNED_WORD,Array[15]>#
NV_GSM_1900_RX_GAIN_RANGE_4_FREQ_COMP_I,1061,ReadWrite,<SIGNED_WORD,Array[0]>#<SIGNED_WORD,Array[1]>#<SIGNED_WORD,Array[2]>#<SIGNED_WORD,Array[3]>#<SIGNED_WORD,Array[4]>#<SIGNED_WORD,Array[5]>#<SIGNED_WORD,Array[6]>#<SIGNED_WORD,Array[7]>#<SIGNED_WORD,Array[8]>#<SIGNED_WORD,Array[9]>#<SIGNED_WORD,Array[10]>#<SIGNED_WORD,Array[11]>#<SIGNED_WORD,Array[12]>#<SIGNED_WORD,Array[13]>#<SIGNED_WORD,Array[14]>#<SIGNED_WORD,Array[15]>#
NV_GSM_1900_TX_BURST_RAMP_UP_INDEX_00_I,1062,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_1900_TX_BURST_RAMP_UP_INDEX_01_I,1063,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_1900_TX_BURST_RAMP_UP_INDEX_02_I,1064,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_1900_TX_BURST_RAMP_UP_INDEX_03_I,1065,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_1900_TX_BURST_RAMP_UP_INDEX_04_I,1066,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_1900_TX_BURST_RAMP_UP_INDEX_05_I,1067,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_1900_TX_BURST_RAMP_UP_INDEX_06_I,1068,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_1900_TX_BURST_RAMP_UP_INDEX_07_I,1069,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_1900_TX_BURST_RAMP_UP_INDEX_08_I,1070,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_1900_TX_BURST_RAMP_UP_INDEX_09_I,1071,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_1900_TX_BURST_RAMP_UP_INDEX_10_I,1072,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_1900_TX_BURST_RAMP_UP_INDEX_11_I,1073,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_1900_TX_BURST_RAMP_UP_INDEX_12_I,1074,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_1900_TX_BURST_RAMP_UP_INDEX_13_I,1075,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_1900_TX_BURST_RAMP_UP_INDEX_14_I,1076,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_1900_TX_BURST_RAMP_UP_INDEX_15_I,1077,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_1900_TX_BURST_RAMP_DOWN_INDEX_00_I,1078,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_1900_TX_BURST_RAMP_DOWN_INDEX_01_I,1079,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_1900_TX_BURST_RAMP_DOWN_INDEX_02_I,1080,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_1900_TX_BURST_RAMP_DOWN_INDEX_03_I,1081,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_1900_TX_BURST_RAMP_DOWN_INDEX_04_I,1082,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_1900_TX_BURST_RAMP_DOWN_INDEX_05_I,1083,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_1900_TX_BURST_RAMP_DOWN_INDEX_06_I,1084,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_1900_TX_BURST_RAMP_DOWN_INDEX_07_I,1085,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_1900_TX_BURST_RAMP_DOWN_INDEX_08_I,1086,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_1900_TX_BURST_RAMP_DOWN_INDEX_09_I,1087,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_1900_TX_BURST_RAMP_DOWN_INDEX_10_I,1088,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_1900_TX_BURST_RAMP_DOWN_INDEX_11_I,1089,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_1900_TX_BURST_RAMP_DOWN_INDEX_12_I,1090,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_1900_TX_BURST_RAMP_DOWN_INDEX_13_I,1091,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_1900_TX_BURST_RAMP_DOWN_INDEX_14_I,1092,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_1900_TX_BURST_RAMP_DOWN_INDEX_15_I,1093,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_1900_PA_GAIN_SLOPE_I,1094,ReadWrite,<BYTE,Array[0]>#<BYTE,Array[1]>#<BYTE,Array[2]>#<BYTE,Array[3]>#<BYTE,Array[4]>#<BYTE,Array[5]>#<BYTE,Array[6]>#<BYTE,Array[7]>#<BYTE,Array[8]>#<BYTE,Array[9]>#<BYTE,Array[10]>#<BYTE,Array[11]>#<BYTE,Array[12]>#<BYTE,Array[13]>#<BYTE,Array[14]>#<BYTE,Array[15]>#
NV_GSM_1900_TX_FREQ_COMP_I,1095,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_GSM_1900_VBATT_HI_PA_COMP_I,1096,ReadWrite,<BYTE,Hi PA comp>#
NV_GSM_1900_VBATT_LO_PA_COMP_I,1097,ReadWrite,<BYTE,Lo PA comp>#
NV_GSM_1900_PA_START_TIME_OFFSET_I,1098,ReadWrite,<SIGNED_BYTE,Start time offset>#
NV_GSM_1900_PA_STOP_TIME_OFFSET_I,1099,ReadWrite,<SIGNED_BYTE,Stop time offset>#
NV_GSM_1900_GAINRANGE_SWITCHPOINTS_I,1100,ReadWrite,<SIGNED_BYTE,Max Gain Range 1>#<SIGNED_BYTE,Min Gain Range 2>#<SIGNED_BYTE,Max Gain Range 2>#<SIGNED_BYTE,Min Gain Range 3>#<SIGNED_BYTE,Max Gain Range 3>#<SIGNED_BYTE,Min Gain Range 4>#
NV_GSM_850_CAL_ARFCN_I,1101,ReadWrite,<SIGNED_WORD,Array[0]>#<SIGNED_WORD,Array[1]>#<SIGNED_WORD,Array[2]>#<SIGNED_WORD,Array[3]>#<SIGNED_WORD,Array[4]>#<SIGNED_WORD,Array[5]>#<SIGNED_WORD,Array[6]>#<SIGNED_WORD,Array[7]>#
NV_GSM_850_RX_GAIN_RANGE_1_FREQ_COMP_I,1102,ReadWrite,<SIGNED_WORD,Array[0]>#<SIGNED_WORD,Array[1]>#<SIGNED_WORD,Array[2]>#<SIGNED_WORD,Array[3]>#<SIGNED_WORD,Array[4]>#<SIGNED_WORD,Array[5]>#<SIGNED_WORD,Array[6]>#<SIGNED_WORD,Array[7]>#
NV_GSM_850_RX_GAIN_RANGE_2_FREQ_COMP_I,1103,ReadWrite,<SIGNED_WORD,Array[0]>#<SIGNED_WORD,Array[1]>#<SIGNED_WORD,Array[2]>#<SIGNED_WORD,Array[3]>#<SIGNED_WORD,Array[4]>#<SIGNED_WORD,Array[5]>#<SIGNED_WORD,Array[6]>#<SIGNED_WORD,Array[7]>#
NV_GSM_850_RX_GAIN_RANGE_3_FREQ_COMP_I,1104,ReadWrite,<SIGNED_WORD,Array[0]>#<SIGNED_WORD,Array[1]>#<SIGNED_WORD,Array[2]>#<SIGNED_WORD,Array[3]>#<SIGNED_WORD,Array[4]>#<SIGNED_WORD,Array[5]>#<SIGNED_WORD,Array[6]>#<SIGNED_WORD,Array[7]>#
NV_GSM_850_RX_GAIN_RANGE_4_FREQ_COMP_I,1105,ReadWrite,<SIGNED_WORD,Array[0]>#<SIGNED_WORD,Array[1]>#<SIGNED_WORD,Array[2]>#<SIGNED_WORD,Array[3]>#<SIGNED_WORD,Array[4]>#<SIGNED_WORD,Array[5]>#<SIGNED_WORD,Array[6]>#<SIGNED_WORD,Array[7]>#
NV_GSM_850_TX_BURST_RAMP_UP_INDEX_00_I,1106,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_850_TX_BURST_RAMP_UP_INDEX_01_I,1107,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_850_TX_BURST_RAMP_UP_INDEX_02_I,1108,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_850_TX_BURST_RAMP_UP_INDEX_03_I,1109,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_850_TX_BURST_RAMP_UP_INDEX_04_I,1110,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_850_TX_BURST_RAMP_UP_INDEX_05_I,1111,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_850_TX_BURST_RAMP_UP_INDEX_06_I,1112,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_850_TX_BURST_RAMP_UP_INDEX_07_I,1113,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_850_TX_BURST_RAMP_UP_INDEX_08_I,1114,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_850_TX_BURST_RAMP_UP_INDEX_09_I,1115,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_850_TX_BURST_RAMP_UP_INDEX_10_I,1116,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_850_TX_BURST_RAMP_UP_INDEX_11_I,1117,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_850_TX_BURST_RAMP_UP_INDEX_12_I,1118,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_850_TX_BURST_RAMP_UP_INDEX_13_I,1119,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_850_TX_BURST_RAMP_UP_INDEX_14_I,1120,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_850_TX_BURST_RAMP_DOWN_INDEX_00_I,1121,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_850_TX_BURST_RAMP_DOWN_INDEX_01_I,1122,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_850_TX_BURST_RAMP_DOWN_INDEX_02_I,1123,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_850_TX_BURST_RAMP_DOWN_INDEX_03_I,1124,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_850_TX_BURST_RAMP_DOWN_INDEX_04_I,1125,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_850_TX_BURST_RAMP_DOWN_INDEX_05_I,1126,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_850_TX_BURST_RAMP_DOWN_INDEX_06_I,1127,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_850_TX_BURST_RAMP_DOWN_INDEX_07_I,1128,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_850_TX_BURST_RAMP_DOWN_INDEX_08_I,1129,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_850_TX_BURST_RAMP_DOWN_INDEX_09_I,1130,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_850_TX_BURST_RAMP_DOWN_INDEX_10_I,1131,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_850_TX_BURST_RAMP_DOWN_INDEX_11_I,1132,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_850_TX_BURST_RAMP_DOWN_INDEX_12_I,1133,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_850_TX_BURST_RAMP_DOWN_INDEX_13_I,1134,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_850_TX_BURST_RAMP_DOWN_INDEX_14_I,1135,ReadWrite,<WORD,Value[0]>#<WORD,Value[1]>#<WORD,Value[2]>#<WORD,Value[3]>#<WORD,Value[4]>#<WORD,Value[5]>#<WORD,Value[6]>#<WORD,Value[7]>#<WORD,Value[8]>#<WORD,Value[9]>#<WORD,Value[10]>#<WORD,Value[11]>#<WORD,Value[12]>#<WORD,Value[13]>#<WORD,Value[14]>#<WORD,Value[15]>#<WORD,Value[16]>#<WORD,Value[17]>#<WORD,Value[18]>#<WORD,Value[19]>#<WORD,Value[20]>#<WORD,Value[21]>#<WORD,Value[22]>#<WORD,Value[23]>#<WORD,Value[24]>#<WORD,Value[25]>#<WORD,Value[26]>#<WORD,Value[27]>#<WORD,Value[28]>#<WORD,Value[29]>#
NV_GSM_850_PA_GAIN_SLOPE_I,1136,ReadWrite,<BYTE,Array[0]>#<BYTE,Array[1]>#<BYTE,Array[2]>#<BYTE,Array[3]>#<BYTE,Array[4]>#<BYTE,Array[5]>#<BYTE,Array[6]>#<BYTE,Array[7]>#<BYTE,Array[8]>#<BYTE,Array[9]>#<BYTE,Array[10]>#<BYTE,Array[11]>#<BYTE,Array[12]>#<BYTE,Array[13]>#<BYTE,Array[14]>#
NV_GSM_850_TX_FREQ_COMP_I,1137,ReadWrite,<SIGNED_BYTE,Value[0]>#<SIGNED_BYTE,Value[1]>#<SIGNED_BYTE,Value[2]>#<SIGNED_BYTE,Value[3]>#<SIGNED_BYTE,Value[4]>#<SIGNED_BYTE,Value[5]>#<SIGNED_BYTE,Value[6]>#<SIGNED_BYTE,Value[7]>#
NV_GSM_850_VBATT_HI_PA_COMP_I,1138,ReadWrite,<BYTE,Hi PA comp>#
NV_GSM_850_VBATT_LO_PA_COMP_I,1139,ReadWrite,<BYTE,Lo PA comp>#
NV_GSM_850_PA_START_TIME_OFFSET_I,1140,ReadWrite,<SIGNED_BYTE,Start time offset>#
NV_GSM_850_PA_STOP_TIME_OFFSET_I,1141,ReadWrite,<SIGNED_BYTE,Stop time offset>#
NV_GSM_850_GAINRANGE_SWITCHPOINTS_I,1142,ReadWrite,<SIGNED_BYTE,Max Gain Range 1>#<SIGNED_BYTE,Min Gain Range 2>#<SIGNED_BYTE,Max Gain Range 2>#<SIGNED_BYTE,Min Gain Range 3>#<SIGNED_BYTE,Max Gain Range 3>#<SIGNED_BYTE,Min Gain Range 4>#
NV_WCDMA_1900_VGA_GAIN_OFFSET_I,1143,ReadWrite,<SIGNED_WORD,Offset>#
NV_WCDMA_1900_VGA_GAIN_OFFSET_VS_FREQ_I,1144,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_WCDMA_1900_VGA_GAIN_OFFSET_VS_TEMP_I,1145,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_WCDMA_1900_LNA_RANGE_RISE_2_I,1146,ReadWrite,<SIGNED_WORD,LNA range rise 2>#
NV_WCDMA_1900_LNA_RANGE_RISE_3_I,1147,ReadWrite,<SIGNED_WORD,LNA range rise 3>#
NV_WCDMA_1900_LNA_RANGE_FALL_2_I,1148,ReadWrite,<SIGNED_WORD,LNA range fall 2>#
NV_WCDMA_1900_LNA_RANGE_FALL_3_I,1149,ReadWrite,<SIGNED_WORD,LNA range fall 3>#
NV_WCDMA_1900_IM_LEVEL_2_I,1150,ReadWrite,<SIGNED_WORD,IM level 2>#
NV_WCDMA_1900_IM_LEVEL_3_I,1151,ReadWrite,<SIGNED_WORD,IM level 3>#
NV_WCDMA_1900_LNA_RANGE_OFFSET_2_I,1152,ReadWrite,<SIGNED_WORD,Offset>#
NV_WCDMA_1900_LNA_RANGE_OFFSET_3_I,1153,ReadWrite,<SIGNED_WORD,Offset>#
NV_WCDMA_1900_LNA_OFFSET_VS_FREQ_2_I,1154,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_WCDMA_1900_LNA_OFFSET_VS_FREQ_3_I,1155,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_WCDMA_1900_IM2_I_VALUE_I,1156,ReadWrite,<BYTE,IM2 I value>#
NV_WCDMA_1900_IM2_Q_VALUE_I,1157,ReadWrite,<BYTE,IM2 Q value>#
NV_WCDMA_1900_IM2_TRANSCONDUCTOR_VALUE_I,1158,ReadWrite,<BYTE,Transconductor value>#
NV_WCDMA_1900_RX_AGC_MIN_2_I,1159,ReadWrite,<SIGNED_WORD,Rx AGC min 2>#
NV_WCDMA_1900_RX_AGC_MIN_3_I,1160,ReadWrite,<SIGNED_WORD,Rx AGC min 3>#
NV_WCDMA_1900_MAX_TX_POWER_I,1161,ReadWrite,<SIGNED_BYTE,Tx Power>#
NV_WCDMA_1900_OUT_OF_SERVICE_THRESH_I,1162,ReadWrite,<SIGNED_WORD,Out of service thresh>#
NV_WCDMA_1900_LNA_RANGE_RISE_I,1163,ReadWrite,<SIGNED_WORD,LNA range rise>#
NV_WCDMA_1900_LNA_RANGE_FALL_I,1164,ReadWrite,<SIGNED_WORD,LNA range fall>#
NV_WCDMA_1900_IM_LEVEL_I,1165,ReadWrite,<SIGNED_WORD,IM level>#
NV_WCDMA_1900_NONBYPASS_TIMER_I,1166,ReadWrite,<BYTE,Nonbypass timer>#
NV_WCDMA_1900_BYPASS_TIMER_I,1167,ReadWrite,<WORD,Bypass timer>#
NV_WCDMA_1900_LNA_RANGE_OFFSET_I,1168,ReadWrite,<SIGNED_WORD,LNA range offset>#
NV_WCDMA_1900_LNA_OFFSET_VS_FREQ_I,1169,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_WCDMA_1900_RX_AGC_MIN_I,1170,ReadWrite,<SIGNED_WORD,Rx AGC min>#
NV_WCDMA_1900_RX_AGC_MAX_I,1171,ReadWrite,<SIGNED_WORD,Rx AGC max>#
NV_WCDMA_1900_AGC_PHASE_OFFSET_I,1172,ReadWrite,<BYTE,Phase offset>#
NV_WCDMA_1900_TX_LIN_MASTER_0_I,1173,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#<WORD,Array[30]>#<WORD,Array[31]>#<WORD,Array[32]>#<WORD,Array[33]>#<WORD,Array[34]>#<WORD,Array[35]>#<WORD,Array[36]>#
NV_WCDMA_1900_TX_LIN_MASTER_1_I,1174,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#<WORD,Array[30]>#<WORD,Array[31]>#<WORD,Array[32]>#<WORD,Array[33]>#<WORD,Array[34]>#<WORD,Array[35]>#<WORD,Array[36]>#
NV_WCDMA_1900_TX_COMP_VS_FREQ_0_I,1175,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_WCDMA_1900_TX_COMP_VS_FREQ_1_I,1176,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_WCDMA_1900_TX_LIN_VS_TEMP_0_I,1177,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#
NV_WCDMA_1900_TX_LIN_VS_TEMP_1_I,1178,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#
NV_WCDMA_1900_TX_SLP_VS_TEMP_0_I,1179,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#
NV_WCDMA_1900_TX_SLP_VS_TEMP_1_I,1180,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#
NV_WCDMA_1900_R1_RISE_I,1181,ReadWrite,<WORD,Rise>#
NV_WCDMA_1900_R1_FALL_I,1182,ReadWrite,<WORD,Fall>#
NV_WCDMA_1900_TX_LIM_VS_TEMP_I,1183,ReadWrite,<BYTE,Array[0]>#<BYTE,Array[1]>#<BYTE,Array[2]>#<BYTE,Array[3]>#<BYTE,Array[4]>#<BYTE,Array[5]>#<BYTE,Array[6]>#<BYTE,Array[7]>#
NV_WCDMA_1900_TX_LIM_VS_FREQ_I,1184,ReadWrite,<SIGNED_WORD,Array[0]>#<SIGNED_WORD,Array[1]>#<SIGNED_WORD,Array[2]>#<SIGNED_WORD,Array[3]>#<SIGNED_WORD,Array[4]>#<SIGNED_WORD,Array[5]>#<SIGNED_WORD,Array[6]>#<SIGNED_WORD,Array[7]>#<SIGNED_WORD,Array[8]>#<SIGNED_WORD,Array[9]>#<SIGNED_WORD,Array[10]>#<SIGNED_WORD,Array[11]>#<SIGNED_WORD,Array[12]>#<SIGNED_WORD,Array[13]>#<SIGNED_WORD,Array[14]>#<SIGNED_WORD,Array[15]>#
NV_WCDMA_1900_ADJ_FACTOR_I,1185,ReadWrite,<BYTE,Adj factor>#
NV_WCDMA_1900_EXP_HDET_VS_AGC_I,1186,ReadWrite,<BYTE,Array[0]>#<BYTE,Array[1]>#<BYTE,Array[2]>#<BYTE,Array[3]>#<BYTE,Array[4]>#<BYTE,Array[5]>#<BYTE,Array[6]>#<BYTE,Array[7]>#<BYTE,Array[8]>#<BYTE,Array[9]>#<BYTE,Array[10]>#<BYTE,Array[11]>#<BYTE,Array[12]>#<BYTE,Array[13]>#<BYTE,Array[14]>#<BYTE,Array[15]>#
NV_WCDMA_1900_HDET_OFF_I,1187,ReadWrite,<BYTE,HDET off>#
NV_WCDMA_1900_HDET_SPN_I,1188,ReadWrite,<BYTE,HDET spn>#
NV_WCDMA_1900_ENC_BTF_I,1189,ReadWrite,<DWORD,Value>#
NV_GSM_GAINRANGE_SWITCHPOINTS_I,916,ReadWrite,<SIGNED_BYTE,Max Gain Range 1>#<SIGNED_BYTE,Min Gain Range 2>#<SIGNED_BYTE,Max Gain Range 2>#<SIGNED_BYTE,Min Gain Range 3>#<SIGNED_BYTE,Max Gain Range 3>#<SIGNED_BYTE,Min Gain Range 4>#
NV_DCS_GAINRANGE_SWITCHPOINTS_I,917,ReadWrite,<SIGNED_BYTE,Max Gain Range 1>#<SIGNED_BYTE,Min Gain Range 2>#<SIGNED_BYTE,Max Gain Range 2>#<SIGNED_BYTE,Min Gain Range 3>#<SIGNED_BYTE,Max Gain Range 3>#<SIGNED_BYTE,Min Gain Range 4>#
NV_C1_PCS_LNA_4_FALL_I,1048,ReadWrite,<BYTE,Fall value>#
NV_RRC_FAKE_SECURITY_ENABLED_I,882,ReadWrite,<BYTE,Enable>#
NV_PWR_BACKOFF_VS_VOLT_MED_I,490,ReadWrite,<BYTE,Array[0]>#<BYTE,Array[1]>#<BYTE,Array[2]>#<BYTE,Array[3]>#<BYTE,Array[4]>#<BYTE,Array[5]>#<BYTE,Array[6]>#<BYTE,Array[7]>#<BYTE,Array[8]>#<BYTE,Array[9]>#<BYTE,Array[10]>#<BYTE,Array[11]>#<BYTE,Array[12]>#<BYTE,Array[13]>#<BYTE,Array[14]>#<BYTE,Array[15]>#<BYTE,Array[16]>#<BYTE,Array[17]>#<BYTE,Array[18]>#<BYTE,Array[19]>#
NV_PWR_BACKOFF_VS_VOLT_LOW_I,491,ReadWrite,<BYTE,Array[0]>#<BYTE,Array[1]>#<BYTE,Array[2]>#<BYTE,Array[3]>#<BYTE,Array[4]>#<BYTE,Array[5]>#<BYTE,Array[6]>#<BYTE,Array[7]>#<BYTE,Array[8]>#<BYTE,Array[9]>#<BYTE,Array[10]>#<BYTE,Array[11]>#<BYTE,Array[12]>#<BYTE,Array[13]>#<BYTE,Array[14]>#<BYTE,Array[15]>#<BYTE,Array[16]>#<BYTE,Array[17]>#<BYTE,Array[18]>#<BYTE,Array[19]>#
NV_PA_BACKOFF_VOLTS_I,492,ReadWrite,<BYTE,Array[0]>#<BYTE,Array[1]>#<BYTE,Array[2]>#
NV_VBATT_MIN_MAX_I,493,ReadWrite,<BYTE,Minimum>#<BYTE,Maximum>#
NV_GSM_PA_TEMP_COMP_INDEX_0_I,1273,ReadWrite,<SIGNED_BYTE,PA Temp CMP Index[0]>#<SIGNED_BYTE,PA Temp CMP Index [1]>#<SIGNED_BYTE,PA Temp CMP Index [2]>#<SIGNED_BYTE,PA Temp CMP Index [3]>#<SIGNED_BYTE,PA Temp CMP Index [4]>#<SIGNED_BYTE,PA Temp CMP Index [5]>#<SIGNED_BYTE,PA Temp CMP Index [6]>#<SIGNED_BYTE,PA Temp CMP Index [7]>#<SIGNED_BYTE,PA Temp CMP Index [8]>#<SIGNED_BYTE,PA Temp CMP Index [9]>#<SIGNED_BYTE,PA Temp CMP Index [10]>#<SIGNED_BYTE,PA Temp CMP Index [11]>#<SIGNED_BYTE,PA Temp CMP Index [12]>#<SIGNED_BYTE,PA Temp CMP Index [13]>#<SIGNED_BYTE,PA Temp CMP Index [14]>#<SIGNED_BYTE,PA Temp CMP Index [15]>#
NV_GSM_PA_TEMP_COMP_INDEX_1_I,1274,ReadWrite,<SIGNED_BYTE,PA Temp CMP Index[0]>#<SIGNED_BYTE,PA Temp CMP Index [1]>#<SIGNED_BYTE,PA Temp CMP Index [2]>#<SIGNED_BYTE,PA Temp CMP Index [3]>#<SIGNED_BYTE,PA Temp CMP Index [4]>#<SIGNED_BYTE,PA Temp CMP Index [5]>#<SIGNED_BYTE,PA Temp CMP Index [6]>#<SIGNED_BYTE,PA Temp CMP Index [7]>#<SIGNED_BYTE,PA Temp CMP Index [8]>#<SIGNED_BYTE,PA Temp CMP Index [9]>#<SIGNED_BYTE,PA Temp CMP Index [10]>#<SIGNED_BYTE,PA Temp CMP Index [11]>#<SIGNED_BYTE,PA Temp CMP Index [12]>#<SIGNED_BYTE,PA Temp CMP Index [13]>#<SIGNED_BYTE,PA Temp CMP Index [14]>#<SIGNED_BYTE,PA Temp CMP Index [15]>#
NV_GSM_PA_TEMP_COMP_INDEX_2_I,1275,ReadWrite,<SIGNED_BYTE,PA Temp CMP Index[0]>#<SIGNED_BYTE,PA Temp CMP Index [1]>#<SIGNED_BYTE,PA Temp CMP Index [2]>#<SIGNED_BYTE,PA Temp CMP Index [3]>#<SIGNED_BYTE,PA Temp CMP Index [4]>#<SIGNED_BYTE,PA Temp CMP Index [5]>#<SIGNED_BYTE,PA Temp CMP Index [6]>#<SIGNED_BYTE,PA Temp CMP Index [7]>#<SIGNED_BYTE,PA Temp CMP Index [8]>#<SIGNED_BYTE,PA Temp CMP Index [9]>#<SIGNED_BYTE,PA Temp CMP Index [10]>#<SIGNED_BYTE,PA Temp CMP Index [11]>#<SIGNED_BYTE,PA Temp CMP Index [12]>#<SIGNED_BYTE,PA Temp CMP Index [13]>#<SIGNED_BYTE,PA Temp CMP Index [14]>#<SIGNED_BYTE,PA Temp CMP Index [15]>#
NV_GSM_PA_TEMP_COMP_INDEX_3_I,1276,ReadWrite,<SIGNED_BYTE,PA Temp CMP Index[0]>#<SIGNED_BYTE,PA Temp CMP Index [1]>#<SIGNED_BYTE,PA Temp CMP Index [2]>#<SIGNED_BYTE,PA Temp CMP Index [3]>#<SIGNED_BYTE,PA Temp CMP Index [4]>#<SIGNED_BYTE,PA Temp CMP Index [5]>#<SIGNED_BYTE,PA Temp CMP Index [6]>#<SIGNED_BYTE,PA Temp CMP Index [7]>#<SIGNED_BYTE,PA Temp CMP Index [8]>#<SIGNED_BYTE,PA Temp CMP Index [9]>#<SIGNED_BYTE,PA Temp CMP Index [10]>#<SIGNED_BYTE,PA Temp CMP Index [11]>#<SIGNED_BYTE,PA Temp CMP Index [12]>#<SIGNED_BYTE,PA Temp CMP Index [13]>#<SIGNED_BYTE,PA Temp CMP Index [14]>#<SIGNED_BYTE,PA Temp CMP Index [15]>#
NV_GSM_PA_TEMP_COMP_INDEX_4_I,1277,ReadWrite,<SIGNED_BYTE,PA Temp CMP Index[0]>#<SIGNED_BYTE,PA Temp CMP Index [1]>#<SIGNED_BYTE,PA Temp CMP Index [2]>#<SIGNED_BYTE,PA Temp CMP Index [3]>#<SIGNED_BYTE,PA Temp CMP Index [4]>#<SIGNED_BYTE,PA Temp CMP Index [5]>#<SIGNED_BYTE,PA Temp CMP Index [6]>#<SIGNED_BYTE,PA Temp CMP Index [7]>#<SIGNED_BYTE,PA Temp CMP Index [8]>#<SIGNED_BYTE,PA Temp CMP Index [9]>#<SIGNED_BYTE,PA Temp CMP Index [10]>#<SIGNED_BYTE,PA Temp CMP Index [11]>#<SIGNED_BYTE,PA Temp CMP Index [12]>#<SIGNED_BYTE,PA Temp CMP Index [13]>#<SIGNED_BYTE,PA Temp CMP Index [14]>#<SIGNED_BYTE,PA Temp CMP Index [15]>#
NV_GSM_PA_TEMP_COMP_INDEX_5_I,1278,ReadWrite,<SIGNED_BYTE,PA Temp CMP Index[0]>#<SIGNED_BYTE,PA Temp CMP Index [1]>#<SIGNED_BYTE,PA Temp CMP Index [2]>#<SIGNED_BYTE,PA Temp CMP Index [3]>#<SIGNED_BYTE,PA Temp CMP Index [4]>#<SIGNED_BYTE,PA Temp CMP Index [5]>#<SIGNED_BYTE,PA Temp CMP Index [6]>#<SIGNED_BYTE,PA Temp CMP Index [7]>#<SIGNED_BYTE,PA Temp CMP Index [8]>#<SIGNED_BYTE,PA Temp CMP Index [9]>#<SIGNED_BYTE,PA Temp CMP Index [10]>#<SIGNED_BYTE,PA Temp CMP Index [11]>#<SIGNED_BYTE,PA Temp CMP Index [12]>#<SIGNED_BYTE,PA Temp CMP Index [13]>#<SIGNED_BYTE,PA Temp CMP Index [14]>#<SIGNED_BYTE,PA Temp CMP Index [15]>#
NV_GSM_PA_TEMP_COMP_INDEX_6_I,1279,ReadWrite,<SIGNED_BYTE,PA Temp CMP Index[0]>#<SIGNED_BYTE,PA Temp CMP Index [1]>#<SIGNED_BYTE,PA Temp CMP Index [2]>#<SIGNED_BYTE,PA Temp CMP Index [3]>#<SIGNED_BYTE,PA Temp CMP Index [4]>#<SIGNED_BYTE,PA Temp CMP Index [5]>#<SIGNED_BYTE,PA Temp CMP Index [6]>#<SIGNED_BYTE,PA Temp CMP Index [7]>#<SIGNED_BYTE,PA Temp CMP Index [8]>#<SIGNED_BYTE,PA Temp CMP Index [9]>#<SIGNED_BYTE,PA Temp CMP Index [10]>#<SIGNED_BYTE,PA Temp CMP Index [11]>#<SIGNED_BYTE,PA Temp CMP Index [12]>#<SIGNED_BYTE,PA Temp CMP Index [13]>#<SIGNED_BYTE,PA Temp CMP Index [14]>#<SIGNED_BYTE,PA Temp CMP Index [15]>#
NV_GSM_PA_TEMP_COMP_INDEX_7_I,1280,ReadWrite,<SIGNED_BYTE,PA Temp CMP Index[0]>#<SIGNED_BYTE,PA Temp CMP Index [1]>#<SIGNED_BYTE,PA Temp CMP Index [2]>#<SIGNED_BYTE,PA Temp CMP Index [3]>#<SIGNED_BYTE,PA Temp CMP Index [4]>#<SIGNED_BYTE,PA Temp CMP Index [5]>#<SIGNED_BYTE,PA Temp CMP Index [6]>#<SIGNED_BYTE,PA Temp CMP Index [7]>#<SIGNED_BYTE,PA Temp CMP Index [8]>#<SIGNED_BYTE,PA Temp CMP Index [9]>#<SIGNED_BYTE,PA Temp CMP Index [10]>#<SIGNED_BYTE,PA Temp CMP Index [11]>#<SIGNED_BYTE,PA Temp CMP Index [12]>#<SIGNED_BYTE,PA Temp CMP Index [13]>#<SIGNED_BYTE,PA Temp CMP Index [14]>#<SIGNED_BYTE,PA Temp CMP Index [15]>#
NV_GSM_PA_TEMP_COMP_INDEX_8_I,1281,ReadWrite,<SIGNED_BYTE,PA Temp CMP Index[0]>#<SIGNED_BYTE,PA Temp CMP Index [1]>#<SIGNED_BYTE,PA Temp CMP Index [2]>#<SIGNED_BYTE,PA Temp CMP Index [3]>#<SIGNED_BYTE,PA Temp CMP Index [4]>#<SIGNED_BYTE,PA Temp CMP Index [5]>#<SIGNED_BYTE,PA Temp CMP Index [6]>#<SIGNED_BYTE,PA Temp CMP Index [7]>#<SIGNED_BYTE,PA Temp CMP Index [8]>#<SIGNED_BYTE,PA Temp CMP Index [9]>#<SIGNED_BYTE,PA Temp CMP Index [10]>#<SIGNED_BYTE,PA Temp CMP Index [11]>#<SIGNED_BYTE,PA Temp CMP Index [12]>#<SIGNED_BYTE,PA Temp CMP Index [13]>#<SIGNED_BYTE,PA Temp CMP Index [14]>#<SIGNED_BYTE,PA Temp CMP Index [15]>#
NV_GSM_PA_TEMP_COMP_INDEX_9_I,1282,ReadWrite,<SIGNED_BYTE,PA Temp CMP Index[0]>#<SIGNED_BYTE,PA Temp CMP Index [1]>#<SIGNED_BYTE,PA Temp CMP Index [2]>#<SIGNED_BYTE,PA Temp CMP Index [3]>#<SIGNED_BYTE,PA Temp CMP Index [4]>#<SIGNED_BYTE,PA Temp CMP Index [5]>#<SIGNED_BYTE,PA Temp CMP Index [6]>#<SIGNED_BYTE,PA Temp CMP Index [7]>#<SIGNED_BYTE,PA Temp CMP Index [8]>#<SIGNED_BYTE,PA Temp CMP Index [9]>#<SIGNED_BYTE,PA Temp CMP Index [10]>#<SIGNED_BYTE,PA Temp CMP Index [11]>#<SIGNED_BYTE,PA Temp CMP Index [12]>#<SIGNED_BYTE,PA Temp CMP Index [13]>#<SIGNED_BYTE,PA Temp CMP Index [14]>#<SIGNED_BYTE,PA Temp CMP Index [15]>#
NV_GSM_PA_TEMP_COMP_INDEX_10_I,1283,ReadWrite,<SIGNED_BYTE,PA Temp CMP Index[0]>#<SIGNED_BYTE,PA Temp CMP Index [1]>#<SIGNED_BYTE,PA Temp CMP Index [2]>#<SIGNED_BYTE,PA Temp CMP Index [3]>#<SIGNED_BYTE,PA Temp CMP Index [4]>#<SIGNED_BYTE,PA Temp CMP Index [5]>#<SIGNED_BYTE,PA Temp CMP Index [6]>#<SIGNED_BYTE,PA Temp CMP Index [7]>#<SIGNED_BYTE,PA Temp CMP Index [8]>#<SIGNED_BYTE,PA Temp CMP Index [9]>#<SIGNED_BYTE,PA Temp CMP Index [10]>#<SIGNED_BYTE,PA Temp CMP Index [11]>#<SIGNED_BYTE,PA Temp CMP Index [12]>#<SIGNED_BYTE,PA Temp CMP Index [13]>#<SIGNED_BYTE,PA Temp CMP Index [14]>#<SIGNED_BYTE,PA Temp CMP Index [15]>#
NV_GSM_PA_TEMP_COMP_INDEX_11_I,1284,ReadWrite,<SIGNED_BYTE,PA Temp CMP Index[0]>#<SIGNED_BYTE,PA Temp CMP Index [1]>#<SIGNED_BYTE,PA Temp CMP Index [2]>#<SIGNED_BYTE,PA Temp CMP Index [3]>#<SIGNED_BYTE,PA Temp CMP Index [4]>#<SIGNED_BYTE,PA Temp CMP Index [5]>#<SIGNED_BYTE,PA Temp CMP Index [6]>#<SIGNED_BYTE,PA Temp CMP Index [7]>#<SIGNED_BYTE,PA Temp CMP Index [8]>#<SIGNED_BYTE,PA Temp CMP Index [9]>#<SIGNED_BYTE,PA Temp CMP Index [10]>#<SIGNED_BYTE,PA Temp CMP Index [11]>#<SIGNED_BYTE,PA Temp CMP Index [12]>#<SIGNED_BYTE,PA Temp CMP Index [13]>#<SIGNED_BYTE,PA Temp CMP Index [14]>#<SIGNED_BYTE,PA Temp CMP Index [15]>#
NV_GSM_PA_TEMP_COMP_INDEX_12_I,1285,ReadWrite,<SIGNED_BYTE,PA Temp CMP Index[0]>#<SIGNED_BYTE,PA Temp CMP Index [1]>#<SIGNED_BYTE,PA Temp CMP Index [2]>#<SIGNED_BYTE,PA Temp CMP Index [3]>#<SIGNED_BYTE,PA Temp CMP Index [4]>#<SIGNED_BYTE,PA Temp CMP Index [5]>#<SIGNED_BYTE,PA Temp CMP Index [6]>#<SIGNED_BYTE,PA Temp CMP Index [7]>#<SIGNED_BYTE,PA Temp CMP Index [8]>#<SIGNED_BYTE,PA Temp CMP Index [9]>#<SIGNED_BYTE,PA Temp CMP Index [10]>#<SIGNED_BYTE,PA Temp CMP Index [11]>#<SIGNED_BYTE,PA Temp CMP Index [12]>#<SIGNED_BYTE,PA Temp CMP Index [13]>#<SIGNED_BYTE,PA Temp CMP Index [14]>#<SIGNED_BYTE,PA Temp CMP Index [15]>#
NV_GSM_PA_TEMP_COMP_INDEX_13_I,1286,ReadWrite,<SIGNED_BYTE,PA Temp CMP Index[0]>#<SIGNED_BYTE,PA Temp CMP Index [1]>#<SIGNED_BYTE,PA Temp CMP Index [2]>#<SIGNED_BYTE,PA Temp CMP Index [3]>#<SIGNED_BYTE,PA Temp CMP Index [4]>#<SIGNED_BYTE,PA Temp CMP Index [5]>#<SIGNED_BYTE,PA Temp CMP Index [6]>#<SIGNED_BYTE,PA Temp CMP Index [7]>#<SIGNED_BYTE,PA Temp CMP Index [8]>#<SIGNED_BYTE,PA Temp CMP Index [9]>#<SIGNED_BYTE,PA Temp CMP Index [10]>#<SIGNED_BYTE,PA Temp CMP Index [11]>#<SIGNED_BYTE,PA Temp CMP Index [12]>#<SIGNED_BYTE,PA Temp CMP Index [13]>#<SIGNED_BYTE,PA Temp CMP Index [14]>#<SIGNED_BYTE,PA Temp CMP Index [15]>#
NV_GSM_PA_TEMP_COMP_INDEX_14_I,934,ReadWrite,<SIGNED_WORD,PA Temp CMP Index[0]>#<SIGNED_WORD,PA Temp CMP Index [1]>#<SIGNED_WORD,PA Temp CMP Index [2]>#<SIGNED_WORD,PA Temp CMP Index [3]>#<SIGNED_WORD,PA Temp CMP Index [4]>#<SIGNED_WORD,PA Temp CMP Index [5]>#<SIGNED_WORD,PA Temp CMP Index [6]>#<SIGNED_WORD,PA Temp CMP Index [7]>#<SIGNED_WORD,PA Temp CMP Index [8]>#<SIGNED_WORD,PA Temp CMP Index [9]>#<SIGNED_WORD,PA Temp CMP Index [10]>#<SIGNED_WORD,PA Temp CMP Index [11]>#<SIGNED_WORD,PA Temp CMP Index [12]>#<SIGNED_WORD,PA Temp CMP Index [13]>#<SIGNED_WORD,PA Temp CMP Index [14]>#<SIGNED_WORD,PA Temp CMP Index [15]>#
NV_GSM_PA_TEMP_COMP_INT8_INDEX_14_I,1303,ReadWrite,<SIGNED_BYTE,PA Temp CMP Index 14[0]>#<SIGNED_BYTE,PA Temp CMP Index 14[1]>#<SIGNED_BYTE,PA Temp CMP Index 14[2]>#<SIGNED_BYTE,PA Temp CMP Index 14[3]>#<SIGNED_BYTE,PA Temp CMP Index 14[4]>#<SIGNED_BYTE,PA Temp CMP Index 14[5]>#<SIGNED_BYTE,PA Temp CMP Index 14[6]>#<SIGNED_BYTE,PA Temp CMP Index 14[7]>#<SIGNED_BYTE,PA Temp CMP Index 14[8]>#<SIGNED_BYTE,PA Temp CMP Index 14[9]>#<SIGNED_BYTE,PA Temp CMP Index 14[10]>#<SIGNED_BYTE,PA Temp CMP Index 14[11]>#<SIGNED_BYTE,PA Temp CMP Index 14[12]>#<SIGNED_BYTE,PA Temp CMP Index 14[13]>#<SIGNED_BYTE,PA Temp CMP Index 14[14]>#<SIGNED_BYTE,PA Temp CMP Index 14[15]>#
NV_DCS_PA_TEMP_COMP_INDEX_0_I,1287,ReadWrite,<SIGNED_BYTE,PA Temp CMP Index[0]>#<SIGNED_BYTE,PA Temp CMP Index [1]>#<SIGNED_BYTE,PA Temp CMP Index [2]>#<SIGNED_BYTE,PA Temp CMP Index [3]>#<SIGNED_BYTE,PA Temp CMP Index [4]>#<SIGNED_BYTE,PA Temp CMP Index [5]>#<SIGNED_BYTE,PA Temp CMP Index [6]>#<SIGNED_BYTE,PA Temp CMP Index [7]>#<SIGNED_BYTE,PA Temp CMP Index [8]>#<SIGNED_BYTE,PA Temp CMP Index [9]>#<SIGNED_BYTE,PA Temp CMP Index [10]>#<SIGNED_BYTE,PA Temp CMP Index [11]>#<SIGNED_BYTE,PA Temp CMP Index [12]>#<SIGNED_BYTE,PA Temp CMP Index [13]>#<SIGNED_BYTE,PA Temp CMP Index [14]>#<SIGNED_BYTE,PA Temp CMP Index [15]>#
NV_DCS_PA_TEMP_COMP_INDEX_1_I,1288,ReadWrite,<SIGNED_BYTE,PA Temp CMP Index[0]>#<SIGNED_BYTE,PA Temp CMP Index [1]>#<SIGNED_BYTE,PA Temp CMP Index [2]>#<SIGNED_BYTE,PA Temp CMP Index [3]>#<SIGNED_BYTE,PA Temp CMP Index [4]>#<SIGNED_BYTE,PA Temp CMP Index [5]>#<SIGNED_BYTE,PA Temp CMP Index [6]>#<SIGNED_BYTE,PA Temp CMP Index [7]>#<SIGNED_BYTE,PA Temp CMP Index [8]>#<SIGNED_BYTE,PA Temp CMP Index [9]>#<SIGNED_BYTE,PA Temp CMP Index [10]>#<SIGNED_BYTE,PA Temp CMP Index [11]>#<SIGNED_BYTE,PA Temp CMP Index [12]>#<SIGNED_BYTE,PA Temp CMP Index [13]>#<SIGNED_BYTE,PA Temp CMP Index [14]>#<SIGNED_BYTE,PA Temp CMP Index [15]>#
NV_DCS_PA_TEMP_COMP_INDEX_2_I,1289,ReadWrite,<SIGNED_BYTE,PA Temp CMP Index[0]>#<SIGNED_BYTE,PA Temp CMP Index [1]>#<SIGNED_BYTE,PA Temp CMP Index [2]>#<SIGNED_BYTE,PA Temp CMP Index [3]>#<SIGNED_BYTE,PA Temp CMP Index [4]>#<SIGNED_BYTE,PA Temp CMP Index [5]>#<SIGNED_BYTE,PA Temp CMP Index [6]>#<SIGNED_BYTE,PA Temp CMP Index [7]>#<SIGNED_BYTE,PA Temp CMP Index [8]>#<SIGNED_BYTE,PA Temp CMP Index [9]>#<SIGNED_BYTE,PA Temp CMP Index [10]>#<SIGNED_BYTE,PA Temp CMP Index [11]>#<SIGNED_BYTE,PA Temp CMP Index [12]>#<SIGNED_BYTE,PA Temp CMP Index [13]>#<SIGNED_BYTE,PA Temp CMP Index [14]>#<SIGNED_BYTE,PA Temp CMP Index [15]>#
NV_DCS_PA_TEMP_COMP_INDEX_3_I,1290,ReadWrite,<SIGNED_BYTE,PA Temp CMP Index[0]>#<SIGNED_BYTE,PA Temp CMP Index [1]>#<SIGNED_BYTE,PA Temp CMP Index [2]>#<SIGNED_BYTE,PA Temp CMP Index [3]>#<SIGNED_BYTE,PA Temp CMP Index [4]>#<SIGNED_BYTE,PA Temp CMP Index [5]>#<SIGNED_BYTE,PA Temp CMP Index [6]>#<SIGNED_BYTE,PA Temp CMP Index [7]>#<SIGNED_BYTE,PA Temp CMP Index [8]>#<SIGNED_BYTE,PA Temp CMP Index [9]>#<SIGNED_BYTE,PA Temp CMP Index [10]>#<SIGNED_BYTE,PA Temp CMP Index [11]>#<SIGNED_BYTE,PA Temp CMP Index [12]>#<SIGNED_BYTE,PA Temp CMP Index [13]>#<SIGNED_BYTE,PA Temp CMP Index [14]>#<SIGNED_BYTE,PA Temp CMP Index [15]>#
NV_DCS_PA_TEMP_COMP_INDEX_4_I,1291,ReadWrite,<SIGNED_BYTE,PA Temp CMP Index[0]>#<SIGNED_BYTE,PA Temp CMP Index [1]>#<SIGNED_BYTE,PA Temp CMP Index [2]>#<SIGNED_BYTE,PA Temp CMP Index [3]>#<SIGNED_BYTE,PA Temp CMP Index [4]>#<SIGNED_BYTE,PA Temp CMP Index [5]>#<SIGNED_BYTE,PA Temp CMP Index [6]>#<SIGNED_BYTE,PA Temp CMP Index [7]>#<SIGNED_BYTE,PA Temp CMP Index [8]>#<SIGNED_BYTE,PA Temp CMP Index [9]>#<SIGNED_BYTE,PA Temp CMP Index [10]>#<SIGNED_BYTE,PA Temp CMP Index [11]>#<SIGNED_BYTE,PA Temp CMP Index [12]>#<SIGNED_BYTE,PA Temp CMP Index [13]>#<SIGNED_BYTE,PA Temp CMP Index [14]>#<SIGNED_BYTE,PA Temp CMP Index [15]>#
NV_DCS_PA_TEMP_COMP_INDEX_5_I,1292,ReadWrite,<SIGNED_BYTE,PA Temp CMP Index[0]>#<SIGNED_BYTE,PA Temp CMP Index [1]>#<SIGNED_BYTE,PA Temp CMP Index [2]>#<SIGNED_BYTE,PA Temp CMP Index [3]>#<SIGNED_BYTE,PA Temp CMP Index [4]>#<SIGNED_BYTE,PA Temp CMP Index [5]>#<SIGNED_BYTE,PA Temp CMP Index [6]>#<SIGNED_BYTE,PA Temp CMP Index [7]>#<SIGNED_BYTE,PA Temp CMP Index [8]>#<SIGNED_BYTE,PA Temp CMP Index [9]>#<SIGNED_BYTE,PA Temp CMP Index [10]>#<SIGNED_BYTE,PA Temp CMP Index [11]>#<SIGNED_BYTE,PA Temp CMP Index [12]>#<SIGNED_BYTE,PA Temp CMP Index [13]>#<SIGNED_BYTE,PA Temp CMP Index [14]>#<SIGNED_BYTE,PA Temp CMP Index [15]>#
NV_DCS_PA_TEMP_COMP_INDEX_6_I,1293,ReadWrite,<SIGNED_BYTE,PA Temp CMP Index[0]>#<SIGNED_BYTE,PA Temp CMP Index [1]>#<SIGNED_BYTE,PA Temp CMP Index [2]>#<SIGNED_BYTE,PA Temp CMP Index [3]>#<SIGNED_BYTE,PA Temp CMP Index [4]>#<SIGNED_BYTE,PA Temp CMP Index [5]>#<SIGNED_BYTE,PA Temp CMP Index [6]>#<SIGNED_BYTE,PA Temp CMP Index [7]>#<SIGNED_BYTE,PA Temp CMP Index [8]>#<SIGNED_BYTE,PA Temp CMP Index [9]>#<SIGNED_BYTE,PA Temp CMP Index [10]>#<SIGNED_BYTE,PA Temp CMP Index [11]>#<SIGNED_BYTE,PA Temp CMP Index [12]>#<SIGNED_BYTE,PA Temp CMP Index [13]>#<SIGNED_BYTE,PA Temp CMP Index [14]>#<SIGNED_BYTE,PA Temp CMP Index [15]>#
NV_DCS_PA_TEMP_COMP_INDEX_7_I,1294,ReadWrite,<SIGNED_BYTE,PA Temp CMP Index[0]>#<SIGNED_BYTE,PA Temp CMP Index [1]>#<SIGNED_BYTE,PA Temp CMP Index [2]>#<SIGNED_BYTE,PA Temp CMP Index [3]>#<SIGNED_BYTE,PA Temp CMP Index [4]>#<SIGNED_BYTE,PA Temp CMP Index [5]>#<SIGNED_BYTE,PA Temp CMP Index [6]>#<SIGNED_BYTE,PA Temp CMP Index [7]>#<SIGNED_BYTE,PA Temp CMP Index [8]>#<SIGNED_BYTE,PA Temp CMP Index [9]>#<SIGNED_BYTE,PA Temp CMP Index [10]>#<SIGNED_BYTE,PA Temp CMP Index [11]>#<SIGNED_BYTE,PA Temp CMP Index [12]>#<SIGNED_BYTE,PA Temp CMP Index [13]>#<SIGNED_BYTE,PA Temp CMP Index [14]>#<SIGNED_BYTE,PA Temp CMP Index [15]>#
NV_DCS_PA_TEMP_COMP_INDEX_8_I,1295,ReadWrite,<SIGNED_BYTE,PA Temp CMP Index[0]>#<SIGNED_BYTE,PA Temp CMP Index [1]>#<SIGNED_BYTE,PA Temp CMP Index [2]>#<SIGNED_BYTE,PA Temp CMP Index [3]>#<SIGNED_BYTE,PA Temp CMP Index [4]>#<SIGNED_BYTE,PA Temp CMP Index [5]>#<SIGNED_BYTE,PA Temp CMP Index [6]>#<SIGNED_BYTE,PA Temp CMP Index [7]>#<SIGNED_BYTE,PA Temp CMP Index [8]>#<SIGNED_BYTE,PA Temp CMP Index [9]>#<SIGNED_BYTE,PA Temp CMP Index [10]>#<SIGNED_BYTE,PA Temp CMP Index [11]>#<SIGNED_BYTE,PA Temp CMP Index [12]>#<SIGNED_BYTE,PA Temp CMP Index [13]>#<SIGNED_BYTE,PA Temp CMP Index [14]>#<SIGNED_BYTE,PA Temp CMP Index [15]>#
NV_DCS_PA_TEMP_COMP_INDEX_9_I,1296,ReadWrite,<SIGNED_BYTE,PA Temp CMP Index[0]>#<SIGNED_BYTE,PA Temp CMP Index [1]>#<SIGNED_BYTE,PA Temp CMP Index [2]>#<SIGNED_BYTE,PA Temp CMP Index [3]>#<SIGNED_BYTE,PA Temp CMP Index [4]>#<SIGNED_BYTE,PA Temp CMP Index [5]>#<SIGNED_BYTE,PA Temp CMP Index [6]>#<SIGNED_BYTE,PA Temp CMP Index [7]>#<SIGNED_BYTE,PA Temp CMP Index [8]>#<SIGNED_BYTE,PA Temp CMP Index [9]>#<SIGNED_BYTE,PA Temp CMP Index [10]>#<SIGNED_BYTE,PA Temp CMP Index [11]>#<SIGNED_BYTE,PA Temp CMP Index [12]>#<SIGNED_BYTE,PA Temp CMP Index [13]>#<SIGNED_BYTE,PA Temp CMP Index [14]>#<SIGNED_BYTE,PA Temp CMP Index [15]>#
NV_DCS_PA_TEMP_COMP_INDEX_10_I,1297,ReadWrite,<SIGNED_BYTE,PA Temp CMP Index[0]>#<SIGNED_BYTE,PA Temp CMP Index [1]>#<SIGNED_BYTE,PA Temp CMP Index [2]>#<SIGNED_BYTE,PA Temp CMP Index [3]>#<SIGNED_BYTE,PA Temp CMP Index [4]>#<SIGNED_BYTE,PA Temp CMP Index [5]>#<SIGNED_BYTE,PA Temp CMP Index [6]>#<SIGNED_BYTE,PA Temp CMP Index [7]>#<SIGNED_BYTE,PA Temp CMP Index [8]>#<SIGNED_BYTE,PA Temp CMP Index [9]>#<SIGNED_BYTE,PA Temp CMP Index [10]>#<SIGNED_BYTE,PA Temp CMP Index [11]>#<SIGNED_BYTE,PA Temp CMP Index [12]>#<SIGNED_BYTE,PA Temp CMP Index [13]>#<SIGNED_BYTE,PA Temp CMP Index [14]>#<SIGNED_BYTE,PA Temp CMP Index [15]>#
NV_DCS_PA_TEMP_COMP_INDEX_11_I,1298,ReadWrite,<SIGNED_BYTE,PA Temp CMP Index[0]>#<SIGNED_BYTE,PA Temp CMP Index [1]>#<SIGNED_BYTE,PA Temp CMP Index [2]>#<SIGNED_BYTE,PA Temp CMP Index [3]>#<SIGNED_BYTE,PA Temp CMP Index [4]>#<SIGNED_BYTE,PA Temp CMP Index [5]>#<SIGNED_BYTE,PA Temp CMP Index [6]>#<SIGNED_BYTE,PA Temp CMP Index [7]>#<SIGNED_BYTE,PA Temp CMP Index [8]>#<SIGNED_BYTE,PA Temp CMP Index [9]>#<SIGNED_BYTE,PA Temp CMP Index [10]>#<SIGNED_BYTE,PA Temp CMP Index [11]>#<SIGNED_BYTE,PA Temp CMP Index [12]>#<SIGNED_BYTE,PA Temp CMP Index [13]>#<SIGNED_BYTE,PA Temp CMP Index [14]>#<SIGNED_BYTE,PA Temp CMP Index [15]>#
NV_DCS_PA_TEMP_COMP_INDEX_12_I,1299,ReadWrite,<SIGNED_BYTE,PA Temp CMP Index[0]>#<SIGNED_BYTE,PA Temp CMP Index [1]>#<SIGNED_BYTE,PA Temp CMP Index [2]>#<SIGNED_BYTE,PA Temp CMP Index [3]>#<SIGNED_BYTE,PA Temp CMP Index [4]>#<SIGNED_BYTE,PA Temp CMP Index [5]>#<SIGNED_BYTE,PA Temp CMP Index [6]>#<SIGNED_BYTE,PA Temp CMP Index [7]>#<SIGNED_BYTE,PA Temp CMP Index [8]>#<SIGNED_BYTE,PA Temp CMP Index [9]>#<SIGNED_BYTE,PA Temp CMP Index [10]>#<SIGNED_BYTE,PA Temp CMP Index [11]>#<SIGNED_BYTE,PA Temp CMP Index [12]>#<SIGNED_BYTE,PA Temp CMP Index [13]>#<SIGNED_BYTE,PA Temp CMP Index [14]>#<SIGNED_BYTE,PA Temp CMP Index [15]>#
NV_DCS_PA_TEMP_COMP_INDEX_13_I,1300,ReadWrite,<SIGNED_BYTE,PA Temp CMP Index[0]>#<SIGNED_BYTE,PA Temp CMP Index [1]>#<SIGNED_BYTE,PA Temp CMP Index [2]>#<SIGNED_BYTE,PA Temp CMP Index [3]>#<SIGNED_BYTE,PA Temp CMP Index [4]>#<SIGNED_BYTE,PA Temp CMP Index [5]>#<SIGNED_BYTE,PA Temp CMP Index [6]>#<SIGNED_BYTE,PA Temp CMP Index [7]>#<SIGNED_BYTE,PA Temp CMP Index [8]>#<SIGNED_BYTE,PA Temp CMP Index [9]>#<SIGNED_BYTE,PA Temp CMP Index [10]>#<SIGNED_BYTE,PA Temp CMP Index [11]>#<SIGNED_BYTE,PA Temp CMP Index [12]>#<SIGNED_BYTE,PA Temp CMP Index [13]>#<SIGNED_BYTE,PA Temp CMP Index [14]>#<SIGNED_BYTE,PA Temp CMP Index [15]>#
NV_DCS_PA_TEMP_COMP_INDEX_14_I,1301,ReadWrite,<SIGNED_BYTE,PA Temp CMP Index[0]>#<SIGNED_BYTE,PA Temp CMP Index [1]>#<SIGNED_BYTE,PA Temp CMP Index [2]>#<SIGNED_BYTE,PA Temp CMP Index [3]>#<SIGNED_BYTE,PA Temp CMP Index [4]>#<SIGNED_BYTE,PA Temp CMP Index [5]>#<SIGNED_BYTE,PA Temp CMP Index [6]>#<SIGNED_BYTE,PA Temp CMP Index [7]>#<SIGNED_BYTE,PA Temp CMP Index [8]>#<SIGNED_BYTE,PA Temp CMP Index [9]>#<SIGNED_BYTE,PA Temp CMP Index [10]>#<SIGNED_BYTE,PA Temp CMP Index [11]>#<SIGNED_BYTE,PA Temp CMP Index [12]>#<SIGNED_BYTE,PA Temp CMP Index [13]>#<SIGNED_BYTE,PA Temp CMP Index [14]>#<SIGNED_BYTE,PA Temp CMP Index [15]>#
NV_DCS_PA_TEMP_COMP_INDEX_15_I,935,ReadWrite,<SIGNED_BYTE,PA Temp CMP Index[0]>#<SIGNED_BYTE,PA Temp CMP Index [1]>#<SIGNED_BYTE,PA Temp CMP Index [2]>#<SIGNED_BYTE,PA Temp CMP Index [3]>#<SIGNED_BYTE,PA Temp CMP Index [4]>#<SIGNED_BYTE,PA Temp CMP Index [5]>#<SIGNED_BYTE,PA Temp CMP Index [6]>#<SIGNED_BYTE,PA Temp CMP Index [7]>#<SIGNED_BYTE,PA Temp CMP Index [8]>#<SIGNED_BYTE,PA Temp CMP Index [9]>#<SIGNED_BYTE,PA Temp CMP Index [10]>#<SIGNED_BYTE,PA Temp CMP Index [11]>#<SIGNED_BYTE,PA Temp CMP Index [12]>#<SIGNED_BYTE,PA Temp CMP Index [13]>#<SIGNED_BYTE,PA Temp CMP Index [14]>#<SIGNED_BYTE,PA Temp CMP Index [15]>#
NV_DCS_PA_TEMP_COMP_INT8_INDEX_15_I,1304,ReadWrite,<SIGNED_BYTE,PA Temp CMP Index 15[0]>#<SIGNED_BYTE,PA Temp CMP Index 15[1]>#<SIGNED_BYTE,PA Temp CMP Index 15[2]>#<SIGNED_BYTE,PA Temp CMP Index 15[3]>#<SIGNED_BYTE,PA Temp CMP Index 15[4]>#<SIGNED_BYTE,PA Temp CMP Index 15[5]>#<SIGNED_BYTE,PA Temp CMP Index 15[6]>#<SIGNED_BYTE,PA Temp CMP Index 15[7]>#<SIGNED_BYTE,PA Temp CMP Index 15[8]>#<SIGNED_BYTE,PA Temp CMP Index 15[9]>#<SIGNED_BYTE,PA Temp CMP Index 15[10]>#<SIGNED_BYTE,PA Temp CMP Index 15[11]>#<SIGNED_BYTE,PA Temp CMP Index 15[12]>#<SIGNED_BYTE,PA Temp CMP Index 15[13]>#<SIGNED_BYTE,PA Temp CMP Index 15[14]>#<SIGNED_BYTE,PA Temp CMP Index 15[15]>#
NV_PA_COMPENSATE_UP_I,1801,ReadWrite,<SIGNED_WORD,PA_Compensate_Up>#
NV_PA_COMPENSATE_DOWN_I,1802,ReadWrite,<SIGNED_WORD,PA_Compensate_Down>#
NV_RFR_BB_FILTER_I,1791,ReadWrite,<BYTE,RFR_Baseband_Filter_Cal_Value>#
NV_RFR_IQ_LINE_RESISTOR_I,1792,ReadWrite,<BYTE,RFR_IQ_Line_Resistor_Cal_Value>#
NV_VCO_COARSE_TUNE_TABLE_I,931,ReadWrite,<BYTE,VCO_Coarse_Tune_Val[0]>#<BYTE,VCO_Coarse_Tune_Val[1]>#<BYTE,VCO_Coarse_Tune_Val[2]>#<BYTE,VCO_Coarse_Tune_Val[3]>#<BYTE,VCO_Coarse_Tune_Val[4]>#<BYTE,VCO_Coarse_Tune_Val[5]>#<BYTE,VCO_Coarse_Tune_Val[6]>#<BYTE,VCO_Coarse_Tune_Val[7]>#<BYTE,VCO_Coarse_Tune_Val[8]>#<BYTE,VCO_Coarse_Tune_Val[9]>#<BYTE,VCO_Coarse_Tune_Val[10]>#<BYTE,VCO_Coarse_Tune_Val[11]>#<BYTE,VCO_Coarse_Tune_Val[12]>#<BYTE,VCO_Coarse_Tune_Val[13]>#<BYTE,VCO_Coarse_Tune_Val[14]>#<BYTE,VCO_Coarse_Tune_Val[15]>#
NV_RFR_VCO_COARSE_TUNING_1900_I,1794,ReadWrite,<BYTE,VCO_Coarse_Tune_Val[0]>#<BYTE,VCO_Coarse_Tune_Val[1]>#<BYTE,VCO_Coarse_Tune_Val[2]>#<BYTE,VCO_Coarse_Tune_Val[3]>#<BYTE,VCO_Coarse_Tune_Val[4]>#<BYTE,VCO_Coarse_Tune_Val[5]>#<BYTE,VCO_Coarse_Tune_Val[6]>#<BYTE,VCO_Coarse_Tune_Val[7]>#<BYTE,VCO_Coarse_Tune_Val[8]>#<BYTE,VCO_Coarse_Tune_Val[9]>#<BYTE,VCO_Coarse_Tune_Val[10]>#<BYTE,VCO_Coarse_Tune_Val[11]>#
NV_BC0_ENC_BTF_I ,1734,ReadWrite,<DWORD,BACK TO future>#
NV_BC0_EXP_HDET_VS_AGC_I ,1733,ReadWrite,<BYTE,Array[0]>#<BYTE,Array[1]>#<BYTE,Array[2]>#<BYTE,Array[3]>#<BYTE,Array[4]>#<BYTE,Array[5]>#<BYTE,Array[6]>#<BYTE,Array[7]>#<BYTE,Array[8]>#<BYTE,Array[9]>#<BYTE,Array[10]>#<BYTE,Array[11]>#<BYTE,Array[12]>#<BYTE,Array[13]>#<BYTE,Array[14]>#<BYTE,Array[15]>#
NV_BC0_HDET_OFF_I,1731,ReadWrite,<BYTE,ADC HDET reading offset>#
NV_BC0_HDET_SPN_I,1732,ReadWrite,<BYTE,ADC HDET reading span>#
NV_BC0_P1_RISE_FALL_OFF_I,1736,ReadWrite,<BYTE,Array[0]>#<BYTE,Array[1]>#<BYTE,Array[2]>#<BYTE,Array[3]>#<BYTE,Array[4]>#<BYTE,Array[5]>#<BYTE,Array[6]>#<BYTE,Array[7]>#
NV_BC0_PA_R1_FALL_I,1726,ReadWrite,<WORD,BC0_PA_R1_FALL>#
NV_BC0_PA_R1_RISE_I,1725,ReadWrite,<WORD,BC0_PA_R1_RISE>#
NV_BC0_PA_R2_FALL_I,1728,ReadWrite,<WORD,BC0_PA_R2_FALL>#
NV_BC0_PA_R2_RISE_I,1727,ReadWrite,<WORD,BC0_PA_R2_RISE>#
NV_BC0_PA_R3_FALL_I,1730,ReadWrite,<WORD,BC0_PA_R3_FALL>#
NV_BC0_PA_R3_RISE_I,1729,ReadWrite,<WORD,BC0_PA_R3_RISE>#
NV_BC0_TX_COMP0_I,1720,ReadWrite,<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[0]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[1]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[2]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[3]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[4]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[5]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[6]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[8]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[9]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[10]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[11]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[12]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[13]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[14]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[15]>#
NV_BC0_TX_COMP1_I,1721,ReadWrite,<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[0]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[1]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[2]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[3]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[4]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[5]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[6]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[8]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[9]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[10]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[11]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[12]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[13]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[14]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[15]>#
NV_BC0_TX_COMP2_I,1722,ReadWrite,<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[0]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[1]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[2]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[3]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[4]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[5]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[6]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[8]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[9]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[10]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[11]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[12]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[13]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[14]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[15]>#
NV_BC0_TX_COMP3_I,1723,ReadWrite,<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[0]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[1]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[2]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[3]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[4]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[5]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[6]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[8]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[9]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[10]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[11]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[12]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[13]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[14]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[15]>#
NV_BC0_TX_LIM_VS_FREQ_I,1724,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_BC0_TX_LIM_VS_TEMP_I,1715,ReadWrite,<BYTE,Array[1]>#<BYTE,Array[1]>#<BYTE,Array[2]>#<BYTE,Array[3]>#<BYTE,Array[4]>#<BYTE,Array[5]>#<BYTE,Array[6]>#<BYTE,Array[7]>#
NV_BC0_TX_LIN_MASTER0_I,1716,ReadWrite,<SIGNED_WORD,Offset>#<BYTE,Slope[0]>#<BYTE,Slope[1]>#<BYTE,Slope[2]>#<BYTE,Slope[3]>#<BYTE,Slope[4]>#<BYTE,Slope[5]>#<BYTE,Slope[6]>#<BYTE,Slope[7]>#<BYTE,Slope[8]>#<BYTE,Slope[9]>#<BYTE,Slope[10]>#<BYTE,Slope[11]>#<BYTE,Slope[12]>#<BYTE,Slope[13]>#<BYTE,Slope[14]>#<BYTE,Slope[15]>#<BYTE,Slope[16]>#<BYTE,Slope[17]>#<BYTE,Slope[18]>#<BYTE,Slope[19]>#<BYTE,Slope[20]>#<BYTE,Slope[21]>#<BYTE,Slope[22]>#<BYTE,Slope[23]>#<BYTE,Slope[24]>#<BYTE,Slope[25]>#<BYTE,Slope[26]>#<BYTE,Slope[27]>#<BYTE,Slope[28]>#<BYTE,Slope[29]>#<BYTE,Slope[30]>#<BYTE,Slope[31]>#<BYTE,Slope[32]>#<BYTE,Slope[33]>#<BYTE,Slope[34]>#<BYTE,Slope[35]>#
NV_BC0_TX_LIN_MASTER1_I,1717,ReadWrite,<SIGNED_WORD,Offset>#<BYTE,Slope[0]>#<BYTE,Slope[1]>#<BYTE,Slope[2]>#<BYTE,Slope[3]>#<BYTE,Slope[4]>#<BYTE,Slope[5]>#<BYTE,Slope[6]>#<BYTE,Slope[7]>#<BYTE,Slope[8]>#<BYTE,Slope[9]>#<BYTE,Slope[10]>#<BYTE,Slope[11]>#<BYTE,Slope[12]>#<BYTE,Slope[13]>#<BYTE,Slope[14]>#<BYTE,Slope[15]>#<BYTE,Slope[16]>#<BYTE,Slope[17]>#<BYTE,Slope[18]>#<BYTE,Slope[19]>#<BYTE,Slope[20]>#<BYTE,Slope[21]>#<BYTE,Slope[22]>#<BYTE,Slope[23]>#<BYTE,Slope[24]>#<BYTE,Slope[25]>#<BYTE,Slope[26]>#<BYTE,Slope[27]>#<BYTE,Slope[28]>#<BYTE,Slope[29]>#<BYTE,Slope[30]>#<BYTE,Slope[31]>#<BYTE,Slope[32]>#<BYTE,Slope[33]>#<BYTE,Slope[34]>#<BYTE,Slope[35]>#
NV_BC0_TX_LIN_MASTER2_I,1718,ReadWrite,<SIGNED_WORD,Offset>#<BYTE,Slope[0]>#<BYTE,Slope[1]>#<BYTE,Slope[2]>#<BYTE,Slope[3]>#<BYTE,Slope[4]>#<BYTE,Slope[5]>#<BYTE,Slope[6]>#<BYTE,Slope[7]>#<BYTE,Slope[8]>#<BYTE,Slope[9]>#<BYTE,Slope[10]>#<BYTE,Slope[11]>#<BYTE,Slope[12]>#<BYTE,Slope[13]>#<BYTE,Slope[14]>#<BYTE,Slope[15]>#<BYTE,Slope[16]>#<BYTE,Slope[17]>#<BYTE,Slope[18]>#<BYTE,Slope[19]>#<BYTE,Slope[20]>#<BYTE,Slope[21]>#<BYTE,Slope[22]>#<BYTE,Slope[23]>#<BYTE,Slope[24]>#<BYTE,Slope[25]>#<BYTE,Slope[26]>#<BYTE,Slope[27]>#<BYTE,Slope[28]>#<BYTE,Slope[29]>#<BYTE,Slope[30]>#<BYTE,Slope[31]>#<BYTE,Slope[32]>#<BYTE,Slope[33]>#<BYTE,Slope[34]>#<BYTE,Slope[35]>#
NV_BC0_TX_LIN_MASTER3_I,1719,ReadWrite,<SIGNED_WORD,Offset>#<BYTE,Slope[0]>#<BYTE,Slope[1]>#<BYTE,Slope[2]>#<BYTE,Slope[3]>#<BYTE,Slope[4]>#<BYTE,Slope[5]>#<BYTE,Slope[6]>#<BYTE,Slope[7]>#<BYTE,Slope[8]>#<BYTE,Slope[9]>#<BYTE,Slope[10]>#<BYTE,Slope[11]>#<BYTE,Slope[12]>#<BYTE,Slope[13]>#<BYTE,Slope[14]>#<BYTE,Slope[15]>#<BYTE,Slope[16]>#<BYTE,Slope[17]>#<BYTE,Slope[18]>#<BYTE,Slope[19]>#<BYTE,Slope[20]>#<BYTE,Slope[21]>#<BYTE,Slope[22]>#<BYTE,Slope[23]>#<BYTE,Slope[24]>#<BYTE,Slope[25]>#<BYTE,Slope[26]>#<BYTE,Slope[27]>#<BYTE,Slope[28]>#<BYTE,Slope[29]>#<BYTE,Slope[30]>#<BYTE,Slope[31]>#<BYTE,Slope[32]>#<BYTE,Slope[33]>#<BYTE,Slope[34]>#<BYTE,Slope[35]>#
NV_BC0_VCO_COARSE_TUNE_TABLE_I  ,1735,ReadWrite,<BYTE,Array[0]>#<BYTE,Array[1]>#<BYTE,Array[2]>#<BYTE,Array[3]>#<BYTE,Array[4]>#<BYTE,Array[5]>#<BYTE,Array[6]>#<BYTE,Array[7]>#<BYTE,Array[8]>#<BYTE,Array[9]>#<BYTE,Array[10]>#<BYTE,Array[11]>#<BYTE,Array[12]>#<BYTE,Array[13]>#<BYTE,Array[14]>#<BYTE,Array[15]>#
NV_BC1_ENC_BTF_I,1645,ReadWrite,<DWORD,BACK TO future>#
NV_BC1_EXP_HDET_VS_AGC_I ,1644,ReadWrite,<BYTE,Array[0]>#<BYTE,Array[1]>#<BYTE,Array[2]>#<BYTE,Array[3]>#<BYTE,Array[4]>#<BYTE,Array[5]>#<BYTE,Array[6]>#<BYTE,Array[7]>#<BYTE,Array[8]>#<BYTE,Array[9]>#<BYTE,Array[10]>#<BYTE,Array[11]>#<BYTE,Array[12]>#<BYTE,Array[13]>#<BYTE,Array[14]>#<BYTE,Array[15]>#
NV_BC1_HDET_OFF_I,1642,ReadWrite,<BYTE,ADC HDET reading offset>#
NV_BC1_HDET_SPN_I,1643,ReadWrite,<BYTE,ADC HDET reading span>#
NV_BC1_P1_RISE_FALL_OFF_I,1647,ReadWrite,<BYTE,Array[0]>#<BYTE,Array[1]>#<BYTE,Array[2]>#<BYTE,Array[3]>#<BYTE,Array[4]>#<BYTE,Array[5]>#<BYTE,Array[6]>#<BYTE,Array[7]>#
NV_BC1_PA_R1_FALL_I,1637,ReadWrite,<WORD,BC1_PA_R1_FALL>#
NV_BC1_PA_R1_RISE_I,1636,ReadWrite,<WORD,BC1_PA_R1_RISE>#
NV_BC1_PA_R2_FALL_I,1639,ReadWrite,<WORD,BC1_PA_R2_FALL>#
NV_BC1_PA_R2_RISE_I,1638,ReadWrite,<WORD,BC1_PA_R2_RISE>#
NV_BC1_PA_R3_FALL_I,1641,ReadWrite,<WORD,BC1_PA_R3_FALL>#
NV_BC1_PA_R3_RISE_I,1640,ReadWrite,<WORD,BC1_PA_R3_RISE>#
NV_BC1_TX_COMP0_I ,1631,ReadWrite,<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[0]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[1]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[2]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[3]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[4]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[5]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[6]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[8]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[9]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[10]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[11]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[12]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[13]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[14]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[15]>#
NV_BC1_TX_COMP1_I,1632,ReadWrite,<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[0]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[1]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[2]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[3]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[4]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[5]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[6]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[8]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[9]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[10]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[11]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[12]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[13]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[14]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[15]>#
NV_BC1_TX_COMP2_I,1633,ReadWrite,<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[0]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[1]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[2]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[3]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[4]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[5]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[6]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[8]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[9]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[10]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[11]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[12]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[13]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[14]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[15]>#
NV_BC1_TX_COMP3_I,1634,ReadWrite,<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[0]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[1]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[2]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[3]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[4]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[5]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[6]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[8]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[9]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[10]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[11]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[12]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[13]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[14]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[15]>#
NV_BC1_TX_LIM_VS_FREQ_I,1635,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_BC1_TX_LIM_VS_TEMP_I,1626,ReadWrite,<BYTE,Array[1]>#<BYTE,Array[1]>#<BYTE,Array[2]>#<BYTE,Array[3]>#<BYTE,Array[4]>#<BYTE,Array[5]>#<BYTE,Array[6]>#<BYTE,Array[7]>#
NV_BC1_TX_LIN_MASTER0_I,1627,ReadWrite,<SIGNED_WORD,Offset>#<BYTE,Slope[0]>#<BYTE,Slope[1]>#<BYTE,Slope[2]>#<BYTE,Slope[3]>#<BYTE,Slope[4]>#<BYTE,Slope[5]>#<BYTE,Slope[6]>#<BYTE,Slope[7]>#<BYTE,Slope[8]>#<BYTE,Slope[9]>#<BYTE,Slope[10]>#<BYTE,Slope[11]>#<BYTE,Slope[12]>#<BYTE,Slope[13]>#<BYTE,Slope[14]>#<BYTE,Slope[15]>#<BYTE,Slope[16]>#<BYTE,Slope[17]>#<BYTE,Slope[18]>#<BYTE,Slope[19]>#<BYTE,Slope[20]>#<BYTE,Slope[21]>#<BYTE,Slope[22]>#<BYTE,Slope[23]>#<BYTE,Slope[24]>#<BYTE,Slope[25]>#<BYTE,Slope[26]>#<BYTE,Slope[27]>#<BYTE,Slope[28]>#<BYTE,Slope[29]>#<BYTE,Slope[30]>#<BYTE,Slope[31]>#<BYTE,Slope[32]>#<BYTE,Slope[33]>#<BYTE,Slope[34]>#<BYTE,Slope[35]>#
NV_BC1_TX_LIN_MASTER1_I,1628,ReadWrite,<SIGNED_WORD,Offset>#<BYTE,Slope[0]>#<BYTE,Slope[1]>#<BYTE,Slope[2]>#<BYTE,Slope[3]>#<BYTE,Slope[4]>#<BYTE,Slope[5]>#<BYTE,Slope[6]>#<BYTE,Slope[7]>#<BYTE,Slope[8]>#<BYTE,Slope[9]>#<BYTE,Slope[10]>#<BYTE,Slope[11]>#<BYTE,Slope[12]>#<BYTE,Slope[13]>#<BYTE,Slope[14]>#<BYTE,Slope[15]>#<BYTE,Slope[16]>#<BYTE,Slope[17]>#<BYTE,Slope[18]>#<BYTE,Slope[19]>#<BYTE,Slope[20]>#<BYTE,Slope[21]>#<BYTE,Slope[22]>#<BYTE,Slope[23]>#<BYTE,Slope[24]>#<BYTE,Slope[25]>#<BYTE,Slope[26]>#<BYTE,Slope[27]>#<BYTE,Slope[28]>#<BYTE,Slope[29]>#<BYTE,Slope[30]>#<BYTE,Slope[31]>#<BYTE,Slope[32]>#<BYTE,Slope[33]>#<BYTE,Slope[34]>#<BYTE,Slope[35]>#
NV_BC1_TX_LIN_MASTER2_I,1629,ReadWrite,<SIGNED_WORD,Offset>#<BYTE,Slope[0]>#<BYTE,Slope[1]>#<BYTE,Slope[2]>#<BYTE,Slope[3]>#<BYTE,Slope[4]>#<BYTE,Slope[5]>#<BYTE,Slope[6]>#<BYTE,Slope[7]>#<BYTE,Slope[8]>#<BYTE,Slope[9]>#<BYTE,Slope[10]>#<BYTE,Slope[11]>#<BYTE,Slope[12]>#<BYTE,Slope[13]>#<BYTE,Slope[14]>#<BYTE,Slope[15]>#<BYTE,Slope[16]>#<BYTE,Slope[17]>#<BYTE,Slope[18]>#<BYTE,Slope[19]>#<BYTE,Slope[20]>#<BYTE,Slope[21]>#<BYTE,Slope[22]>#<BYTE,Slope[23]>#<BYTE,Slope[24]>#<BYTE,Slope[25]>#<BYTE,Slope[26]>#<BYTE,Slope[27]>#<BYTE,Slope[28]>#<BYTE,Slope[29]>#<BYTE,Slope[30]>#<BYTE,Slope[31]>#<BYTE,Slope[32]>#<BYTE,Slope[33]>#<BYTE,Slope[34]>#<BYTE,Slope[35]>#
NV_BC1_TX_LIN_MASTER3_I,1630,ReadWrite,<SIGNED_WORD,Offset>#<BYTE,Slope[0]>#<BYTE,Slope[1]>#<BYTE,Slope[2]>#<BYTE,Slope[3]>#<BYTE,Slope[4]>#<BYTE,Slope[5]>#<BYTE,Slope[6]>#<BYTE,Slope[7]>#<BYTE,Slope[8]>#<BYTE,Slope[9]>#<BYTE,Slope[10]>#<BYTE,Slope[11]>#<BYTE,Slope[12]>#<BYTE,Slope[13]>#<BYTE,Slope[14]>#<BYTE,Slope[15]>#<BYTE,Slope[16]>#<BYTE,Slope[17]>#<BYTE,Slope[18]>#<BYTE,Slope[19]>#<BYTE,Slope[20]>#<BYTE,Slope[21]>#<BYTE,Slope[22]>#<BYTE,Slope[23]>#<BYTE,Slope[24]>#<BYTE,Slope[25]>#<BYTE,Slope[26]>#<BYTE,Slope[27]>#<BYTE,Slope[28]>#<BYTE,Slope[29]>#<BYTE,Slope[30]>#<BYTE,Slope[31]>#<BYTE,Slope[32]>#<BYTE,Slope[33]>#<BYTE,Slope[34]>#<BYTE,Slope[35]>#
NV_BC1_VCO_COARSE_TUNE_TABLE_I  ,1646,ReadWrite,<BYTE,Array[0]>#<BYTE,Array[1]>#<BYTE,Array[2]>#<BYTE,Array[3]>#<BYTE,Array[4]>#<BYTE,Array[5]>#<BYTE,Array[6]>#<BYTE,Array[7]>#<BYTE,Array[8]>#<BYTE,Array[9]>#<BYTE,Array[10]>#<BYTE,Array[11]>#<BYTE,Array[12]>#<BYTE,Array[13]>#<BYTE,Array[14]>#<BYTE,Array[15]>#
NV_BC3_ENC_BTF_I,1567,ReadWrite,<DWORD,BACK TO future>#
NV_BC3_EXP_HDET_VS_AGC_I ,1566,ReadWrite,<BYTE,Array[0]>#<BYTE,Array[1]>#<BYTE,Array[2]>#<BYTE,Array[3]>#<BYTE,Array[4]>#<BYTE,Array[5]>#<BYTE,Array[6]>#<BYTE,Array[7]>#<BYTE,Array[8]>#<BYTE,Array[9]>#<BYTE,Array[10]>#<BYTE,Array[11]>#<BYTE,Array[12]>#<BYTE,Array[13]>#<BYTE,Array[14]>#<BYTE,Array[15]>#
NV_BC3_HDET_OFF_I ,1564,ReadWrite,<BYTE,ADC HDET reading offset>#
NV_BC3_HDET_SPN_I ,1565,ReadWrite,<BYTE,ADC HDET reading span>#
NV_BC3_P1_RISE_FALL_OFF_I,1569,ReadWrite,<BYTE,Array[0]>#<BYTE,Array[1]>#<BYTE,Array[2]>#<BYTE,Array[3]>#<BYTE,Array[4]>#<BYTE,Array[5]>#<BYTE,Array[6]>#<BYTE,Array[7]>#
NV_BC3_PA_R1_FALL_I,1559,ReadWrite,<WORD,BC3_PA_R1_FALL>#
NV_BC3_PA_R1_RISE_I,1558,ReadWrite,<WORD,BC3_PA_R1_RISE>#
NV_BC3_PA_R2_FALL_I,1561,ReadWrite,<WORD,BC3_PA_R2_FALL>#
NV_BC3_PA_R2_RISE_I,1560,ReadWrite,<WORD,BC3_PA_R2_RISE>#
NV_BC3_PA_R3_FALL_I,1563,ReadWrite,<WORD,BC3_PA_R3_RISE>#
NV_BC3_PA_R3_RISE_I,1562,ReadWrite,<WORD,BC3_PA_R3_RISE>#
NV_BC3_TX_COMP0_I,1552,ReadWrite,<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[0]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[1]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[2]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[3]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[4]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[5]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[6]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[8]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[9]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[10]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[11]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[12]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[13]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[14]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[15]>#
NV_BC3_TX_COMP1_I ,1553,ReadWrite,<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[0]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[1]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[2]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[3]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[4]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[5]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[6]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[8]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[9]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[10]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[11]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[12]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[13]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[14]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[15]>#
NV_BC3_TX_COMP2_I ,1554,ReadWrite,<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[0]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[1]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[2]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[3]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[4]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[5]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[6]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[8]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[9]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[10]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[11]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[12]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[13]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[14]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[15]>#
NV_BC3_TX_COMP3_I ,1555,ReadWrite,<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[0]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[1]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[2]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[3]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[4]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[5]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[6]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[8]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[9]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[10]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[11]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[12]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[13]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[14]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[15]>#
NV_BC3_TX_LIM_VS_FREQ_I,1557,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_BC3_TX_LIM_VS_TEMP_I,1547,ReadWrite,<BYTE,Array[1]>#<BYTE,Array[1]>#<BYTE,Array[2]>#<BYTE,Array[3]>#<BYTE,Array[4]>#<BYTE,Array[5]>#<BYTE,Array[6]>#<BYTE,Array[7]>#
NV_BC3_TX_LIN_MASTER0_I,1548,ReadWrite,<SIGNED_WORD,Offset>#<BYTE,Slope[0]>#<BYTE,Slope[1]>#<BYTE,Slope[2]>#<BYTE,Slope[3]>#<BYTE,Slope[4]>#<BYTE,Slope[5]>#<BYTE,Slope[6]>#<BYTE,Slope[7]>#<BYTE,Slope[8]>#<BYTE,Slope[9]>#<BYTE,Slope[10]>#<BYTE,Slope[11]>#<BYTE,Slope[12]>#<BYTE,Slope[13]>#<BYTE,Slope[14]>#<BYTE,Slope[15]>#<BYTE,Slope[16]>#<BYTE,Slope[17]>#<BYTE,Slope[18]>#<BYTE,Slope[19]>#<BYTE,Slope[20]>#<BYTE,Slope[21]>#<BYTE,Slope[22]>#<BYTE,Slope[23]>#<BYTE,Slope[24]>#<BYTE,Slope[25]>#<BYTE,Slope[26]>#<BYTE,Slope[27]>#<BYTE,Slope[28]>#<BYTE,Slope[29]>#<BYTE,Slope[30]>#<BYTE,Slope[31]>#<BYTE,Slope[32]>#<BYTE,Slope[33]>#<BYTE,Slope[34]>#<BYTE,Slope[35]>#
NV_BC3_TX_LIN_MASTER1_I,1549,ReadWrite,<SIGNED_WORD,Offset>#<BYTE,Slope[0]>#<BYTE,Slope[1]>#<BYTE,Slope[2]>#<BYTE,Slope[3]>#<BYTE,Slope[4]>#<BYTE,Slope[5]>#<BYTE,Slope[6]>#<BYTE,Slope[7]>#<BYTE,Slope[8]>#<BYTE,Slope[9]>#<BYTE,Slope[10]>#<BYTE,Slope[11]>#<BYTE,Slope[12]>#<BYTE,Slope[13]>#<BYTE,Slope[14]>#<BYTE,Slope[15]>#<BYTE,Slope[16]>#<BYTE,Slope[17]>#<BYTE,Slope[18]>#<BYTE,Slope[19]>#<BYTE,Slope[20]>#<BYTE,Slope[21]>#<BYTE,Slope[22]>#<BYTE,Slope[23]>#<BYTE,Slope[24]>#<BYTE,Slope[25]>#<BYTE,Slope[26]>#<BYTE,Slope[27]>#<BYTE,Slope[28]>#<BYTE,Slope[29]>#<BYTE,Slope[30]>#<BYTE,Slope[31]>#<BYTE,Slope[32]>#<BYTE,Slope[33]>#<BYTE,Slope[34]>#<BYTE,Slope[35]>#
NV_BC3_TX_LIN_MASTER2_I,1550,ReadWrite,<SIGNED_WORD,Offset>#<BYTE,Slope[0]>#<BYTE,Slope[1]>#<BYTE,Slope[2]>#<BYTE,Slope[3]>#<BYTE,Slope[4]>#<BYTE,Slope[5]>#<BYTE,Slope[6]>#<BYTE,Slope[7]>#<BYTE,Slope[8]>#<BYTE,Slope[9]>#<BYTE,Slope[10]>#<BYTE,Slope[11]>#<BYTE,Slope[12]>#<BYTE,Slope[13]>#<BYTE,Slope[14]>#<BYTE,Slope[15]>#<BYTE,Slope[16]>#<BYTE,Slope[17]>#<BYTE,Slope[18]>#<BYTE,Slope[19]>#<BYTE,Slope[20]>#<BYTE,Slope[21]>#<BYTE,Slope[22]>#<BYTE,Slope[23]>#<BYTE,Slope[24]>#<BYTE,Slope[25]>#<BYTE,Slope[26]>#<BYTE,Slope[27]>#<BYTE,Slope[28]>#<BYTE,Slope[29]>#<BYTE,Slope[30]>#<BYTE,Slope[31]>#<BYTE,Slope[32]>#<BYTE,Slope[33]>#<BYTE,Slope[34]>#<BYTE,Slope[35]>#
NV_BC3_TX_LIN_MASTER3_I,1551,ReadWrite,<SIGNED_WORD,Offset>#<BYTE,Slope[0]>#<BYTE,Slope[1]>#<BYTE,Slope[2]>#<BYTE,Slope[3]>#<BYTE,Slope[4]>#<BYTE,Slope[5]>#<BYTE,Slope[6]>#<BYTE,Slope[7]>#<BYTE,Slope[8]>#<BYTE,Slope[9]>#<BYTE,Slope[10]>#<BYTE,Slope[11]>#<BYTE,Slope[12]>#<BYTE,Slope[13]>#<BYTE,Slope[14]>#<BYTE,Slope[15]>#<BYTE,Slope[16]>#<BYTE,Slope[17]>#<BYTE,Slope[18]>#<BYTE,Slope[19]>#<BYTE,Slope[20]>#<BYTE,Slope[21]>#<BYTE,Slope[22]>#<BYTE,Slope[23]>#<BYTE,Slope[24]>#<BYTE,Slope[25]>#<BYTE,Slope[26]>#<BYTE,Slope[27]>#<BYTE,Slope[28]>#<BYTE,Slope[29]>#<BYTE,Slope[30]>#<BYTE,Slope[31]>#<BYTE,Slope[32]>#<BYTE,Slope[33]>#<BYTE,Slope[34]>#<BYTE,Slope[35]>#
NV_BC3_VCO_COARSE_TUNE_TABLE_I  ,1568,ReadWrite,<BYTE,Array[0]>#<BYTE,Array[1]>#<BYTE,Array[2]>#<BYTE,Array[3]>#<BYTE,Array[4]>#<BYTE,Array[5]>#<BYTE,Array[6]>#<BYTE,Array[7]>#<BYTE,Array[8]>#<BYTE,Array[9]>#<BYTE,Array[10]>#<BYTE,Array[11]>#<BYTE,Array[12]>#<BYTE,Array[13]>#<BYTE,Array[14]>#<BYTE,Array[15]>#
NV_BC4_ENC_BTF_I,1488,ReadWrite,<DWORD,BACK TO future>#
NV_BC4_EXP_HDET_VS_AGC_I ,1487,ReadWrite,<BYTE,Array[0]>#<BYTE,Array[1]>#<BYTE,Array[2]>#<BYTE,Array[3]>#<BYTE,Array[4]>#<BYTE,Array[5]>#<BYTE,Array[6]>#<BYTE,Array[7]>#<BYTE,Array[8]>#<BYTE,Array[9]>#<BYTE,Array[10]>#<BYTE,Array[11]>#<BYTE,Array[12]>#<BYTE,Array[13]>#<BYTE,Array[14]>#<BYTE,Array[15]>#
NV_BC4_HDET_OFF_I ,1485,ReadWrite,<BYTE,ADC HDET reading offset>#
NV_BC4_HDET_SPN_I ,1486,ReadWrite,<BYTE,ADC HDET reading span>#
NV_BC4_P1_RISE_FALL_OFF_I,1490,ReadWrite,<BYTE,Array[0]>#<BYTE,Array[1]>#<BYTE,Array[2]>#<BYTE,Array[3]>#<BYTE,Array[4]>#<BYTE,Array[5]>#<BYTE,Array[6]>#<BYTE,Array[7]>#
NV_BC4_PA_R1_FALL_I,1480,ReadWrite,<WORD,BC4_PA_R1_FALL>#
NV_BC4_PA_R1_RISE_I,1479,ReadWrite,<WORD,BC4_PA_R1_RISE>#
NV_BC4_PA_R2_FALL_I,1482,ReadWrite,<WORD,BC4_PA_R2_FALL>#
NV_BC4_PA_R2_RISE_I,1481,ReadWrite,<WORD,BC4_PA_R2_RISE>#
NV_BC4_PA_R3_FALL_I,1484,ReadWrite,<WORD,BC4_PA_R3_FALL>#
NV_BC4_PA_R3_RISE_I,1483,ReadWrite,<WORD,BC4_PA_R3_RISE>#
NV_BC4_TX_COMP0_I ,1474,ReadWrite,<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[0]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[1]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[2]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[3]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[4]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[5]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[6]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[8]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[9]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[10]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[11]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[12]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[13]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[14]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[15]>#
NV_BC4_TX_COMP1_I ,1475,ReadWrite,<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[0]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[1]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[2]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[3]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[4]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[5]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[6]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[8]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[9]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[10]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[11]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[12]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[13]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[14]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[15]>#
NV_BC4_TX_COMP2_I ,1476,ReadWrite,<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[0]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[1]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[2]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[3]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[4]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[5]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[6]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[8]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[9]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[10]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[11]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[12]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[13]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[14]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[15]>#
NV_BC4_TX_COMP3_I ,1477,ReadWrite,<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[0]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[1]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[2]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[3]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[4]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[5]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[6]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[8]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[9]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[10]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[11]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[12]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[13]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[14]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[15]>#
NV_BC4_TX_LIM_VS_FREQ_I,1478,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_BC4_TX_LIM_VS_TEMP_I,1469,ReadWrite,<BYTE,Array[1]>#<BYTE,Array[1]>#<BYTE,Array[2]>#<BYTE,Array[3]>#<BYTE,Array[4]>#<BYTE,Array[5]>#<BYTE,Array[6]>#<BYTE,Array[7]>#
NV_BC4_TX_LIN_MASTER0_I,1470,ReadWrite,<SIGNED_WORD,Offset>#<BYTE,Slope[0]>#<BYTE,Slope[1]>#<BYTE,Slope[2]>#<BYTE,Slope[3]>#<BYTE,Slope[4]>#<BYTE,Slope[5]>#<BYTE,Slope[6]>#<BYTE,Slope[7]>#<BYTE,Slope[8]>#<BYTE,Slope[9]>#<BYTE,Slope[10]>#<BYTE,Slope[11]>#<BYTE,Slope[12]>#<BYTE,Slope[13]>#<BYTE,Slope[14]>#<BYTE,Slope[15]>#<BYTE,Slope[16]>#<BYTE,Slope[17]>#<BYTE,Slope[18]>#<BYTE,Slope[19]>#<BYTE,Slope[20]>#<BYTE,Slope[21]>#<BYTE,Slope[22]>#<BYTE,Slope[23]>#<BYTE,Slope[24]>#<BYTE,Slope[25]>#<BYTE,Slope[26]>#<BYTE,Slope[27]>#<BYTE,Slope[28]>#<BYTE,Slope[29]>#<BYTE,Slope[30]>#<BYTE,Slope[31]>#<BYTE,Slope[32]>#<BYTE,Slope[33]>#<BYTE,Slope[34]>#<BYTE,Slope[35]>#
NV_BC4_TX_LIN_MASTER1_I,1471,ReadWrite,<SIGNED_WORD,Offset>#<BYTE,Slope[0]>#<BYTE,Slope[1]>#<BYTE,Slope[2]>#<BYTE,Slope[3]>#<BYTE,Slope[4]>#<BYTE,Slope[5]>#<BYTE,Slope[6]>#<BYTE,Slope[7]>#<BYTE,Slope[8]>#<BYTE,Slope[9]>#<BYTE,Slope[10]>#<BYTE,Slope[11]>#<BYTE,Slope[12]>#<BYTE,Slope[13]>#<BYTE,Slope[14]>#<BYTE,Slope[15]>#<BYTE,Slope[16]>#<BYTE,Slope[17]>#<BYTE,Slope[18]>#<BYTE,Slope[19]>#<BYTE,Slope[20]>#<BYTE,Slope[21]>#<BYTE,Slope[22]>#<BYTE,Slope[23]>#<BYTE,Slope[24]>#<BYTE,Slope[25]>#<BYTE,Slope[26]>#<BYTE,Slope[27]>#<BYTE,Slope[28]>#<BYTE,Slope[29]>#<BYTE,Slope[30]>#<BYTE,Slope[31]>#<BYTE,Slope[32]>#<BYTE,Slope[33]>#<BYTE,Slope[34]>#<BYTE,Slope[35]>#
NV_BC4_TX_LIN_MASTER2_I,1472,ReadWrite,<SIGNED_WORD,Offset>#<BYTE,Slope[0]>#<BYTE,Slope[1]>#<BYTE,Slope[2]>#<BYTE,Slope[3]>#<BYTE,Slope[4]>#<BYTE,Slope[5]>#<BYTE,Slope[6]>#<BYTE,Slope[7]>#<BYTE,Slope[8]>#<BYTE,Slope[9]>#<BYTE,Slope[10]>#<BYTE,Slope[11]>#<BYTE,Slope[12]>#<BYTE,Slope[13]>#<BYTE,Slope[14]>#<BYTE,Slope[15]>#<BYTE,Slope[16]>#<BYTE,Slope[17]>#<BYTE,Slope[18]>#<BYTE,Slope[19]>#<BYTE,Slope[20]>#<BYTE,Slope[21]>#<BYTE,Slope[22]>#<BYTE,Slope[23]>#<BYTE,Slope[24]>#<BYTE,Slope[25]>#<BYTE,Slope[26]>#<BYTE,Slope[27]>#<BYTE,Slope[28]>#<BYTE,Slope[29]>#<BYTE,Slope[30]>#<BYTE,Slope[31]>#<BYTE,Slope[32]>#<BYTE,Slope[33]>#<BYTE,Slope[34]>#<BYTE,Slope[35]>#
NV_BC4_TX_LIN_MASTER3_I,1473,ReadWrite,<SIGNED_WORD,Offset>#<BYTE,Slope[0]>#<BYTE,Slope[1]>#<BYTE,Slope[2]>#<BYTE,Slope[3]>#<BYTE,Slope[4]>#<BYTE,Slope[5]>#<BYTE,Slope[6]>#<BYTE,Slope[7]>#<BYTE,Slope[8]>#<BYTE,Slope[9]>#<BYTE,Slope[10]>#<BYTE,Slope[11]>#<BYTE,Slope[12]>#<BYTE,Slope[13]>#<BYTE,Slope[14]>#<BYTE,Slope[15]>#<BYTE,Slope[16]>#<BYTE,Slope[17]>#<BYTE,Slope[18]>#<BYTE,Slope[19]>#<BYTE,Slope[20]>#<BYTE,Slope[21]>#<BYTE,Slope[22]>#<BYTE,Slope[23]>#<BYTE,Slope[24]>#<BYTE,Slope[25]>#<BYTE,Slope[26]>#<BYTE,Slope[27]>#<BYTE,Slope[28]>#<BYTE,Slope[29]>#<BYTE,Slope[30]>#<BYTE,Slope[31]>#<BYTE,Slope[32]>#<BYTE,Slope[33]>#<BYTE,Slope[34]>#<BYTE,Slope[35]>#
NV_BC4_VCO_COARSE_TUNE_TABLE_I  ,1489,ReadWrite,<BYTE,Array[0]>#<BYTE,Array[1]>#<BYTE,Array[2]>#<BYTE,Array[3]>#<BYTE,Array[4]>#<BYTE,Array[5]>#<BYTE,Array[6]>#<BYTE,Array[7]>#<BYTE,Array[8]>#<BYTE,Array[9]>#<BYTE,Array[10]>#<BYTE,Array[11]>#<BYTE,Array[12]>#<BYTE,Array[13]>#<BYTE,Array[14]>#<BYTE,Array[15]>#
NV_BC5_ENC_BTF_I,1410,ReadWrite,<DWORD,BACK TO future>#
NV_BC5_EXP_HDET_VS_AGC_I ,1409,ReadWrite,<BYTE,Array[0]>#<BYTE,Array[1]>#<BYTE,Array[2]>#<BYTE,Array[3]>#<BYTE,Array[4]>#<BYTE,Array[5]>#<BYTE,Array[6]>#<BYTE,Array[7]>#<BYTE,Array[8]>#<BYTE,Array[9]>#<BYTE,Array[10]>#<BYTE,Array[11]>#<BYTE,Array[12]>#<BYTE,Array[13]>#<BYTE,Array[14]>#<BYTE,Array[15]>#
NV_BC5_HDET_OFF_I ,1407,ReadWrite,<BYTE,ADC HDET reading offset>#
NV_BC5_HDET_SPN_I ,1408,ReadWrite,<BYTE,ADC HDET reading span>#
NV_BC5_P1_RISE_FALL_OFF_I,1412,ReadWrite,<BYTE,Array[0]>#<BYTE,Array[1]>#<BYTE,Array[2]>#<BYTE,Array[3]>#<BYTE,Array[4]>#<BYTE,Array[5]>#<BYTE,Array[6]>#<BYTE,Array[7]>#
NV_BC5_PA_R1_FALL_I,1402,ReadWrite,<WORD,BC5_PA_R1_FALL>#
NV_BC5_PA_R1_RISE_I,1401,ReadWrite,<WORD,BC5_PA_R1_RISE>#
NV_BC5_PA_R2_FALL_I,1404,ReadWrite,<WORD,BC5_PA_R2_FALL>#
NV_BC5_PA_R2_RISE_I,1403,ReadWrite,<WORD,BC5_PA_R2_RISE>#
NV_BC5_PA_R3_FALL_I,1406,ReadWrite,<WORD,BC5_PA_R3_RISE>#
NV_BC5_PA_R3_RISE_I,1405,ReadWrite,<WORD,BC5_PA_R3_RISE>#
NV_BC5_TX_COMP0_I ,1396,ReadWrite,<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[0]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[1]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[2]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[3]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[4]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[5]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[6]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[8]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[9]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[10]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[11]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[12]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[13]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[14]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[15]>#
NV_BC5_TX_COMP1_I ,1397,ReadWrite,<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[0]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[1]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[2]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[3]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[4]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[5]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[6]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[8]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[9]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[10]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[11]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[12]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[13]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[14]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[15]>#
NV_BC5_TX_COMP2_I ,1398,ReadWrite,<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[0]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[1]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[2]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[3]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[4]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[5]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[6]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[8]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[9]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[10]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[11]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[12]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[13]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[14]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[15]>#
NV_BC5_TX_COMP3_I ,1399,ReadWrite,<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[0]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[1]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[2]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[3]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[4]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[5]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[6]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[8]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[9]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[10]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[11]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[12]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[13]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[14]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[15]>#
NV_BC5_TX_LIM_VS_FREQ_I,1400,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_BC5_TX_LIM_VS_TEMP_I,1391,ReadWrite,<BYTE,Array[1]>#<BYTE,Array[1]>#<BYTE,Array[2]>#<BYTE,Array[3]>#<BYTE,Array[4]>#<BYTE,Array[5]>#<BYTE,Array[6]>#<BYTE,Array[7]>#
NV_BC5_TX_LIN_MASTER0_I,1392,ReadWrite,<SIGNED_WORD,Offset>#<BYTE,Slope[0]>#<BYTE,Slope[1]>#<BYTE,Slope[2]>#<BYTE,Slope[3]>#<BYTE,Slope[4]>#<BYTE,Slope[5]>#<BYTE,Slope[6]>#<BYTE,Slope[7]>#<BYTE,Slope[8]>#<BYTE,Slope[9]>#<BYTE,Slope[10]>#<BYTE,Slope[11]>#<BYTE,Slope[12]>#<BYTE,Slope[13]>#<BYTE,Slope[14]>#<BYTE,Slope[15]>#<BYTE,Slope[16]>#<BYTE,Slope[17]>#<BYTE,Slope[18]>#<BYTE,Slope[19]>#<BYTE,Slope[20]>#<BYTE,Slope[21]>#<BYTE,Slope[22]>#<BYTE,Slope[23]>#<BYTE,Slope[24]>#<BYTE,Slope[25]>#<BYTE,Slope[26]>#<BYTE,Slope[27]>#<BYTE,Slope[28]>#<BYTE,Slope[29]>#<BYTE,Slope[30]>#<BYTE,Slope[31]>#<BYTE,Slope[32]>#<BYTE,Slope[33]>#<BYTE,Slope[34]>#<BYTE,Slope[35]>#
NV_BC5_TX_LIN_MASTER1_I,1393,ReadWrite,<SIGNED_WORD,Offset>#<BYTE,Slope[0]>#<BYTE,Slope[1]>#<BYTE,Slope[2]>#<BYTE,Slope[3]>#<BYTE,Slope[4]>#<BYTE,Slope[5]>#<BYTE,Slope[6]>#<BYTE,Slope[7]>#<BYTE,Slope[8]>#<BYTE,Slope[9]>#<BYTE,Slope[10]>#<BYTE,Slope[11]>#<BYTE,Slope[12]>#<BYTE,Slope[13]>#<BYTE,Slope[14]>#<BYTE,Slope[15]>#<BYTE,Slope[16]>#<BYTE,Slope[17]>#<BYTE,Slope[18]>#<BYTE,Slope[19]>#<BYTE,Slope[20]>#<BYTE,Slope[21]>#<BYTE,Slope[22]>#<BYTE,Slope[23]>#<BYTE,Slope[24]>#<BYTE,Slope[25]>#<BYTE,Slope[26]>#<BYTE,Slope[27]>#<BYTE,Slope[28]>#<BYTE,Slope[29]>#<BYTE,Slope[30]>#<BYTE,Slope[31]>#<BYTE,Slope[32]>#<BYTE,Slope[33]>#<BYTE,Slope[34]>#<BYTE,Slope[35]>#
NV_BC5_TX_LIN_MASTER2_I,1394,ReadWrite,<SIGNED_WORD,Offset>#<BYTE,Slope[0]>#<BYTE,Slope[1]>#<BYTE,Slope[2]>#<BYTE,Slope[3]>#<BYTE,Slope[4]>#<BYTE,Slope[5]>#<BYTE,Slope[6]>#<BYTE,Slope[7]>#<BYTE,Slope[8]>#<BYTE,Slope[9]>#<BYTE,Slope[10]>#<BYTE,Slope[11]>#<BYTE,Slope[12]>#<BYTE,Slope[13]>#<BYTE,Slope[14]>#<BYTE,Slope[15]>#<BYTE,Slope[16]>#<BYTE,Slope[17]>#<BYTE,Slope[18]>#<BYTE,Slope[19]>#<BYTE,Slope[20]>#<BYTE,Slope[21]>#<BYTE,Slope[22]>#<BYTE,Slope[23]>#<BYTE,Slope[24]>#<BYTE,Slope[25]>#<BYTE,Slope[26]>#<BYTE,Slope[27]>#<BYTE,Slope[28]>#<BYTE,Slope[29]>#<BYTE,Slope[30]>#<BYTE,Slope[31]>#<BYTE,Slope[32]>#<BYTE,Slope[33]>#<BYTE,Slope[34]>#<BYTE,Slope[35]>#
NV_BC5_TX_LIN_MASTER3_I,1395,ReadWrite,<SIGNED_WORD,Offset>#<BYTE,Slope[0]>#<BYTE,Slope[1]>#<BYTE,Slope[2]>#<BYTE,Slope[3]>#<BYTE,Slope[4]>#<BYTE,Slope[5]>#<BYTE,Slope[6]>#<BYTE,Slope[7]>#<BYTE,Slope[8]>#<BYTE,Slope[9]>#<BYTE,Slope[10]>#<BYTE,Slope[11]>#<BYTE,Slope[12]>#<BYTE,Slope[13]>#<BYTE,Slope[14]>#<BYTE,Slope[15]>#<BYTE,Slope[16]>#<BYTE,Slope[17]>#<BYTE,Slope[18]>#<BYTE,Slope[19]>#<BYTE,Slope[20]>#<BYTE,Slope[21]>#<BYTE,Slope[22]>#<BYTE,Slope[23]>#<BYTE,Slope[24]>#<BYTE,Slope[25]>#<BYTE,Slope[26]>#<BYTE,Slope[27]>#<BYTE,Slope[28]>#<BYTE,Slope[29]>#<BYTE,Slope[30]>#<BYTE,Slope[31]>#<BYTE,Slope[32]>#<BYTE,Slope[33]>#<BYTE,Slope[34]>#<BYTE,Slope[35]>#
NV_BC5_VCO_COARSE_TUNE_TABLE_I  ,1411,ReadWrite,<BYTE,Array[0]>#<BYTE,Array[1]>#<BYTE,Array[2]>#<BYTE,Array[3]>#<BYTE,Array[4]>#<BYTE,Array[5]>#<BYTE,Array[6]>#<BYTE,Array[7]>#<BYTE,Array[8]>#<BYTE,Array[9]>#<BYTE,Array[10]>#<BYTE,Array[11]>#<BYTE,Array[12]>#<BYTE,Array[13]>#<BYTE,Array[14]>#<BYTE,Array[15]>#
NV_BC6_ENC_BTF_I,1240,ReadWrite,<DWORD,BACK TO future>#
NV_BC6_EXP_HDET_VS_AGC_I ,1217,ReadWrite,<BYTE,Array[0]>#<BYTE,Array[1]>#<BYTE,Array[2]>#<BYTE,Array[3]>#<BYTE,Array[4]>#<BYTE,Array[5]>#<BYTE,Array[6]>#<BYTE,Array[7]>#<BYTE,Array[8]>#<BYTE,Array[9]>#<BYTE,Array[10]>#<BYTE,Array[11]>#<BYTE,Array[12]>#<BYTE,Array[13]>#<BYTE,Array[14]>#<BYTE,Array[15]>#
NV_BC6_HDET_OFF_I ,1218,ReadWrite,<BYTE,ADC HDET reading offset>#
NV_BC6_HDET_SPN_I ,1219,ReadWrite,<BYTE,ADC HDET reading span>#
NV_BC6_LNA_1_FALL_I,1224,ReadWrite,<BYTE,BC6_LNA_1_FALL>#
NV_BC6_LNA_1_RISE_I,1223,ReadWrite,<BYTE,BC6_LNA_1_RISE>#
NV_BC6_LNA_2_FALL_I,1228,ReadWrite,<BYTE,BC6_LNA_2_FALL>#
NV_BC6_LNA_2_RISE_I,1227,ReadWrite,<BYTE,BC6_LNA_2_RISE>#
NV_BC6_LNA_3_FALL_I,1242,ReadWrite,<BYTE,BC6_LNA_3_FALL>#
NV_BC6_LNA_3_OFFSET_I  ,1244,ReadWrite,<SIGNED_WORD,Offset added to Receive power >#
NV_BC6_LNA_3_RISE_I,1243,ReadWrite,<BYTE,BC6_LNA_3_RISE>#
NV_BC6_LNA_4_FALL_I,1247,ReadWrite,<BYTE,BC6_LNA_4_FALL>#
NV_BC6_LNA_4_RISE_I,1248,ReadWrite,<BYTE,BC6_LNA_4_RISE>#
NV_BC6_LNA_RANGE_12_OFFSET_I,1229,ReadWrite,<SIGNED_WORD,Offset added to Receive power when the first and second LNAs are bypassed>#
NV_BC6_LNA_RANGE_POL_I ,1222,ReadWrite,<BYTE,LNA range polarity>#
NV_BC6_P1_RISE_FALL_OFF_I,1261,ReadWrite,<BYTE,Array[0]>#<BYTE,Array[1]>#<BYTE,Array[2]>#<BYTE,Array[3]>#<BYTE,Array[4]>#<BYTE,Array[5]>#<BYTE,Array[6]>#<BYTE,Array[7]>#
NV_BC6_PA_R1_FALL_I,1221,ReadWrite,<WORD,BC6_PA_R1_FALSE>#
NV_BC6_PA_R1_RISE_I,1220,ReadWrite,<WORD,BC6_PA_R1_RISE>#
NV_BC6_PA_R2_FALL_I,1356,ReadWrite,<WORD,BC6_PA_R2_FALL>#
NV_BC6_PA_R2_RISE_I,1355,ReadWrite,<WORD,BC6_PA_R2_RISE>#
NV_BC6_PA_R3_FALL_I,1358,ReadWrite,<WORD,BC6_PA_R3_FALL>#
NV_BC6_PA_R3_RISE_I,1357,ReadWrite,<WORD,BC6_PA_R3_RISE>#
NV_BC6_TX_COMP0_I ,1214,ReadWrite,<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[0]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[1]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[2]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[3]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[4]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[5]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[6]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[8]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[9]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[10]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[11]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[12]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[13]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[14]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[15]>#
NV_BC6_TX_COMP1_I ,1215,ReadWrite,<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[0]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[1]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[2]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[3]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[4]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[5]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[6]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[8]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[9]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[10]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[11]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[12]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[13]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[14]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[15]>#
NV_BC6_TX_COMP2_I ,1353,ReadWrite,<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[0]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[1]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[2]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[3]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[4]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[5]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[6]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[8]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[9]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[10]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[11]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[12]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[13]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[14]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[15]>#
NV_BC6_TX_COMP3_I ,1354,ReadWrite,<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_lin_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[0]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[1]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[2]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[3]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[4]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[5]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[6]>#<SIGNED_BYTE,nv_cdma_tx_slp_vs_temp[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[0]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[1]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[2]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[3]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[4]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[5]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[6]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[7]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[8]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[9]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[10]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[11]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[12]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[13]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[14]>#<SIGNED_BYTE,nv_cdma_tx_comp_vs_freq[15]>#
NV_BC6_TX_LIM_VS_FREQ_I,1216,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_BC6_TX_LIM_VS_TEMP_I,1210,ReadWrite,<BYTE,Array[1]>#<BYTE,Array[1]>#<BYTE,Array[2]>#<BYTE,Array[3]>#<BYTE,Array[4]>#<BYTE,Array[5]>#<BYTE,Array[6]>#<BYTE,Array[7]>#
NV_BC6_TX_LIN_MASTER0_I,1212,ReadWrite,<SIGNED_WORD,Offset>#<BYTE,Slope[0]>#<BYTE,Slope[1]>#<BYTE,Slope[2]>#<BYTE,Slope[3]>#<BYTE,Slope[4]>#<BYTE,Slope[5]>#<BYTE,Slope[6]>#<BYTE,Slope[7]>#<BYTE,Slope[8]>#<BYTE,Slope[9]>#<BYTE,Slope[10]>#<BYTE,Slope[11]>#<BYTE,Slope[12]>#<BYTE,Slope[13]>#<BYTE,Slope[14]>#<BYTE,Slope[15]>#<BYTE,Slope[16]>#<BYTE,Slope[17]>#<BYTE,Slope[18]>#<BYTE,Slope[19]>#<BYTE,Slope[20]>#<BYTE,Slope[21]>#<BYTE,Slope[22]>#<BYTE,Slope[23]>#<BYTE,Slope[24]>#<BYTE,Slope[25]>#<BYTE,Slope[26]>#<BYTE,Slope[27]>#<BYTE,Slope[28]>#<BYTE,Slope[29]>#<BYTE,Slope[30]>#<BYTE,Slope[31]>#<BYTE,Slope[32]>#<BYTE,Slope[33]>#<BYTE,Slope[34]>#<BYTE,Slope[35]>#
NV_BC6_TX_LIN_MASTER1_I,1213,ReadWrite,<SIGNED_WORD,Offset>#<BYTE,Slope[0]>#<BYTE,Slope[1]>#<BYTE,Slope[2]>#<BYTE,Slope[3]>#<BYTE,Slope[4]>#<BYTE,Slope[5]>#<BYTE,Slope[6]>#<BYTE,Slope[7]>#<BYTE,Slope[8]>#<BYTE,Slope[9]>#<BYTE,Slope[10]>#<BYTE,Slope[11]>#<BYTE,Slope[12]>#<BYTE,Slope[13]>#<BYTE,Slope[14]>#<BYTE,Slope[15]>#<BYTE,Slope[16]>#<BYTE,Slope[17]>#<BYTE,Slope[18]>#<BYTE,Slope[19]>#<BYTE,Slope[20]>#<BYTE,Slope[21]>#<BYTE,Slope[22]>#<BYTE,Slope[23]>#<BYTE,Slope[24]>#<BYTE,Slope[25]>#<BYTE,Slope[26]>#<BYTE,Slope[27]>#<BYTE,Slope[28]>#<BYTE,Slope[29]>#<BYTE,Slope[30]>#<BYTE,Slope[31]>#<BYTE,Slope[32]>#<BYTE,Slope[33]>#<BYTE,Slope[34]>#<BYTE,Slope[35]>#
NV_BC6_TX_LIN_MASTER2_I,1351,ReadWrite,<SIGNED_WORD,Offset>#<BYTE,Slope[0]>#<BYTE,Slope[1]>#<BYTE,Slope[2]>#<BYTE,Slope[3]>#<BYTE,Slope[4]>#<BYTE,Slope[5]>#<BYTE,Slope[6]>#<BYTE,Slope[7]>#<BYTE,Slope[8]>#<BYTE,Slope[9]>#<BYTE,Slope[10]>#<BYTE,Slope[11]>#<BYTE,Slope[12]>#<BYTE,Slope[13]>#<BYTE,Slope[14]>#<BYTE,Slope[15]>#<BYTE,Slope[16]>#<BYTE,Slope[17]>#<BYTE,Slope[18]>#<BYTE,Slope[19]>#<BYTE,Slope[20]>#<BYTE,Slope[21]>#<BYTE,Slope[22]>#<BYTE,Slope[23]>#<BYTE,Slope[24]>#<BYTE,Slope[25]>#<BYTE,Slope[26]>#<BYTE,Slope[27]>#<BYTE,Slope[28]>#<BYTE,Slope[29]>#<BYTE,Slope[30]>#<BYTE,Slope[31]>#<BYTE,Slope[32]>#<BYTE,Slope[33]>#<BYTE,Slope[34]>#<BYTE,Slope[35]>#
NV_BC6_TX_LIN_MASTER3_I,1352,ReadWrite,<SIGNED_WORD,Offset>#<BYTE,Slope[0]>#<BYTE,Slope[1]>#<BYTE,Slope[2]>#<BYTE,Slope[3]>#<BYTE,Slope[4]>#<BYTE,Slope[5]>#<BYTE,Slope[6]>#<BYTE,Slope[7]>#<BYTE,Slope[8]>#<BYTE,Slope[9]>#<BYTE,Slope[10]>#<BYTE,Slope[11]>#<BYTE,Slope[12]>#<BYTE,Slope[13]>#<BYTE,Slope[14]>#<BYTE,Slope[15]>#<BYTE,Slope[16]>#<BYTE,Slope[17]>#<BYTE,Slope[18]>#<BYTE,Slope[19]>#<BYTE,Slope[20]>#<BYTE,Slope[21]>#<BYTE,Slope[22]>#<BYTE,Slope[23]>#<BYTE,Slope[24]>#<BYTE,Slope[25]>#<BYTE,Slope[26]>#<BYTE,Slope[27]>#<BYTE,Slope[28]>#<BYTE,Slope[29]>#<BYTE,Slope[30]>#<BYTE,Slope[31]>#<BYTE,Slope[32]>#<BYTE,Slope[33]>#<BYTE,Slope[34]>#<BYTE,Slope[35]>#
NV_BC6_VCO_COARSE_TUNE_TABLE_I  ,1272,ReadWrite,<BYTE,Array[0]>#<BYTE,Array[1]>#<BYTE,Array[2]>#<BYTE,Array[3]>#<BYTE,Array[4]>#<BYTE,Array[5]>#<BYTE,Array[6]>#<BYTE,Array[7]>#<BYTE,Array[8]>#<BYTE,Array[9]>#<BYTE,Array[10]>#<BYTE,Array[11]>#<BYTE,Array[12]>#<BYTE,Array[13]>#<BYTE,Array[14]>#<BYTE,Array[15]>#
NV_C0_BC0_IM_LEVEL1_I,1760,ReadWrite,<BYTE, InterMod antijamming threshold power level>#
NV_C0_BC0_IM_LEVEL2_I,1761,ReadWrite,<BYTE, InterMod antijamming threshold power level>#
NV_C0_BC0_IM_LEVEL3_I,1762,ReadWrite,<BYTE, InterMod antijamming threshold power level>#
NV_C0_BC0_IM_LEVEL4_I,1763,ReadWrite,<BYTE, InterMod antijamming threshold power level>#
NV_C0_BC0_IM2_I_VALUE_I,1747,ReadWrite,<BYTE, InterMod antijamming setting>#
NV_C0_BC0_IM2_Q_VALUE_I,1748,ReadWrite,<BYTE, InterMod antijamming setting>#
NV_C0_BC0_IM2_TRANSCONDUCTOR_VALUE_I,1751,ReadWrite,<BYTE,Transconductor value>#
NV_C0_BC0_LNA_1_FALL_I ,1753,ReadWrite,<BYTE,LNA_1_FALL>#
NV_C0_BC0_LNA_1_OFFSET_I ,1743,ReadWrite,<SIGNED_WORD, LNA range  offset>#
NV_C0_BC0_LNA_1_OFFSET_VS_FREQ_I,1739,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C0_BC0_LNA_1_RISE_I ,1752,ReadWrite,<BYTE,LNA_1_RISE>#
NV_C0_BC0_LNA_2_FALL_I ,1755,ReadWrite,<BYTE,LNA_2_FALL>#
NV_C0_BC0_LNA_2_OFFSET_I ,1744,ReadWrite,<SIGNED_WORD, LNA range  offset>#
NV_C0_BC0_LNA_2_OFFSET_VS_FREQ_I,1740,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C0_BC0_LNA_2_RISE_I ,1754,ReadWrite,<BYTE,LNA_2_RISE>#
NV_C0_BC0_LNA_3_FALL_I ,1757,ReadWrite,<BYTE,LNA_3_FALL>#
NV_C0_BC0_LNA_3_OFFSET_I ,1745,ReadWrite,<SIGNED_WORD, LNA range  offset>#
NV_C0_BC0_LNA_3_OFFSET_VS_FREQ_I,1741,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C0_BC0_LNA_3_RISE_I ,1756,ReadWrite,<BYTE,LNA_3_RISE>#
NV_C0_BC0_LNA_4_FALL_I ,1759,ReadWrite,<BYTE,LNA_4_FALL>#
NV_C0_BC0_LNA_4_OFFSET_I ,1746,ReadWrite,<SIGNED_WORD, LNA range  offset>#
NV_C0_BC0_LNA_4_OFFSET_VS_FREQ_I,1742,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C0_BC0_LNA_4_RISE_I ,1758,ReadWrite,<BYTE,LNA_4_RISE>#
NV_C0_BC0_TX_CAL_CHAN_I,1737,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#
NV_C0_BC0_RX_CAL_CHAN_I,1738,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#
NV_C0_BC0_VGA_GAIN_OFFSET_I,1749,ReadWrite,<SIGNED_WORD,Offset>#
NV_C0_BC0_VGA_GAIN_OFFSET_VS_FREQ_I,1750,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C0_BC1_IM_LEVEL1_I,1681,ReadWrite,<BYTE, InterMod antijamming threshold power level>#
NV_C0_BC1_IM_LEVEL2_I,1682,ReadWrite,<BYTE, InterMod antijamming threshold power level>#
NV_C0_BC1_IM_LEVEL3_I,1683,ReadWrite,<BYTE, InterMod antijamming threshold power level>#
NV_C0_BC1_IM_LEVEL4_I,1684,ReadWrite,<BYTE, InterMod antijamming threshold power level>#
NV_C0_BC1_IM2_I_VALUE_I,1668,ReadWrite,<BYTE, InterMod antijamming setting>#
NV_C0_BC1_IM2_Q_VALUE_I,1669,ReadWrite,<BYTE, InterMod antijamming setting>#
NV_C0_BC1_IM2_TRANSCONDUCTOR_VALUE_I,1672,ReadWrite,<BYTE,Transconductor value>#
NV_C0_BC1_LNA_1_FALL_I ,1674,ReadWrite,<BYTE,LNA_1_FALL>#
NV_C0_BC1_LNA_1_OFFSET_I ,1654,ReadWrite,<SIGNED_WORD, LNA range  offset>#
NV_C0_BC1_LNA_1_OFFSET_VS_FREQ_I,1650,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C0_BC1_LNA_1_RISE_I ,1673,ReadWrite,<BYTE,LNA_1_RISE>#
NV_C0_BC1_LNA_2_FALL_I ,1676,ReadWrite,<BYTE,LNA_2_FALL>#
NV_C0_BC1_LNA_2_OFFSET_I ,1655,ReadWrite,<SIGNED_WORD, LNA range  offset>#
NV_C0_BC1_LNA_2_OFFSET_VS_FREQ_I,1651,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C0_BC1_LNA_2_RISE_I ,1675,ReadWrite,<BYTE,LNA_2_RISE>#
NV_C0_BC1_LNA_3_FALL_I ,1678,ReadWrite,<BYTE,LNA_3_FALL>#
NV_C0_BC1_LNA_3_OFFSET_I ,1666,ReadWrite,<SIGNED_WORD, LNA range  offset>#
NV_C0_BC1_LNA_3_OFFSET_VS_FREQ_I,1652,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C0_BC1_LNA_3_RISE_I ,1677,ReadWrite,<BYTE,LNA_3_RISE>#
NV_C0_BC1_LNA_4_FALL_I ,1680,ReadWrite,<BYTE,LNA_4_FALL>#
NV_C0_BC1_LNA_4_OFFSET_I ,1667,ReadWrite,<SIGNED_WORD, LNA range  offset>#
NV_C0_BC1_LNA_4_OFFSET_VS_FREQ_I,1653,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C0_BC1_LNA_4_RISE_I ,1679,ReadWrite,<BYTE,LNA_4_RISE>#
NV_C0_BC1_TX_CAL_CHAN_I,1648,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#
NV_C0_BC1_RX_CAL_CHAN_I,1649,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#
NV_C0_BC1_VGA_GAIN_OFFSET_I,1670,ReadWrite,<SIGNED_WORD,Offset>#
NV_C0_BC1_VGA_GAIN_OFFSET_VS_FREQ_I,1671,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C0_BC3__VS_FREQ_I,1572,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C0_BC3_IM_LEVEL1_I,1593,ReadWrite,<BYTE, InterMod antijamming threshold power level>#
NV_C0_BC3_IM_LEVEL2_I  ,1594,ReadWrite,<BYTE, InterMod antijamming threshold power level>#
NV_C0_BC3_IM_LEVEL3_I  ,1595,ReadWrite,<BYTE, InterMod antijamming threshold power level>#
NV_C0_BC3_IM_LEVEL4_I  ,1596,ReadWrite,<BYTE, InterMod antijamming threshold power level>#
NV_C0_BC3_IM2_I_VALUE_I,1580,ReadWrite,<BYTE, InterMod antijamming setting>#
NV_C0_BC3_IM2_Q_VALUE_I,1581,ReadWrite,<BYTE, InterMod antijamming setting>#
NV_C0_BC3_IM2_TRANSCONDUCTOR_VALUE_I,1584,ReadWrite,<BYTE,Transconductor value>#
NV_C0_BC3_LNA_1_FALL_I ,1586,ReadWrite,<BYTE,C0_BC3_LNA_1_FALL>#
NV_C0_BC3_LNA_1_OFFSET_I ,1576,ReadWrite,<SIGNED_WORD, LNA range  offset>#
NV_C0_BC3_LNA_1_RISE_I ,1585,ReadWrite,<BYTE,C0_BC3_LNA_1_RISE>#
NV_C0_BC3_LNA_2_FALL_I ,1588,ReadWrite,<BYTE,C0_BC3_LNA_2_FALL>#
NV_C0_BC3_LNA_2_OFFSET_I ,1577,ReadWrite,<SIGNED_WORD, LNA range  offset>#
NV_C0_BC3_LNA_2_OFFSET_VS_FREQ_I,1573,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C0_BC3_LNA_2_RISE_I ,1587,ReadWrite,<BYTE,C0_BC3_LNA_2_RISE>#
NV_C0_BC3_LNA_3_FALL_I ,1590,ReadWrite,<BYTE,C0_BC3_LNA_3_FALL>#
NV_C0_BC3_LNA_3_OFFSET_I ,1578,ReadWrite,<SIGNED_WORD, LNA range  offset>#
NV_C0_BC3_LNA_3_OFFSET_VS_FREQ_I,1574,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C0_BC3_LNA_3_RISE_I ,1589,ReadWrite,<BYTE,C0_BC3_LNA_3_RISE>#
NV_C0_BC3_LNA_4_FALL_I ,1592,ReadWrite,<BYTE,C0_BC3_LNA_4_FALL>#
NV_C0_BC3_LNA_4_OFFSET_I ,1579,ReadWrite,<SIGNED_WORD, LNA range  offset>#
NV_C0_BC3_LNA_4_OFFSET_VS_FREQ_I,1575,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C0_BC3_LNA_4_RISE_I ,1591,ReadWrite,<BYTE,C0_BC3_LNA_4_RISE>#
NV_C0_BC3_TX_CAL_CHAN_I,1570,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#
NV_C0_BC3_RX_CAL_CHAN_I,1571,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#
NV_C0_BC3_VGA_GAIN_OFFSET_I,1582,ReadWrite,<SIGNED_WORD,Offset>#
NV_C0_BC3_VGA_GAIN_OFFSET_VS_FREQ_I,1583,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C0_BC4__VS_FREQ_I,1493,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C0_BC4_IM_LEVEL1_I  ,1514,ReadWrite,<BYTE, InterMod antijamming threshold power level>#
NV_C0_BC4_IM_LEVEL2_I  ,1515,ReadWrite,<BYTE, InterMod antijamming threshold power level>#
NV_C0_BC4_IM_LEVEL3_I  ,1516,ReadWrite,<BYTE, InterMod antijamming threshold power level>#
NV_C0_BC4_IM_LEVEL4_I  ,1517,ReadWrite,<BYTE, InterMod antijamming threshold power level>#
NV_C0_BC4_IM2_I_VALUE_I,1501,ReadWrite,<BYTE, InterMod antijamming setting>#
NV_C0_BC4_IM2_Q_VALUE_I,1502,ReadWrite,<BYTE, InterMod antijamming setting>#
NV_C0_BC4_IM2_TRANSCONDUCTOR_VALUE_I,1505,ReadWrite,<BYTE,Transconductor value>#
NV_C0_BC4_LNA_1_FALL_I ,1507,ReadWrite,<BYTE,C0_BC4_LNA_1_FALL>#
NV_C0_BC4_LNA_1_OFFSET_I ,1497,ReadWrite,<SIGNED_WORD, LNA range  offset>#
NV_C0_BC4_LNA_1_RISE_I ,1506,ReadWrite,<BYTE,C0_BC4_LNA_1_RISE>#
NV_C0_BC4_LNA_2_FALL_I ,1509,ReadWrite,<BYTE,C0_BC4_LNA_2_FALL>#
NV_C0_BC4_LNA_2_OFFSET_I ,1498,ReadWrite,<SIGNED_WORD, LNA range  offset>#
NV_C0_BC4_LNA_2_OFFSET_VS_FREQ_I,1494,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C0_BC4_LNA_2_RISE_I ,1508,ReadWrite,<BYTE,C0_BC4_LNA_2_RISE>#
NV_C0_BC4_LNA_3_FALL_I ,1511,ReadWrite,<BYTE,C0_BC4_LNA_3_RISE>#
NV_C0_BC4_LNA_3_OFFSET_I ,1499,ReadWrite,<SIGNED_WORD, LNA range  offset>#
NV_C0_BC4_LNA_3_OFFSET_VS_FREQ_I,1495,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C0_BC4_LNA_3_RISE_I ,1510,ReadWrite,<BYTE,C0_BC4_LNA_3_RISE>#
NV_C0_BC4_LNA_4_FALL_I ,1513,ReadWrite,<BYTE,C0_BC4_LNA_4_RISE>#
NV_C0_BC4_LNA_4_OFFSET_I ,1500,ReadWrite,<SIGNED_WORD, LNA range  offset>#
NV_C0_BC4_LNA_4_OFFSET_VS_FREQ_I,1496,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C0_BC4_LNA_4_RISE_I ,1512,ReadWrite,<BYTE,C0_BC4_LNA_4_RISE>#
NV_C0_BC4_TX_CAL_CHAN_I,1491,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#
NV_C0_BC4_RX_CAL_CHAN_I,1492,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#
NV_C0_BC4_VGA_GAIN_OFFSET_I,1503,ReadWrite,<SIGNED_WORD,Offset>#
NV_C0_BC4_VGA_GAIN_OFFSET_VS_FREQ_I,1504,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C0_BC5_IM_LEVEL1_I  ,1436,ReadWrite,<BYTE, InterMod antijamming threshold power level>#
NV_C0_BC5_IM_LEVEL2_I  ,1437,ReadWrite,<BYTE, InterMod antijamming threshold power level>#
NV_C0_BC5_IM_LEVEL3_I  ,1438,ReadWrite,<BYTE, InterMod antijamming threshold power level>#
NV_C0_BC5_IM_LEVEL4_I  ,1439,ReadWrite,<BYTE, InterMod antijamming threshold power level>#
NV_C0_BC5_IM2_I_VALUE_I,1423,ReadWrite,<BYTE, InterMod antijamming setting>#
NV_C0_BC5_IM2_Q_VALUE_I,1424,ReadWrite,<BYTE, InterMod antijamming setting>#
NV_C0_BC5_IM2_TRANSCONDUCTOR_VALUE_I,1427,ReadWrite,<BYTE,Transconductor value>#
NV_C0_BC5_LNA_1_FALL_I ,1429,ReadWrite,<BYTE,CO_BC5_LNA_1_FALL>#
NV_C0_BC5_LNA_1_OFFSET_I ,1419,ReadWrite,<SIGNED_WORD, LNA range  offset>#
NV_C0_BC5_LNA_1_OFFSET_VS_FREQ_I,1415,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C0_BC5_LNA_1_RISE_I ,1428,ReadWrite,<BYTE,CO_BC5_LNA_1_RISE>#
NV_C0_BC5_LNA_2_FALL_I ,1431,ReadWrite,<BYTE,CO_BC5_LNA_2_FALL>#
NV_C0_BC5_LNA_2_OFFSET_I ,1420,ReadWrite,<SIGNED_WORD, LNA range  offset>#
NV_C0_BC5_LNA_2_OFFSET_VS_FREQ_I,1416,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C0_BC5_LNA_2_RISE_I ,1430,ReadWrite,<BYTE,CO_BC5_LNA_2_RISE>#
NV_C0_BC5_LNA_3_FALL_I ,1433,ReadWrite,<BYTE,CO_BC5_LNA_3_FALL>#
NV_C0_BC5_LNA_3_OFFSET_I ,1421,ReadWrite,<SIGNED_WORD, LNA range  offset>#
NV_C0_BC5_LNA_3_OFFSET_VS_FREQ_I,1417,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C0_BC5_LNA_3_RISE_I ,1432,ReadWrite,<BYTE,CO_BC5_LNA_3_RISE>#
NV_C0_BC5_LNA_4_FALL_I ,1435,ReadWrite,<BYTE,CO_BC5_LNA_4_RISE>#
NV_C0_BC5_LNA_4_OFFSET_I ,1422,ReadWrite,<SIGNED_WORD, LNA range offset>#
NV_C0_BC5_LNA_4_OFFSET_VS_FREQ_I,1418,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C0_BC5_LNA_4_RISE_I ,1434,ReadWrite,<BYTE,CO_BC5_LNA_4_RISE>#
NV_C0_BC5_TX_CAL_CHAN_I,1413,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#
NV_C0_BC5_RX_CAL_CHAN_I,1414,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#
NV_C0_BC5_VGA_GAIN_OFFSET_I,1425,ReadWrite,<SIGNED_WORD,Offset>#
NV_C0_BC5_VGA_GAIN_OFFSET_VS_FREQ_I,1426,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C0_BC6_DIGITAL_MIS_COMP_A_OFFSET_I,1266,ReadWrite,<SIGNED_DWORD,Offset>#
NV_C0_BC6_DIGITAL_MIS_COMP_B_OFFSET_I,1268,ReadWrite,<SIGNED_DWORD,Offset>#
NV_C0_BC6_IM_LEVEL1_I  ,1230,ReadWrite,<BYTE, InterMod antijamming threshold power level>#
NV_C0_BC6_IM_LEVEL2_I  ,1231,ReadWrite,<BYTE,InterMod antijamming threshold power level>#
NV_C0_BC6_IM_LEVEL3_I  ,1232,ReadWrite,<BYTE, InterMod antijamming threshold power level>#
NV_C0_BC6_IM_LEVEL4_I  ,1233,ReadWrite,<BYTE, InterMod antijamming threshold power level>#
NV_C0_BC6_IM2_I_VALUE_I,1251,ReadWrite,<BYTE, InterMod antijamming setting>#
NV_C0_BC6_IM2_Q_VALUE_I,1253,ReadWrite,<BYTE, InterMod antijamming setting>#
NV_C0_BC6_IM2_TRANSCONDUCTOR_VALUE_I,1270,ReadWrite,<BYTE,Transconductor value>#
NV_C0_BC6_LNA_1_FALL_I ,1364,ReadWrite,<BYTE,CO_BC6_LNA_1_FALL>#
NV_C0_BC6_LNA_1_OFFSET_I ,1360,ReadWrite,<SIGNED_WORD, LNA range 1 offset>#
NV_C0_BC6_LNA_1_OFFSET_VS_FREQ_I,1234,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C0_BC6_LNA_1_RISE_I ,1363,ReadWrite,<BYTE,CO_BC6_LNA_1_RISE>#
NV_C0_BC6_LNA_2_FALL_I ,1366,ReadWrite,<BYTE,CO_BC6_LNA_2_FALL>#
NV_C0_BC6_LNA_2_OFFSET_I ,1361,ReadWrite,<SIGNED_WORD, LNA range 2 offset>#
NV_C0_BC6_LNA_2_OFFSET_VS_FREQ_I,1359,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C0_BC6_LNA_2_RISE_I ,1365,ReadWrite,<BYTE,CO_BC6_LNA_2_RISE>#
NV_C0_BC6_LNA_3_FALL_I ,1368,ReadWrite,<BYTE,CO_BC6_LNA_3_FALL>#
NV_C0_BC6_LNA_3_OFFSET_I ,1362,ReadWrite,<SIGNED_WORD, LNA range 3 offset>#
NV_C0_BC6_LNA_3_OFFSET_VS_FREQ_I,1245,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C0_BC6_LNA_3_RISE_I ,1367,ReadWrite,<BYTE,CO_BC6_LNA_3_RISE>#
NV_C0_BC6_LNA_4_FALL_I ,1370,ReadWrite,<BYTE,CO_BC6_LNA_4_FALL>#
NV_C0_BC6_LNA_4_OFFSET_I ,1249,ReadWrite,<SIGNED_WORD,Offset added to Receive >#
NV_C0_BC6_LNA_4_OFFSET_VS_FREQ_I,1262,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C0_BC6_LNA_4_RISE_I ,1369,ReadWrite,<BYTE,CO_BC6_LNA_4_RISE>#
NV_C0_BC6_LNA_RANGE_OFFSET_I,1225,ReadWrite,<WORD,LNA range offset>#
NV_C0_BC6_P1_RISE_FALL_OFFSET_I ,1264,ReadWrite,<BYTE,Array[0]>#<BYTE,Array[1]>#<BYTE,Array[2]>#<BYTE,Array[3]>#<BYTE,Array[4]>#<BYTE,Array[5]>#<BYTE,Array[6]>#<BYTE,Array[7]>#
NV_C0_BC6_TX_CAL_CHAN_I,1306,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#
NV_C0_BC6_RX_CAL_CHAN_I,1211,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#
NV_C0_BC6_VGA_GAIN_OFFSET_I,1255,ReadWrite,<SIGNED_WORD,Offset>#
NV_C0_BC6_VGA_GAIN_OFFSET_VS_FREQ_I,1257,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C0_BC6_VGA_GAIN_OFFSET_VS_TEMP_I,1259,ReadWrite,<SIGNED_WORD,Array[0]>#<SIGNED_WORD,Array[1]>#<SIGNED_WORD,Array[2]>#<SIGNED_WORD,Array[3]>#<SIGNED_WORD,Array[4]>#<SIGNED_WORD,Array[5]>#<SIGNED_WORD,Array[6]>#<SIGNED_WORD,Array[7]>#<SIGNED_WORD,Array[8]>#<SIGNED_WORD,Array[9]>#<SIGNED_WORD,Array[10]>#<SIGNED_WORD,Array[11]>#<SIGNED_WORD,Array[12]>#<SIGNED_WORD,Array[13]>#<SIGNED_WORD,Array[14]>#<SIGNED_WORD,Array[15]>#
NV_C1_BC0_IM_LEVEL1_I  ,1787,ReadWrite,<BYTE, InterMod antijamming threshold power level>#
NV_C1_BC0_IM_LEVEL2_I  ,1788,ReadWrite,<BYTE, InterMod antijamming threshold power level>#
NV_C1_BC0_IM_LEVEL3_I  ,1789,ReadWrite,<BYTE, InterMod antijamming threshold power level>#
NV_C1_BC0_IM_LEVEL4_I  ,1790, ReadWrite,<BYTE, InterMod antijamming threshold power level>#
NV_C1_BC0_IM2_I_VALUE_I,1774,ReadWrite,<BYTE, InterMod antijamming setting>#
NV_C1_BC0_IM2_Q_VALUE_I,1775,ReadWrite,<BYTE, InterMod antijamming setting>#
NV_C1_BC0_IM2_TRANSCONDUCTOR_VALUE_I,1778,ReadWrite,<BYTE,Transconductor value>#
NV_C1_BC0_LNA_1_FALL_I ,1780,ReadWrite,<BYTE,LNA_1_FALL>#
NV_C1_BC0_LNA_1_OFFSET_I ,1770,ReadWrite,<SIGNED_WORD, LNA range offset>#
NV_C1_BC0_LNA_1_OFFSET_VS_FREQ_I,1766,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C1_BC0_LNA_1_RISE_I ,1779,ReadWrite,<BYTE,LNA_1_RISE>#
NV_C1_BC0_LNA_2_FALL_I ,1782,ReadWrite,<BYTE,LNA_2_FALL>#
NV_C1_BC0_LNA_2_OFFSET_I ,1771,ReadWrite,<SIGNED_WORD, LNA range  offset>#
NV_C1_BC0_LNA_2_OFFSET_VS_FREQ_I,1767,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C1_BC0_LNA_2_RISE_I ,1781,ReadWrite,<BYTE,LNA_2_RISE>#
NV_C1_BC0_LNA_3_FALL_I ,1784,ReadWrite,<BYTE,LNA_3_FALL>#
NV_C1_BC0_LNA_3_OFFSET_I ,1772,ReadWrite,<SIGNED_WORD, LNA range  offset>#
NV_C1_BC0_LNA_3_OFFSET_VS_FREQ_I,1768,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C1_BC0_LNA_3_RISE_I ,1783,ReadWrite,<BYTE,LNA_3_RISE>#
NV_C1_BC0_LNA_4_FALL_I ,1786,ReadWrite,<BYTE,LNA_4_FALL>#
NV_C1_BC0_LNA_4_OFFSET_I ,1773,ReadWrite,<SIGNED_WORD, LNA range  offset>#
NV_C1_BC0_LNA_4_OFFSET_VS_FREQ_I,1769,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C1_BC0_LNA_4_RISE_I ,1785,ReadWrite,<BYTE,LNA_4_RISE>#
NV_C1_BC0_TX_CAL_CHAN_I,1764,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#
NV_C1_BC0_RX_CAL_CHAN_I,1765,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#
NV_C1_BC0_VGA_GAIN_OFFSET_I,1776,ReadWrite,<SIGNED_WORD,Offset>#
NV_C1_BC0_VGA_GAIN_OFFSET_VS_FREQ_I,1777,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C1_BC1_IM_LEVEL1_I  ,1709,ReadWrite,<BYTE, InterMod antijamming threshold power level>#
NV_C1_BC1_IM_LEVEL2_I  ,1710,ReadWrite,<BYTE, InterMod antijamming threshold power level>#
NV_C1_BC1_IM_LEVEL3_I  ,1711,ReadWrite,<BYTE, InterMod antijamming threshold power level>#
NV_C1_BC1_IM_LEVEL4_I  ,1712,ReadWrite,<BYTE, InterMod antijamming threshold power level>#
NV_C1_BC1_IM2_I_VALUE_I,1696,ReadWrite,<BYTE, InterMod antijamming setting>#
NV_C1_BC1_IM2_Q_VALUE_I,1697,ReadWrite,<BYTE, InterMod antijamming setting>#
NV_C1_BC1_IM2_TRANSCONDUCTOR_VALUE_I,1700,ReadWrite,<BYTE,Transconductor value>#
NV_C1_BC1_LNA_1_FALL_I ,1702,ReadWrite,<BYTE,LNA_1_FALL>#
NV_C1_BC1_LNA_1_OFFSET_I ,1692,ReadWrite,<SIGNED_WORD, LNA range  offset>#
NV_C1_BC1_LNA_1_OFFSET_VS_FREQ_I,1687,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C1_BC1_LNA_1_RISE_I ,1701,ReadWrite,<BYTE,LNA_1_RISE>#
NV_C1_BC1_LNA_2_FALL_I ,1704,ReadWrite,<BYTE,LNA_2_FALL>#
NV_C1_BC1_LNA_2_OFFSET_I ,1693,ReadWrite,<SIGNED_WORD, LNA range  offset>#
NV_C1_BC1_LNA_2_OFFSET_VS_FREQ_I,1689,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C1_BC1_LNA_2_RISE_I ,1703,ReadWrite,<BYTE,LNA_2_RISE>#
NV_C1_BC1_LNA_3_FALL_I ,1706,ReadWrite,<BYTE,LNA_3_FALL>#
NV_C1_BC1_LNA_3_OFFSET_I ,1694,ReadWrite,<SIGNED_WORD, LNA range  offset>#
NV_C1_BC1_LNA_3_OFFSET_VS_FREQ_I,1690,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C1_BC1_LNA_3_RISE_I ,1705,ReadWrite,<BYTE,LNA_3_RISE>#
NV_C1_BC1_LNA_4_FALL_I ,1708,ReadWrite,<BYTE,LNA_4_FALL>#
NV_C1_BC1_LNA_4_OFFSET_I ,1695,ReadWrite,<SIGNED_WORD, LNA range  offset>#
NV_C1_BC1_LNA_4_OFFSET_VS_FREQ_I,1691,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C1_BC1_LNA_4_RISE_I ,1707,ReadWrite,<BYTE,LNA_4_RISE>#
NV_C1_BC1_TX_CAL_CHAN_I,1685,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#
NV_C1_BC1_RX_CAL_CHAN_I,1686,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#
NV_C1_BC1_VGA_GAIN_OFFSET_I,1698,ReadWrite,<SIGNED_WORD, LNA range  offset>#
NV_C1_BC1_VGA_GAIN_OFFSET_VS_FREQ_I,1699,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C1_BC3_IM_LEVEL1_I  ,1620,ReadWrite,<BYTE, InterMod antijamming threshold power level>#
NV_C1_BC3_IM_LEVEL2_I  ,1621,ReadWrite,<BYTE, InterMod antijamming threshold power level>#
NV_C1_BC3_IM_LEVEL3_I  ,1622,ReadWrite,<BYTE, InterMod antijamming threshold power level>#
NV_C1_BC3_IM_LEVEL4_I  ,1623,ReadWrite,<BYTE, InterMod antijamming threshold power level>#
NV_C1_BC3_IM2_I_VALUE_I,1607,ReadWrite,<BYTE, InterMod antijamming setting>#
NV_C1_BC3_IM2_Q_VALUE_I,1608,ReadWrite,<BYTE, InterMod antijamming setting>#
NV_C1_BC3_IM2_TRANSCONDUCTOR_VALUE_I,1611,ReadWrite,<BYTE,Transconductor value>#
NV_C1_BC3_LNA_1_FALL_I ,1613,ReadWrite,<BYTE,LNA_1_FALL>#
NV_C1_BC3_LNA_1_OFFSET_I ,1603,ReadWrite,<SIGNED_WORD, LNA range  offset>#
NV_C1_BC3_LNA_1_OFFSET_VS_FREQ_I,1599,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C1_BC3_LNA_1_RISE_I ,1612,ReadWrite,<BYTE,LNA_1_RISE>#
NV_C1_BC3_LNA_2_FALL_I ,1615,ReadWrite,<BYTE,LNA_2_FALL>#
NV_C1_BC3_LNA_2_OFFSET_I ,1604,ReadWrite,<SIGNED_WORD, LNA range  offset>#
NV_C1_BC3_LNA_2_OFFSET_VS_FREQ_I,1600,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C1_BC3_LNA_2_RISE_I ,1614,ReadWrite,<BYTE,LNA_2_RISE>#
NV_C1_BC3_LNA_3_FALL_I ,1617,ReadWrite,<BYTE,LNA_3_FALL>#
NV_C1_BC3_LNA_3_OFFSET_I ,1605,ReadWrite,<SIGNED_WORD, LNA range  offset>#
NV_C1_BC3_LNA_3_OFFSET_VS_FREQ_I,1601,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C1_BC3_LNA_3_RISE_I ,1616,ReadWrite,<BYTE,LNA_3_RISE>#
NV_C1_BC3_LNA_4_FALL_I ,1619,ReadWrite,<BYTE,LNA_4_FALL>#
NV_C1_BC3_LNA_4_OFFSET_I ,1606,ReadWrite,<SIGNED_WORD, LNA range  offset>#
NV_C1_BC3_LNA_4_OFFSET_VS_FREQ_I,1602,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C1_BC3_LNA_4_RISE_I ,1618,ReadWrite,<BYTE,LNA_4_RISE>#
NV_C1_BC3_TX_CAL_CHAN_I,1597,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#
NV_C1_BC3_RX_CAL_CHAN_I,1598,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#
NV_C1_BC3_VGA_GAIN_OFFSET_I,1609,ReadWrite,<SIGNED_WORD,Offset>#
NV_C1_BC3_VGA_GAIN_OFFSET_VS_FREQ_I,1610,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C1_BC4_IM_LEVEL1_I  ,1541,ReadWrite,<BYTE, InterMod antijamming threshold power level>#
NV_C1_BC4_IM_LEVEL2_I  ,1542,ReadWrite,<BYTE, InterMod antijamming threshold power level>#
NV_C1_BC4_IM_LEVEL3_I  ,1543,ReadWrite,<BYTE, InterMod antijamming threshold power level>#
NV_C1_BC4_IM_LEVEL4_I  ,1544,ReadWrite,<BYTE, InterMod antijamming threshold power level>#
NV_C1_BC4_IM2_I_VALUE_I,1528,ReadWrite,<BYTE, InterMod antijamming setting>#
NV_C1_BC4_IM2_Q_VALUE_I,1529,ReadWrite,<BYTE, InterMod antijamming setting>#
NV_C1_BC4_IM2_TRANSCONDUCTOR_VALUE_I,1532,ReadWrite,<BYTE,Transconductor value>#
NV_C1_BC4_LNA_1_FALL_I ,1534,ReadWrite,<BYTE,C1_BC4_LNA_1_FALL>#
NV_C1_BC4_LNA_1_OFFSET_I ,1524,ReadWrite,<SIGNED_WORD, LNA range  offset>#
NV_C1_BC4_LNA_1_OFFSET_VS_FREQ_I,1520,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C1_BC4_LNA_1_RISE_I ,1533,ReadWrite,<BYTE,C1_BC4_LNA_1_RISE>#
NV_C1_BC4_LNA_2_FALL_I ,1536,ReadWrite,<BYTE,C1_BC4_LNA_2_FALL>#
NV_C1_BC4_LNA_2_OFFSET_I ,1525,ReadWrite,<SIGNED_WORD, LNA range  offset>#
NV_C1_BC4_LNA_2_OFFSET_VS_FREQ_I,1521,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C1_BC4_LNA_2_RISE_I ,1535,ReadWrite,<BYTE,C1_BC4_LNA_2_RISE>#
NV_C1_BC4_LNA_3_FALL_I ,1538,ReadWrite,<BYTE,C1_BC4_LNA_3_RISE>#
NV_C1_BC4_LNA_3_OFFSET_I ,1526,ReadWrite,<SIGNED_WORD, LNA range  offset>#
NV_C1_BC4_LNA_3_OFFSET_VS_FREQ_I,1522,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C1_BC4_LNA_3_RISE_I ,1537,ReadWrite,<BYTE,C1_BC4_LNA_3_RISE>#
NV_C1_BC4_LNA_4_FALL_I ,1540,ReadWrite,<BYTE,C1_BC4_LNA_4_RISE>#
NV_C1_BC4_LNA_4_OFFSET_I ,1527,ReadWrite,<SIGNED_WORD, LNA range  offset>#
NV_C1_BC4_LNA_4_OFFSET_VS_FREQ_I,1523,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C1_BC4_LNA_4_RISE_I ,1539,ReadWrite,<BYTE,C1_BC4_LNA_4_RISE>#
NV_C1_BC4_TX_CAL_CHAN_I,1518,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#
NV_C1_BC4_RX_CAL_CHAN_I,1519,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#
NV_C1_BC4_VGA_GAIN_OFFSET_I,1530,ReadWrite,<SIGNED_WORD,Offset>#
NV_C1_BC4_VGA_GAIN_OFFSET_VS_FREQ_I,1531,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C1_BC5_IM_LEVEL1_I  ,1463,ReadWrite,<BYTE, InterMod antijamming threshold power level>#
NV_C1_BC5_IM_LEVEL2_I  ,1464,ReadWrite,<BYTE, InterMod antijamming threshold power level>#
NV_C1_BC5_IM_LEVEL3_I  ,1465,ReadWrite,<BYTE, InterMod antijamming threshold power level>#
NV_C1_BC5_IM_LEVEL4_I  ,1466,ReadWrite,<BYTE, InterMod antijamming threshold power level>#
NV_C1_BC5_IM2_I_VALUE_I,1450,ReadWrite,<BYTE, InterMod antijamming setting>#
NV_C1_BC5_IM2_Q_VALUE_I,1451,ReadWrite,<BYTE, InterMod antijamming setting>#
NV_C1_BC5_IM2_TRANSCONDUCTOR_VALUE_I,1454,ReadWrite,<BYTE,Transconductor value>#
NV_C1_BC5_LNA_1_FALL_I ,1456,ReadWrite,<BYTE,C1_BC5_LNA_1_FALL>#
NV_C1_BC5_LNA_1_OFFSET_I ,1446,ReadWrite,<SIGNED_WORD, LNA range  offset>#
NV_C1_BC5_LNA_1_OFFSET_VS_FREQ_I,1442,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C1_BC5_LNA_1_RISE_I ,1455,ReadWrite,<BYTE,C1_BC5_LNA_1_RISE>#
NV_C1_BC5_LNA_2_FALL_I ,1458,ReadWrite,<BYTE,C1_BC5_LNA_2_FALL>#
NV_C1_BC5_LNA_2_OFFSET_I ,1447,ReadWrite,<SIGNED_WORD, LNA range  offset>#
NV_C1_BC5_LNA_2_OFFSET_VS_FREQ_I,1443,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C1_BC5_LNA_2_RISE_I ,1457,ReadWrite,<BYTE,C1_BC5_LNA_2_RISE>#
NV_C1_BC5_LNA_3_FALL_I ,1460,ReadWrite,<BYTE,C1_BC5_LNA_3_FALL>#
NV_C1_BC5_LNA_3_OFFSET_I ,1448,ReadWrite,<SIGNED_WORD, LNA range  offset>#
NV_C1_BC5_LNA_3_OFFSET_VS_FREQ_I,1444,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C1_BC5_LNA_3_RISE_I ,1459,ReadWrite,<BYTE,C1_BC5_LNA_3_RISE>#
NV_C1_BC5_LNA_4_FALL_I ,1462,ReadWrite,<BYTE,C1_BC5_LNA_4_RISE>#
NV_C1_BC5_LNA_4_OFFSET_I ,1449,ReadWrite,<SIGNED_WORD, LNA range  offset>#
NV_C1_BC5_LNA_4_OFFSET_VS_FREQ_I,1445,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C1_BC5_LNA_4_RISE_I ,1461,ReadWrite,<BYTE,C1_BC5_LNA_4_RISE>#
NV_C1_BC5_TX_CAL_CHAN_I,1440,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#
NV_C1_BC5_RX_CAL_CHAN_I,1441,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#
NV_C1_BC5_VGA_GAIN_OFFSET_I,1452,ReadWrite,<SIGNED_WORD,Offset>#
NV_C1_BC5_VGA_GAIN_OFFSET_VS_FREQ_I,1453,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C1_BC6_DIGITAL_MIS_COMP_A_OFFSET_I,1267,ReadWrite,<SIGNED_DWORD,Offset>#
NV_C1_BC6_DIGITAL_MIS_COMP_B_OFFSET_I,1269,ReadWrite,<SIGNED_DWORD,Offset>#
NV_C1_BC6_IM_LEVEL1_I  ,1385,ReadWrite,<BYTE, InterMod antijamming threshold power level>#
NV_C1_BC6_IM_LEVEL2_I  ,1386,ReadWrite,<BYTE, InterMod antijamming threshold power level>#
NV_C1_BC6_IM_LEVEL3_I  ,1387,ReadWrite,<BYTE, InterMod antijamming threshold power level>#
NV_C1_BC6_IM_LEVEL4_I  ,1388,ReadWrite,<BYTE, InterMod antijamming threshold power level>#
NV_C1_BC6_IM2_I_VALUE_I,1252,ReadWrite,<BYTE, InterMod antijamming setting>#
NV_C1_BC6_IM2_Q_VALUE_I,1254,ReadWrite,<BYTE, InterMod antijamming setting>#
NV_C1_BC6_IM2_TRANSCONDUCTOR_VALUE_I,1271,ReadWrite,<BYTE,Transconductor value>#
NV_C1_BC6_LNA_1_FALL_I ,1378,ReadWrite,<BYTE,C1_BC6_LNA_1_FALL>#
NV_C1_BC6_LNA_1_OFFSET_I ,1374,ReadWrite,<SIGNED_WORD, LNA range 1 offset>#
NV_C1_BC6_LNA_1_OFFSET_VS_FREQ_I,1235,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C1_BC6_LNA_1_RISE_I ,1377,ReadWrite,<BYTE,C1_BC6_LNA_1_RISE>#
NV_C1_BC6_LNA_2_FALL_I ,1380,ReadWrite,<BYTE,C1_BC6_LNA_2_FALL>#
NV_C1_BC6_LNA_2_OFFSET_I ,1375,ReadWrite,<SIGNED_WORD, LNA range 1 offset>#
NV_C1_BC6_LNA_2_OFFSET_VS_FREQ_I,1373,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C1_BC6_LNA_2_RISE_I ,1379,ReadWrite,<BYTE,C1_BC6_LNA_2_RISE>#
NV_C1_BC6_LNA_3_FALL_I ,1382,ReadWrite,<BYTE,C1_BC6_LNA_3_FALL>#
NV_C1_BC6_LNA_3_OFFSET_I ,1376,ReadWrite,<SIGNED_WORD, LNA range 1 offset>#
NV_C1_BC6_LNA_3_OFFSET_VS_FREQ_I,1246,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C1_BC6_LNA_3_RISE_I ,1381,ReadWrite,<BYTE,C1_BC6_LNA_3_RISE>#
NV_C1_BC6_LNA_4_FALL_I ,1384,ReadWrite,<BYTE,C1_BC6_LNA_4_FALL>#
NV_C1_BC6_LNA_4_OFFSET_I ,1250,ReadWrite,<SIGNED_WORD,Offset added to Receive >#
NV_C1_BC6_LNA_4_OFFSET_VS_FREQ_I,1263,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C1_BC6_LNA_4_RISE_I ,1383,ReadWrite,<BYTE,C1_BC6_LNA_4_RISE>#
NV_C1_BC6_LNA_RANGE_OFFSET_I,1226,ReadWrite,<WORD,LNA range offset>#
NV_C1_BC6_P1_RISE_FALL_OFFSET_I ,1265,ReadWrite,<BYTE,Array[0]>#<BYTE,Array[1]>#<BYTE,Array[2]>#<BYTE,Array[3]>#<BYTE,Array[4]>#<BYTE,Array[5]>#<BYTE,Array[6]>#<BYTE,Array[7]>#
NV_C1_BC6_TX_CAL_CHAN_I,1371,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#
NV_C1_BC6_RX_CAL_CHAN_I,1372,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#
NV_C1_BC6_VGA_GAIN_OFFSET_I,1256,ReadWrite,<SIGNED_WORD,Offset>#
NV_C1_BC6_VGA_GAIN_OFFSET_VS_FREQ_I,1258,ReadWrite,<SIGNED_BYTE,Array[0]>#<SIGNED_BYTE,Array[1]>#<SIGNED_BYTE,Array[2]>#<SIGNED_BYTE,Array[3]>#<SIGNED_BYTE,Array[4]>#<SIGNED_BYTE,Array[5]>#<SIGNED_BYTE,Array[6]>#<SIGNED_BYTE,Array[7]>#<SIGNED_BYTE,Array[8]>#<SIGNED_BYTE,Array[9]>#<SIGNED_BYTE,Array[10]>#<SIGNED_BYTE,Array[11]>#<SIGNED_BYTE,Array[12]>#<SIGNED_BYTE,Array[13]>#<SIGNED_BYTE,Array[14]>#<SIGNED_BYTE,Array[15]>#
NV_C1_BC6_VGA_GAIN_OFFSET_VS_TEMP_I,1260,ReadWrite,<SIGNED_WORD,Array[0]>#<SIGNED_WORD,Array[1]>#<SIGNED_WORD,Array[2]>#<SIGNED_WORD,Array[3]>#<SIGNED_WORD,Array[4]>#<SIGNED_WORD,Array[5]>#<SIGNED_WORD,Array[6]>#<SIGNED_WORD,Array[7]>#<SIGNED_WORD,Array[8]>#<SIGNED_WORD,Array[9]>#<SIGNED_WORD,Array[10]>#<SIGNED_WORD,Array[11]>#<SIGNED_WORD,Array[12]>#<SIGNED_WORD,Array[13]>#<SIGNED_WORD,Array[14]>#<SIGNED_WORD,Array[15]>#
NV_CDMA_TX_CAL_CHAN_I,1307,ReadWrite,<WORD,Channel 0>#<WORD,Channel 1>#<WORD,Channel 2>#<WORD,Channel 3>#<WORD,Channel 4>#<WORD,Channel 5>#<WORD,Channel 6>#<WORD,Channel 7>#<WORD,Channel 8>#<WORD,Channel 9>#<WORD,Channel 10>#<WORD,Channel 11>#<WORD,Channel 12>#<WORD,Channel 13>#<WORD,Channel 14>#<WORD,Channel 15>#
NV_CDMA_RX_CAL_CHAN_I,1308,ReadWrite,<WORD,Channel 0>#<WORD,Channel 1>#<WORD,Channel 2>#<WORD,Channel 3>#<WORD,Channel 4>#<WORD,Channel 5>#<WORD,Channel 6>#<WORD,Channel 7>#<WORD,Channel 8>#<WORD,Channel 9>#<WORD,Channel 10>#<WORD,Channel 11>#<WORD,Channel 12>#<WORD,Channel 13>#<WORD,Channel 14>#<WORD,Channel 15>#
NV_PCS_RX_CAL_CHAN_I,1309,ReadWrite,<WORD,Channel 0>#<WORD,Channel 1>#<WORD,Channel 2>#<WORD,Channel 3>#<WORD,Channel 4>#<WORD,Channel 5>#<WORD,Channel 6>#<WORD,Channel 7>#<WORD,Channel 8>#<WORD,Channel 9>#<WORD,Channel 10>#<WORD,Channel 11>#<WORD,Channel 12>#<WORD,Channel 13>#<WORD,Channel 14>#<WORD,Channel 15>#
NV_PCS_TX_CAL_CHAN_I,1310,ReadWrite,<WORD,Channel 0>#<WORD,Channel 1>#<WORD,Channel 2>#<WORD,Channel 3>#<WORD,Channel 4>#<WORD,Channel 5>#<WORD,Channel 6>#<WORD,Channel 7>#<WORD,Channel 8>#<WORD,Channel 9>#<WORD,Channel 10>#<WORD,Channel 11>#<WORD,Channel 12>#<WORD,Channel 13>#<WORD,Channel 14>#<WORD,Channel 15>#
NV_WCDMA_1900_AGC_PA_ON_FALL_DELAY_I ,1202,ReadWrite,<WORD,_AGC_PA_ON_fall_DELAY>#
NV_WCDMA_1900_AGC_PA_ON_RISE_DELAY_I ,1201,ReadWrite,<WORD,_AGC_PA_ON_RISE_DELAY>#
NV_WCDMA_1900_AGC_TX_ON_FALL_DELAY_I ,1204,ReadWrite,<WORD,_AGC_PA_ON_fall_DELAY>#
NV_WCDMA_1900_AGC_TX_ON_RISE_DELAY_I ,1203,ReadWrite,<WORD,_AGC_PA_ON_RISE_DELAY>#
NV_WCDMA_1900_AGC_UPDATE_TX_AGC_TIME_I ,1205,ReadWrite,<WORD,_AGC_PA_ON_RISE_DELAY>#
NV_WCDMA_AGC_PA_ON_FALL_DELAY_I , 1197,ReadWrite,<WORD,_AGC_PA_ON_fall_DELAY>#
NV_WCDMA_AGC_PA_ON_RISE_DELAY_I ,1196,ReadWrite,<WORD,_AGC_PA_ON_RISE_DELAY>#
NV_WCDMA_AGC_TX_ON_FALL_DELAY_I , 1199,ReadWrite,<WORD,_AGC_tx_ON_fall_DELAY>#
NV_WCDMA_AGC_TX_ON_RISE_DELAY_I , 1198,ReadWrite,<WORD,_AGC_tx_ON_RISE_DELAY>#
NV_WCDMA_AGC_UPDATE_TX_AGC_TIME_I ,1200,ReadWrite,<WORD,AGC_UPDATE_TX_AGC_TIME>#
NV_WCDMA_800_VGA_GAIN_OFFSET_I,1814,ReadWrite,<SIGNED_WORD,Offset>#
NV_WCDMA_800_VGA_GAIN_OFFSET_VS_FREQ_I,1815,ReadWrite,<SIGNED_BYTE,Array 0>#<SIGNED_BYTE,Array 1>#<SIGNED_BYTE,Array 2>#<SIGNED_BYTE,Array 3>#<SIGNED_BYTE,Array 4>#<SIGNED_BYTE,Array 5>#<SIGNED_BYTE,Array 6>#<SIGNED_BYTE,Array 7>#<SIGNED_BYTE,Array 8>#<SIGNED_BYTE,Array 9>#<SIGNED_BYTE,Array 10>#<SIGNED_BYTE,Array 11>#<SIGNED_BYTE,Array 12>#<SIGNED_BYTE,Array 13>#<SIGNED_BYTE,Array 14>#<SIGNED_BYTE,Array 15>#
NV_WCDMA_800_VGA_GAIN_OFFSET_VS_TEMP_I,1816,ReadWrite,<SIGNED_BYTE,Array 0>#<SIGNED_BYTE,Array 1>#<SIGNED_BYTE,Array 2>#<SIGNED_BYTE,Array 3>#<SIGNED_BYTE,Array 4>#<SIGNED_BYTE,Array 5>#<SIGNED_BYTE,Array 6>#<SIGNED_BYTE,Array 7>#<SIGNED_BYTE,Array 8>#<SIGNED_BYTE,Array 9>#<SIGNED_BYTE,Array 10>#<SIGNED_BYTE,Array 11>#<SIGNED_BYTE,Array 12>#<SIGNED_BYTE,Array 13>#<SIGNED_BYTE,Array 14>#<SIGNED_BYTE,Array 15>#
NV_WCDMA_800_LNA_RANGE_RISE_2_I,1817,ReadWrite,<SIGNED_WORD,Rise Value>#
NV_WCDMA_800_LNA_RANGE_RISE_3_I,1818,ReadWrite,<SIGNED_WORD,Rise Value>#
NV_WCDMA_800_LNA_RANGE_FALL_2_I,1819,ReadWrite,<SIGNED_WORD,Fall Value>#
NV_WCDMA_800_LNA_RANGE_FALL_3_I,1820,ReadWrite,<SIGNED_WORD,Fall Value>#
NV_WCDMA_800_IM_LEVEL_2_I,1821,ReadWrite,<SIGNED_WORD,IM Level>#
NV_WCDMA_800_IM_LEVEL_3_I,1822,ReadWrite,<SIGNED_WORD,IM Level>#
NV_WCDMA_800_LNA_RANGE_OFFSET_2_I,1823,ReadWrite,<SIGNED_WORD,Offset>#
NV_WCDMA_800_LNA_RANGE_OFFSET_3_I,1824,ReadWrite,<SIGNED_WORD,Offset>#
NV_WCDMA_800_LNA_OFFSET_VS_FREQ_2_I,1825,ReadWrite,<SIGNED_BYTE,Array 0>#<SIGNED_BYTE,Array 1>#<SIGNED_BYTE,Array 2>#<SIGNED_BYTE,Array 3>#<SIGNED_BYTE,Array 4>#<SIGNED_BYTE,Array 5>#<SIGNED_BYTE,Array 6>#<SIGNED_BYTE,Array 7>#<SIGNED_BYTE,Array 8>#<SIGNED_BYTE,Array 9>#<SIGNED_BYTE,Array 10>#<SIGNED_BYTE,Array 11>#<SIGNED_BYTE,Array 12>#<SIGNED_BYTE,Array 13>#<SIGNED_BYTE,Array 14>#<SIGNED_BYTE,Array 15>#
NV_WCDMA_800_LNA_OFFSET_VS_FREQ_3_I,1826,ReadWrite,<SIGNED_BYTE,Array 0>#<SIGNED_BYTE,Array 1>#<SIGNED_BYTE,Array 2>#<SIGNED_BYTE,Array 3>#<SIGNED_BYTE,Array 4>#<SIGNED_BYTE,Array 5>#<SIGNED_BYTE,Array 6>#<SIGNED_BYTE,Array 7>#<SIGNED_BYTE,Array 8>#<SIGNED_BYTE,Array 9>#<SIGNED_BYTE,Array 10>#<SIGNED_BYTE,Array 11>#<SIGNED_BYTE,Array 12>#<SIGNED_BYTE,Array 13>#<SIGNED_BYTE,Array 14>#<SIGNED_BYTE,Array 15>#
NV_WCDMA_800_IM2_I_VALUE_I,1827,ReadWrite,<BYTE,I Value>#
NV_WCDMA_800_IM2_Q_VALUE_I,1828,ReadWrite,<BYTE,Q Value>#
NV_WCDMA_800_IM2_TRANSCONDUCTOR_VALUE_I,1829,ReadWrite,<BYTE,Transconductor Value>#
NV_WCDMA_800_RX_AGC_MIN_2_I,1830,ReadWrite,<SIGNED_WORD,Rx AGC Min Value>#
NV_WCDMA_800_RX_AGC_MIN_3_I,1831,ReadWrite,<SIGNED_WORD,Rx AGC Min Value>#
NV_WCDMA_800_MAX_TX_POWER_I,1832,ReadWrite,<SIGNED_BYTE,Max Power>#
NV_WCDMA_800_OUT_OF_SERVICE_THRESH_I,1833,ReadWrite,<SIGNED_WORD,Thresh Value>#
NV_WCDMA_800_LNA_RANGE_RISE_I,1834,ReadWrite,<SIGNED_WORD,LNA Rise Value>#
NV_WCDMA_800_LNA_RANGE_FALL_I,1835,ReadWrite,<SIGNED_WORD,LNA Fall Value>#
NV_WCDMA_800_IM_LEVEL_I,1836,ReadWrite,<SIGNED_WORD,IM Level>#
NV_WCDMA_800_NONBYPASS_TIMER_I,1837,ReadWrite,<BYTE,Timer Value>#
NV_WCDMA_800_BYPASS_TIMER_I,1838,ReadWrite,<WORD,Timer Value>#
NV_WCDMA_800_LNA_RANGE_OFFSET_I,1839,ReadWrite,<SIGNED_WORD,Offset>#
NV_WCDMA_800_LNA_OFFSET_VS_FREQ_I,1840,ReadWrite,<SIGNED_BYTE,Array 0>#<SIGNED_BYTE,Array 1>#<SIGNED_BYTE,Array 2>#<SIGNED_BYTE,Array 3>#<SIGNED_BYTE,Array 4>#<SIGNED_BYTE,Array 5>#<SIGNED_BYTE,Array 6>#<SIGNED_BYTE,Array 7>#<SIGNED_BYTE,Array 8>#<SIGNED_BYTE,Array 9>#<SIGNED_BYTE,Array 10>#<SIGNED_BYTE,Array 11>#<SIGNED_BYTE,Array 12>#<SIGNED_BYTE,Array 13>#<SIGNED_BYTE,Array 14>#<SIGNED_BYTE,Array 15>#
NV_WCDMA_800_RX_AGC_MIN_I,1841,ReadWrite,<SIGNED_WORD,Rx AGC Min Value>#
NV_WCDMA_800_RX_AGC_MAX_I,1842,ReadWrite,<SIGNED_WORD,Rx AGC Min Value>#
NV_WCDMA_800_AGC_PHASE_OFFSET_I,1843,ReadWrite,<BYTE,Phase Offset>#
NV_WCDMA_800_TX_LIN_MASTER_0_I,1844,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#<WORD,Array[30]>#<WORD,Array[31]>#<WORD,Array[32]>#<WORD,Array[33]>#<WORD,Array[34]>#<WORD,Array[35]>#<WORD,Array[36]>#
NV_WCDMA_800_TX_LIN_MASTER_1_I,1845,ReadWrite,<WORD,Array[0]>#<WORD,Array[1]>#<WORD,Array[2]>#<WORD,Array[3]>#<WORD,Array[4]>#<WORD,Array[5]>#<WORD,Array[6]>#<WORD,Array[7]>#<WORD,Array[8]>#<WORD,Array[9]>#<WORD,Array[10]>#<WORD,Array[11]>#<WORD,Array[12]>#<WORD,Array[13]>#<WORD,Array[14]>#<WORD,Array[15]>#<WORD,Array[16]>#<WORD,Array[17]>#<WORD,Array[18]>#<WORD,Array[19]>#<WORD,Array[20]>#<WORD,Array[21]>#<WORD,Array[22]>#<WORD,Array[23]>#<WORD,Array[24]>#<WORD,Array[25]>#<WORD,Array[26]>#<WORD,Array[27]>#<WORD,Array[28]>#<WORD,Array[29]>#<WORD,Array[30]>#<WORD,Array[31]>#<WORD,Array[32]>#<WORD,Array[33]>#<WORD,Array[34]>#<WORD,Array[35]>#<WORD,Array[36]>#
NV_WCDMA_800_TX_COMP_VS_FREQ_0_I,1846,ReadWrite,<SIGNED_BYTE,Array 0>#<SIGNED_BYTE,Array 1>#<SIGNED_BYTE,Array 2>#<SIGNED_BYTE,Array 3>#<SIGNED_BYTE,Array 4>#<SIGNED_BYTE,Array 5>#<SIGNED_BYTE,Array 6>#<SIGNED_BYTE,Array 7>#<SIGNED_BYTE,Array 8>#<SIGNED_BYTE,Array 9>#<SIGNED_BYTE,Array 10>#<SIGNED_BYTE,Array 11>#<SIGNED_BYTE,Array 12>#<SIGNED_BYTE,Array 13>#<SIGNED_BYTE,Array 14>#<SIGNED_BYTE,Array 15>#
NV_WCDMA_800_TX_COMP_VS_FREQ_1_I,1847,ReadWrite,<SIGNED_BYTE,Array 0>#<SIGNED_BYTE,Array 1>#<SIGNED_BYTE,Array 2>#<SIGNED_BYTE,Array 3>#<SIGNED_BYTE,Array 4>#<SIGNED_BYTE,Array 5>#<SIGNED_BYTE,Array 6>#<SIGNED_BYTE,Array 7>#<SIGNED_BYTE,Array 8>#<SIGNED_BYTE,Array 9>#<SIGNED_BYTE,Array 10>#<SIGNED_BYTE,Array 11>#<SIGNED_BYTE,Array 12>#<SIGNED_BYTE,Array 13>#<SIGNED_BYTE,Array 14>#<SIGNED_BYTE,Array 15>#
NV_WCDMA_800_TX_LIN_VS_TEMP_0_I,1848,ReadWrite,<SIGNED_BYTE,Array 0>#<SIGNED_BYTE,Array 1>#<SIGNED_BYTE,Array 2>#<SIGNED_BYTE,Array 3>#<SIGNED_BYTE,Array 4>#<SIGNED_BYTE,Array 5>#<SIGNED_BYTE,Array 6>#<SIGNED_BYTE,Array 7>#<SIGNED_BYTE,Array 8>#<SIGNED_BYTE,Array 9>#<SIGNED_BYTE,Array 10>#<SIGNED_BYTE,Array 11>#<SIGNED_BYTE,Array 12>#<SIGNED_BYTE,Array 13>#<SIGNED_BYTE,Array 14>#<SIGNED_BYTE,Array 15>#
NV_WCDMA_800_TX_LIN_VS_TEMP_1_I,1849,ReadWrite,<SIGNED_BYTE,Array 0>#<SIGNED_BYTE,Array 1>#<SIGNED_BYTE,Array 2>#<SIGNED_BYTE,Array 3>#<SIGNED_BYTE,Array 4>#<SIGNED_BYTE,Array 5>#<SIGNED_BYTE,Array 6>#<SIGNED_BYTE,Array 7>#<SIGNED_BYTE,Array 8>#<SIGNED_BYTE,Array 9>#<SIGNED_BYTE,Array 10>#<SIGNED_BYTE,Array 11>#<SIGNED_BYTE,Array 12>#<SIGNED_BYTE,Array 13>#<SIGNED_BYTE,Array 14>#<SIGNED_BYTE,Array 15>#
NV_WCDMA_800_TX_SLP_VS_TEMP_0_I,1850,ReadWrite,<SIGNED_BYTE,Array 0>#<SIGNED_BYTE,Array 1>#<SIGNED_BYTE,Array 2>#<SIGNED_BYTE,Array 3>#<SIGNED_BYTE,Array 4>#<SIGNED_BYTE,Array 5>#<SIGNED_BYTE,Array 6>#<SIGNED_BYTE,Array 7>#<SIGNED_BYTE,Array 8>#<SIGNED_BYTE,Array 9>#<SIGNED_BYTE,Array 10>#<SIGNED_BYTE,Array 11>#<SIGNED_BYTE,Array 12>#<SIGNED_BYTE,Array 13>#<SIGNED_BYTE,Array 14>#<SIGNED_BYTE,Array 15>#
NV_WCDMA_800_TX_SLP_VS_TEMP_1_I,1860,ReadWrite,<SIGNED_BYTE,Array 0>#<SIGNED_BYTE,Array 1>#<SIGNED_BYTE,Array 2>#<SIGNED_BYTE,Array 3>#<SIGNED_BYTE,Array 4>#<SIGNED_BYTE,Array 5>#<SIGNED_BYTE,Array 6>#<SIGNED_BYTE,Array 7>#<SIGNED_BYTE,Array 8>#<SIGNED_BYTE,Array 9>#<SIGNED_BYTE,Array 10>#<SIGNED_BYTE,Array 11>#<SIGNED_BYTE,Array 12>#<SIGNED_BYTE,Array 13>#<SIGNED_BYTE,Array 14>#<SIGNED_BYTE,Array 15>#
NV_WCDMA_800_R1_RISE_I,1861,ReadWrite,<WORD,Rise Value>#
NV_WCDMA_800_R1_FALL_I,1862,ReadWrite,<WORD,Fall Value>#
NV_WCDMA_800_TX_LIM_VS_TEMP_I,1863,ReadWrite,<BYTE,Array[0]>#<BYTE,Array[1]>#<BYTE,Array[2]>#<BYTE,Array[3]>#<BYTE,Array[4]>#<BYTE,Array[5]>#<BYTE,Array[6]>#<BYTE,Array[7]>#<BYTE,Array[8]>#<BYTE,Array[9]>#<BYTE,Array[10]>#<BYTE,Array[11]>#<BYTE,Array[12]>#<BYTE,Array[13]>#<BYTE,Array[14]>#<BYTE,Array[15]>#
NV_WCDMA_800_TX_LIM_VS_FREQ_I,1864,ReadWrite,<SIGNED_WORD,Array[0]>#<SIGNED_WORD,Array[1]>#<SIGNED_WORD,Array[2]>#<SIGNED_WORD,Array[3]>#<SIGNED_WORD,Array[4]>#<SIGNED_WORD,Array[5]>#<SIGNED_WORD,Array[6]>#<SIGNED_WORD,Array[7]>#<SIGNED_WORD,Array[8]>#<SIGNED_WORD,Array[9]>#<SIGNED_WORD,Array[10]>#<SIGNED_WORD,Array[11]>#<SIGNED_WORD,Array[12]>#<SIGNED_WORD,Array[13]>#<SIGNED_WORD,Array[14]>#<SIGNED_WORD,Array[15]>#
NV_WCDMA_800_ADJ_FACTOR_I,1865,ReadWrite,<BYTE,Value>#
NV_WCDMA_800_EXP_HDET_VS_AGC_I,1866,ReadWrite,<BYTE,Array[0]>#<BYTE,Array[1]>#<BYTE,Array[2]>#<BYTE,Array[3]>#<BYTE,Array[4]>#<BYTE,Array[5]>#<BYTE,Array[6]>#<BYTE,Array[7]>#<BYTE,Array[8]>#<BYTE,Array[9]>#<BYTE,Array[10]>#<BYTE,Array[11]>#<BYTE,Array[12]>#<BYTE,Array[13]>#<BYTE,Array[14]>#<BYTE,Array[15]>#
NV_WCDMA_800_HDET_OFF_I,1867,ReadWrite,<BYTE,Value>#
NV_WCDMA_800_HDET_SPN_I,1868,ReadWrite,<BYTE,Value>#
NV_WCDMA_800_ENC_BTF_I,1869,ReadWrite,<DWORD,Value>#
NV_WCDMA_800_AGC_PA_ON_RISE_DELAY_I,1870,ReadWrite,<WORD,Delay>#
NV_WCDMA_800_AGC_PA_ON_FALL_DELAY_I,1871,ReadWrite,<WORD,Delay>#
NV_WCDMA_800_AGC_TX_ON_RISE_DELAY_I,1872,ReadWrite,<WORD,Delay>#
NV_WCDMA_800_AGC_TX_ON_FALL_DELAY_I,1873,ReadWrite,<WORD,Delay>#
NV_WCDMA_800_AGC_UPDATE_TX_AGC_TIME_I,1874,ReadWrite,<WORD,Value>#